For 1990-2009 cars

### Removal Procedure

1. Remove the rear door sill plate. Refer to Rear Side Door Sill Plate Replacement .
2. Remove the center pillar lower trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
3. Remove the rear door opening weatherstrip.

### Installation Procedure

1. Install the rear door opening weatherstrip.
2. Install the center pillar lower trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
3. Install the rear door sill plate. Refer to Rear Side Door Sill Plate Replacement .