For 1990-2009 cars

## VIN Derivative North America

#### Passenger Car Vehicle Identification Number - North America Type

Position | Definition | Character | Description
--- | --- | --- | ---
1 | Country of Origin | K | Korea
2 | Manufacturer | L | General Motors Daewoo Auto and Technology Company
3 | Identifier | A 1 2 4 5 | Daewoo Chevrolet Pontiac Buick Suzuki
4 | Car Line | M T J V U | Matiz, Spark Aveo, Barina, Kalos Lacetti, Nubira, Optra, Viva Epica, Evanda Rezzo, Tacuma, Vivant
5 | Series | D J M | SE, Base, M SX, LS, X CDX, LT, C
6 | Body Type | 2 5 6 8 9 | 2-Door Hatchback 4-Door Notchback 4-Door Hatchback 4-Door Station Wagon (35) 4-Door Station Wagon (75)
7 | Restraint Code | 1 |

- Active Restraints - Manual Belts in All Positions

2 |

• | Active Restraints - Manual Belts in All Positions

• | Frontal Inflatable Restraint System - Left Front and Right Front

3 |

• | Active Restraints - Manual Belts - Left Front

• | Inflatable Restraint System

4 |

• | Active Restraints - Manual Belts in All Positions

• | Frontal Inflatable Restraint System - Left Front and Right Front

• | Side Inflatable Restraints - Left Front and Right Front

5 |

• | Active Restraints - Manual Belts in All Positions

• | Frontal Inflatable Restraint System - Left Front and Right Front

• | Side Inflatable Restraint System - Left Front

6 |

• | Active Restraints - Manual Belts in All Positions

• | Frontal Inflatable Restraint System - Left Front and Right Front

• | Side Inflatable Restraint System - Left Front and Right Front

• | Automatic Occupant Sensor - Right Front

7 |

• | Active Restraints - Manual Belts in All Positions

• | Frontal Inflatable Restraint System - Left Front and Right Front

• | Side Inflatable Restraint System - Left Front, Right Front, Left Rear, Right Rear

8 |

• | Active Restraints - Manual Belts in All Positions

• | Side Inflatable Restraint System - Left Front

9 |

• | Active Restraints - Manual Belts in All Positions

• | Frontal Inflatable Restraint System - Left Front and Right Front

• | Automatic Occupant Sensor - Right Front

8 | Engine Type | 4 0 (Zero) T D A

7

Y

V

6

B

3

W

Z

2

K

L

0.8L, SOHC, MPFI, L3

1.0L, SOHC, MPFI, L4

1.2L, SOHC, MPFI, L4

1.2L, DOHC, MPFI, L4

1.4L, SOHC, MPFI, L4

1.4L, DOHC, MPFI, L4

1.5L, SOHC, MPFI, L4

1.5L, DOHC, MPFI, L4

1.6L, DOHC, MPFI, L4

1.8L, DOHC, MPFI, L4, FAM I

1.8L, DOHC, MPFI, L4, FAM II

2.0L, SOHC, MPFI, L4

2.0L, DOHC, MPFI, L4

2.2L, DOHC, MPFI, L4

2.0L, DOHC, MPFI, L6

2.5L, DOHC, MPFI, L6

9 | Check Digit | -- | Check Digit
10 | Model Year | 3 4 5 6 7

8

9

A

2003

2004

2005

2006

2007

2008

2009

2010

11 | Plant Location | B C K | Bupyung, South Korea Changwon, South Korea Kunsan, South Korea
12-17 | Production Sequence | -- | Plant Sequential Number

## VIN Derivative Except North America

#### Passenger Car Vehicle Identification Number - EU Type

Position | Definition | Character | Description
--- | --- | --- | ---
1 | Country of Origin | K | Korea
2 | Manufacturer | L | General Motors Daewoo Auto and Technology Company
3 | Trade Name | A 1 2 3 4

5

Daewoo

Chevrolet

Pontiac

Holden

Buick

Suzuki

4 | Car Line | S N L U K | Aveo, Barina, Kalos Lacetti, Nubira, Optra, Viva Epica, Evanda, Tosca Rezzo, Tacuma, Vivant Matiz, Spark
5 | Drive System and Transmission | F A | Front-Wheel Drive, MT Front-Wheel Drive, AT
6-7 | Body Style | 08 19 35 48 68

69

75

2-Door Hatchback

4-Door Notchback, 6 - Windows

4-Door Station Wagon

4-Door Hatchback, 4 - Windows

4-Door Hatchback, 6 - Windows

4-Door Notchback, 4 - Windows

4-Door MPV

8 | Engine Type | 4 0 (Zero) T D C

A

7

Y

V

6

H

B

8

3

W

Z

K

P

2

L

F

G

R

U

0.8L, SOHC, MPFI, L3

1.0L, SOHC, MPFI, L4

1.2L, SOHC, MPFI, L4

1.2L, DOHC, L4

1.3L, SOHC, L4, FAM I

1.4L, SOHC, MPFI, L4, FAM I

1.4L, DOHC, MPFI, L4

1.5L, SOHC, MPFI, L4

1.5L, DOHC, MPFI, L4

1.6L, DOHC, MPFI, L4

1.8L, SOHC, MPFI, L4, FAM I

1.8L, DOHC, MPFI, L4, FAM I

1.8L, SOHC, L4, FAM II

1.8L, DOHC, MPFI, L4, FAM ll

2.0L, SOHC, MPFI, L4, FAM ll

2.0L, DOHC, MPFI, L4

2.0L, DOHC, MPFI, L6

2.0L, DOHC, L6, LPG

2.2L, DOHC, FAM II

2.5L, DOHC, L6

2.4L, DOHC, MPFI, L4

3.2L, DOHC, MPFI, HFV6

2.0L, Diesel, 150 PS

2.0L, Diesel, 120 PS

9 | Purpose | 1 E L J | Euro 2000 only Except Euro 2000 Leaded Euro 2005 only
10 | Model Year | 6 7 8 9 A | 2006 2007 2008 2009 2010
11 | Plant Location | B C K | Bupyung, South Korea Changwon, South Korea Kunsan, South Korea
12-17 | Production Sequence | -- | Plant Sequential Number