For 1990-2009 cars

Table 1: | Inflatable Restraint Front Passenger Presence Sensor
Table 2: | Inflatable Restraint I/P Module (1.4L, 1.6L and 1.8L) (Single Stage)
Table 3: | Inflatable Restraint I/P Module (2.0L) (Dual Stage)
Table 4: | Inflatable Restraint Front End Discriminating Sensor - Left
Table 5: | Inflatable Restraint Front End Discriminating Sensor - Right
Table 6: | Inflatable Restraint Sensing and Diagnostic Module (SDM) (Except North America)
Table 7: | Inflatable Restraint Sensing and Diagnostic Module (SDM) (North America)
Table 8: | Inflatable Restraint Side Impact Module - Left
Table 9: | Inflatable Restraint Side Impact Module - Right
Table 10: | Inflatable Restraint Side Impact Sensor - Left
Table 11: | Inflatable Restraint Side Impact Sensor - Right
Table 12: | Inflatable Restraint Steering Wheel Module C1 (North America)
Table 13: | Inflatable Restraint Steering Wheel Module C2 (North America)
Table 14: | Inflatable Restraint Steering Wheel Module (1.4L, 1.6L and 1.8L) (Single Stage)
Table 15: | Inflatable Restraint Steering Wheel Module (2.0L) (Dual Stage)
Table 16: | Inflatable Restraint Steering Wheel Module Coil - C1 (1.4L, 1.6L and 1.8L) (Single Stage)
Table 17: | Inflatable Restraint Steering Wheel Module Coil - C1 (2.0L) (Dual Stage)
Table 18: | Inflatable Restraint Steering Wheel Module Coil - C2 (w/ Cruise)
Table 19: | Inflatable Restraint Steering Wheel Module Coil - C2 (w/o Cruise)
Table 20: | Seat Belt Pretensioner - LF
Table 21: | Seat Belt Pretensioner - RF

#### Inflatable Restraint Front Passenger Presence Sensor

Connector Part Information |

• | AMP 1-0967640-1

• | 4-Way F Connector (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | PK | 939 | Ignition 1 Voltage
2 | YE/WH | 1415 | Communication
3 | BK | 252 | Ground
BK/WH (North America)
4 | -- | -- | Not Used

#### Inflatable Restraint I/P Module (1.4L, 1.6L and 1.8L) (Single Stage)

Connector Part Information |

• | FCI60201704

• | 2-Way Connector (YE)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | BK/D-BU | 1403 | I/P Module - High Control (LHD)
WH/BK | I/P Module - High Control (RHD)
2 | OG/D-BU | 1404 | I/P Module - Low Control (LHD)
D-GN/WH | I/P Module - Low Control (RHD)

#### Inflatable Restraint I/P Module (2.0L) (Dual Stage)

Connector Part Information |

• | FCI54550400

• | 4-Way F Connector (YE)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | OG/D-BU | 1404 | IP Module - Low Control
2 | BK/D-BU | 1403 | IP Module - High Control
3 | D-GN/D-BU | 1411 | IP - Stage 2 - High Control
4 | BK/D-GN | 1412 | IP Module - Stage 2 - Low Control

#### Inflatable Restraint Front End Discriminating Sensor - Left

Connector Part Information |

• | YAZAKI 7283-6507-70

• | 2-Way F Connector (YE)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | L-GN/RD | 2106 | Front End Sensor - Left Signal
2 | BN/BK | 2105 | Front End Sensor - Left Voltage

#### Inflatable Restraint Front End Discriminating Sensor - Right

Connector Part Information |

• | YAZAKI 7283-6507-70

• | 2-Way F Connector (YE)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | D-GN/WH | 2104 | Front End Sensor - Right Signal
2 | PU | 2103 | Front End Sensor - Right Signal

#### Inflatable Restraint Sensing and Diagnostic Module (SDM) (Except North America)

Connector Part Information |

• | AMP 368233-1

• | 50-Way Air Bag 50P Plug Ass'y (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | PK/BK | 1186 | Seat Belt Pretensioner - Passenger High Control
2 | D-BU/WH | 1187 | Seat Belt Pretensioner - Passenger Low Control
3 | PK | 1184 | Seat Belt Pretensioner - Driver Low Control
4 | D-BU | 1185 | Seat Belt Pretensioner - Driver High Control
5 | YE | 1139 | Ignition 1 Voltage
6 | BK/WH | 251 | Ground
7 | D-GN | 358 | Air Bag Indicator Control
8 | -- | -- | Not Used
9 | L-BU | 327 | Serial Data
10 | BN | 347 | Steering Wheel Module - Low Control
11 | BU | 348 | Steering Wheel Module - Low Control
12 | BN/WH | 238 | Seat Belt Switch - Left
13 | BK/D-BU | 1403 | I/P Module - High Control (LHD)
WH/BK | I/P Module - High Control (RHD)
14 | OG/D-BU | 1404 | I/P Module - Low Control (LHD)
D-GN/WH | I/P Module - Low Control (RHD)
15 | -- | -- | Not Used
16 | WH/YE | 1180 | Side Impact Module - Right - Low Control
17 | D-GN/YE | 1181 | Side Impact Module - Right - High Control
18 | D-GN/D-BU | 1183 | Side Impact Module - Driver High Control
19 | WH/D-BU | 1182 | Side Impact Module - Driver Low Control
20 | RD/YE | 753 | Side Impact Sensor - Driver - Voltage (LHD)
PK/WH | 714 | Side Impact Sensor - Passenger Voltage (RHD)
21 | PK/WH | 714 | Side Impact Sensor - Passenger Voltage (LHD)
RD/YE | 753 | Side Impact Sensor - Driver Voltage (RHD)
22-44 | -- | -- | Not Used
45 | BK | 754 | Side Impact Sensor - Driver Signal (LHD)
BN/WH | 715 | Side Impact Sensor - Passenger Signal (RHD)
46 | BN/WH | 715 | Side Impact Sensor - Passenger Signal (LHD)
BK | 754 | Side Impact Sensor - Driver Signal (RHD)
47-50 | -- | -- | Not Used

#### Inflatable Restraint Sensing and Diagnostic Module (SDM) (North America)

Connector Part Information |

• | AMP 0-1393359-2

• | 75-Way F Connector (OG)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2-25 | -- | -- | Not Used (Shorting Bar)
26 | YE | 1139 | Ignition 1 Voltage
27 | D-GN | 358 | Air Bag Indicator Control
28 | BK/WH | 251 | Ground
29 | D-BU | 348 | Steering Wheel Module - Low Control
30 | BN | 347 | Steering Wheel Module - High Control
31 | BK/D-BU | 1403 | I/P Module - High Control
32 | OG/D-BU | 1404 | I/P Module - Low Control
33 | D-BU | 1185 | Seat Belt Pretensioner - Driver - High Control
34 | PK | 1184 | Seat Belt Pretensioner - Driver - Low Control
35 | PK/BK | 1186 | Seat Belt Pretensioner - Passenger - High Control
36 | D-BU/WH | 1187 | Seat Belt Pretensioner - Passenger - Low Control
37 | WH/D-BU | 1182 | Side Impact Module - Driver High Control
38 | D-GN/D-BU | 1183 | Side Impact Module - Driver Low Control
39 | D-GN/YE | 1181 | Side Impact Module - Passenger Low Control
40 | WH/YE | 1180 | Side Impact Module - Passenger High Control
41 | YE | 1409 | Steering Wheel Module - High Control
42 | YE/BK | 1410 | Steering Wheel Module - High Control
43 | D-GN/D-BU | 1411 | IP Module - Stage 2 - High Control
44 | BK/D-GN | 1412 | IP Module - Stage 2 - Low Control
45-53 | -- | -- | Not Used
54 | L-BU | 327 | Serial Data
55 | -- | -- | Not Used
56 | D-GN/WH | 1358 | Driver Information Center (DIC) Switch Signal
57-60 | -- | -- | Not Used
61 | BN/WH | 238 | Seat Belt Switch - Left
62-63 | -- | -- | Not Used
64 | YE/WH | 1415 | Communication
65-67 | -- | -- | Not Used
68 | BN/WH | 715 | Side Impact Sensor - Passenger Signal
69 | PK/WH | 714 | Side Impact Sensor - Passenger Voltage
70 | RD/YE | 753 | Side Impact Sensor - Driver Voltage
71 | BK | 754 | Side Impact Sensor - Driver Signal
72 | D-GN/WH | 2104 | Discriminating Sensor - Right - Signal
73 | PU | 2103 | Discriminating Sensor - Right - Signal
74 | BN/BK | 2105 | Discriminating Sensor - Left - Signal
75 | L-GN/RD | 2106 | Discriminating Sensor - Left - Signal

#### Inflatable Restraint Side Impact Module - Left

Connector Part Information |

• | Yazaki 7C83-5524-70

• | 2-Way Connector (YE)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | WH/D-BU | 1182 | Side Impact Module - Driver Low Control
2 | D-GN/D-BU | 1183 | Side Impact Module - Driver High Control

#### Inflatable Restraint Side Impact Module - Right

Connector Part Information |

• | Yazaki 7C83-5524-70

• | 2-Way Connector (YE)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | WH/YE | 1180 | Side Impact Module - Passenger Low Control
2 | D-GN/YE | 1181 | Side Impact Module - Passenger High Control

#### Inflatable Restraint Side Impact Sensor - Left

Connector Part Information |

• | V23540-M5602-Y120

• | 2-Way

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | BK/WH | 754 | Side Impact Sensor - Driver Signal
2 | PK | 753 | Side Impact Sensor - Driver Voltage

#### Inflatable Restraint Side Impact Sensor - Right

Connector Part Information |

• | V23540-M5602-Y120

• | 2-Way

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | BN/WH | 715 | Side Impact Sensor - Passenger Signal
2 | PK/WH | 714 | Side Impact Sensor - Passenger Voltage

#### Inflatable Restraint Steering Wheel Module C1 (North America)

Connector Part Information |

• | OEM: 54550267

• | 2-Way F ABX-3 Code B (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | BN | 347 | Steering Wheel Module - High Control
B | D-GN/WH | 348 | Steering Wheel Module - Low Control

#### Inflatable Restraint Steering Wheel Module C2 (North America)

Connector Part Information |

• | OEM: 54550271

• | 2-Way F ABX-3 Code G (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | L-BU/RD | 1410 | Steering Wheel Module - High Control
B | BK/WH | 1409 | Steering Wheel Module - Low Control

#### Inflatable Restraint Steering Wheel Module (1.4L, 1.6L and 1.8L) (Single Stage)

Connector Part Information |

• | PED 12162794

• | 2-Way M Metri-Pack 280 Series, Unsealed (YE)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | D-BU | 348 | Steering Wheel Module - Low Control
2 | BN | 347 | Steering Wheel Module - High Control

#### Inflatable Restraint Steering Wheel Module (2.0L) (Dual Stage)

Connector Part Information |

• | FC I54550400

• | 4-Way Connector (YE)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | YE/BK | 1410 | Trailer ABS Failure Indicator Control
2 | YE | 1409 | Discriminating Sensor - Right Signal
3 | BN | 347 | Steering Wheel Module - High Control
4 | D-BU | 348 | Steering Wheel Module - Low Control

#### Inflatable Restraint Steering Wheel Module Coil - C1 (1.4L, 1.6L and 1.8L) (Single Stage)

Connector Part Information |

• | PED 12162794

• | 2-Way M Metri-Pack 280 Series, Unsealed (YE)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | D-BU | 348 | Steering Wheel Module - Low Control
2 | BN | 347 | Steering Wheel Module - High Control

#### Inflatable Restraint Steering Wheel Module Coil - C1 (2.0L) (Dual Stage)

Connector Part Information |

• | FC 154550400

• | 4-Way F Connector (YE)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | YE/BK | 1410 | Steering Wheel Module - High Control
2 | YE | 1409 | Steering Wheel Module - High Control
3 | BN | 347 | Steering Wheel Module - High Control
4 | D-BU | 348 | Steering Wheel Module - Low Control

#### Inflatable Restraint Steering Wheel Module Coil - C2 (w/ Cruise)

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | D-BU | 1796 | Radio Control - Steering Column Signal
2 | BK/WH | 372 | Remote Radio Return - Audio
3 | BK | 28 | Horn Relay Control
4 | GY | 397 | Cruise Control Switch Signal
5 | GY/BK | 87 | Cruise Control Release Signal
6 | D-BU | 84 | Cruise Control SET/Coast Switch Signal
7 | OG | 1540 | Battery Positive Voltage
8 | -- | -- | Not Used

#### Inflatable Restraint Steering Wheel Module Coil - C2 (w/o Cruise)

Connector Part Information |

• | KET MG 641032

• | 3-Way F

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | D-BU | 1796 | Radio Control - Steering Column Signal
2 | BK/WH | 372 | Remote Radio Return - Audio
3 | BK | 28 | Horn Relay Control

#### Seat Belt Pretensioner - LF

Connector Part Information |

• | V23540-M5302-Y22

• | 2-Way F Connector (GN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | 1185 | Seat Belt Pretensioner - Driver High Control
2 | YE/D-BU | 1184 | Seat Belt Pretensioner Driver Low Control

#### Seat Belt Pretensioner - RF

Connector Part Information |

• | V23540-M5302-Y22

• | 2-Way F Connector (GN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD/BK | 1187 | Seat Belt Pretensioner - Passenger Low Control
2 | D-BU/WH | 1186 | Seat Belt Pretensioner - Passenger High Control