For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ignition Switch Housing Shear Bolts | 11 N·m | 97 lb in
Ignition Switch Retaining Screw | 2.5 N·m | 22 lb in
Steering Column Jacket Assembly Front Bracket Bolts | 22 N·m | 16 lb ft
Steering Column Jacket Assembly Rear Bracket Bolts | 22 N·m | 16 lb ft
Steering Shaft Universal Joint Pinch bolt | 25 N·m | 18 lb ft
Steering Wheel Horn Cap Screws | 4.5 N·m | 40 lb in
Steering Wheel Nut | 38 N·m | 28 lb ft
Steering Wheel Rotation Sensor Retaining Screw | 2 N·m | 18 lb in
Support Housing Screws | 16 N·m | 12 lb ft
Turn Signal Switch Housing Screws | 3 N·m | 27 lb in
Upper and Lower Steering Column Cover Panel Screws | 2.5 N·m | 22 lb in