For 1990-2009 cars

Figure 1: |

#### Manifold Absoulte Pressure (MAP), Oil Pressure, Throttle Position (TP) Sensors

(1) | Manifold Absoulte Pressure (MAP) Sensor
(2) | Engine Oil Pressure Switch
(3) | Throttle Position (TP) Sensor
(4) | Idle Air Control (IAC)

Figure 2: |

#### Fuel Injectors, Heated Oxygen Sensor (HO2S) 1, Heated Oxygen Sensor (HO2S) 2, Idle Air Control (IAC) Valve, Intake Air Temperature (IAT) Sensor

(1) | Fuel Injector 1
(2) | Fuel Injector 2
(3) | Fuel Injector 3
(4) | Fuel Injector 4
(5) | Heated Oxygen Sensor (HO2S) 1 (MR-140), Oxygen Sensor (HV-240)
(6) | Heated Oxygen Sensor (HO2S) 2 (MR-140)
(7) | Idle Air Control (IAC) Valve
(8) | Intake Air Temperature (IAT) Sensor

Figure 3: |

#### Crankshaft Position (CKP) Sensors, EVAP, Ignition Coils

(1) | Evporative Emissions (EVAP) Canister Purge Solenoid Valve
(2) | Crankshaft Position (CKP) Sensor
(3) | Ignition Coil Modules

Figure 4: |

#### Engine Control Module (ECM), Engine Coolant Temperature (ECT), Camshaft Position (CMP) and Rough Road Sensors

(1) | Engine Control Module (ECM)
(2) | Engine Coolant Temperature (ECT) Sensor
(3) | Camshaft Position (CMP) Sensor
(4) | Rough Road Sensor

Figure 5: |

#### Exhaust Gas Recirculation (EGR) Valve, Knock Sensor (KS)

(1) | Exhaust Gas Recirculation (EGR) Valve (Euro Emissions)
(2) | Knock Sensor (KS)
(3) | Exhaust Gas Recirculation (EGR) Valve (ECE 83 Emissions)