For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Check Valve Spring Bolts | 6.5 N·m | 57 lb in
Control Cable Adjusting Nut | 8 N·m | 71 lb in
Damping Block Connection Nut and Bolt | 80 N·m | 59 lb ft
Differential Case-to-Differential Ring Gear Bolt | 102 N·m | 75 lb ft
Drain Plug | 17 N·m | 13 lb ft
Fluid Cooler Inlet Pipe Bolt | 9 N·m | 80 lb in
Fluid Cooler Inlet Pipe Fitting Nut | 35 N·m | 26 lb ft
Fluid Cooler Rear Outlet Pipe Clip Bolt | 9 N·m | 80 lb in
Fluid Cooler Rear Outlet Pipe Fitting Nut | 35 N·m | 26 lb ft
Front Outlet Pipe Clip Bolt | 9 N·m | 80 lb in
Front Outlet Pipe Union Bolt | 35 N·m | 26 lb ft
Input Speed Sensor Retaining Bolt | 5.4 N·m | 48 lb in
Manual Detent Spring Bolt | 9.8 N·m | 87 lb in
Manual Valve Lever Shaft Nut | 12 N·m | 106 lb in
Lower Transaxle-to-Engine Retaining Bolts | 73 N·m | 54 lb ft
Lower Transaxle-to-Engine Retaining Bolts | 31 N·m | 23 lb ft
Lower Transaxle-to-Engine Retaining Bolts | 21 N·m | 15 lb ft
Oil Pan Bolts | 7 N·m | 62 lb in
Oil Pump Bolts | 25 N·m | 18 lb ft
Oil Reservoir Lock Plate Bolts | 5.4 N·m | 48 lb in
Oil Strainer Bolts | 9.8 N·m | 87 lb in
Output Speed Sensor Retaining Bolt | 7.4 N·m | 65 lb in
Park/Neutral Position Switch Bolts | 5.4 N·m | 48 lb in
Parking Lock Pawl Bracket Bolts | 7.4 N·m | 65 lb in
Planetary Ring Gear Nut--Maximum | 29 N·m | 22 lb ft
Planetary Ring Gear Nut--Standard | 9.8 N·m | 87 lb in
Rear Mounting Bracket Bolts | 60 N·m | 44 lb ft
Screw Plugs | 7.4 N·m | 65 lb in
Shift Control Lever Assembly Mounting Bolts | 8 N·m | 71 lb in
Shift Solenoid Valve Bolts | 11 N·m | 97 lb in
Stator Shaft Bolts | 25 N·m | 18 lb ft
TCM Retaining Bolts | 5 N·m | 44 lb in
Torque Converter Bolts | 45 N·m | 43 lb ft
Transaxle Apply Clamp Bolt | 5.4 N·m | 48 lb in
Transaxle Case Plate Bolt | 9.8 N·m | 87 lb in
Transaxle Housing Bolts | 29 N·m | 22 lb ft
Transaxle Rear Cover Bolts | 25 N·m | 18 lb ft
Unions | 25 N·m | 18 lb ft
Upper Transaxle Mounting Bracket Bolts | 60 N·m | 44 lb ft
Upper Transaxle-to-Engine Mounting Bolts | 73 N·m | 54 lb ft
Valve Body Bolts | 11 N·m | 97 lb in