For 1990-2009 cars

Connector 1: | A/C Compressor Clutch (C60, C68)
Connector 2: | A/C Refrigerant Pressure Sensor Manual HVAC (L95, LXT)
Connector 3: | A/C Refrigerant Pressure Sensor Manual HVAC (LDA, L79, L34)
Connector 4: | A/C Refrigerant Pressure Sensor - Automatic/HVAC (L95, LXT)
Connector 5: | A/C Refrigerant Pressure Sensor - Automatic/HVAC (LDA, L79, L34)
Connector 6: | A/C Refrigerant Pressure Sensor - Automatic/HVAC (LMN)
Connector 7: | A/C Refrigerant Pressure Sensor (LMN)
Connector 8: | Accelerator Pedal Position (APP) Sensor (L34)
Connector 9: | Accelerator Pedal Position Sensor (LMN)
Connector 10: | Air Temperature Actuator (C68)
Connector 11: | Ambient Air Temperature Sensor (C68)
Connector 12: | Ashtray Lamp
Connector 13: | Automatic Transmission Shift Lever (Except North America)
Connector 14: | Automatic Transmission Shift Lever (North America)
Connector 15: | Auxiliary Power Outlet
Connector 16: | Back Up Lamp - Left
Connector 17: | Back Up Lamp - Right
Connector 18: | Backup Lamp Switch (M/T)
Connector 19: | Battery Saver (ER1)
Connector 20: | Blower Motor
Connector 21: | Blower Motor Control Module (C68)
Connector 22: | Blower Motor Relay (C68)
Connector 23: | Blower Motor Relay (C60)
Connector 24: | Blower Motor Resistor (C60)
Connector 25: | Blower Switch (C60)
Connector 26: | Boost Pressure Sensor (LMN)
Connector 27: | Brake Fluid Level Switch
Connector 28: | Camshaft Position (CMP) Sensor (L95, LXT)
Connector 29: | Camshaft Position (CMP) Sensor (L79)
Connector 30: | Camshaft Position (CMP) Sensor (LDA)
Connector 31: | Camshaft Position (CMP) Sensor (w/Throttle Actuator Control) (L34)
Connector 32: | Camshaft Position (CMP) Sensor (w/o Throttle Actuator Control) (L34)
Connector 33: | Camshaft Position (CMP) Sensor (LMN)
Connector 34: | Center High Mounted Stop Lamp (CHMSL) Hatchback
Connector 35: | Center High Mounted Stop Lamp (CHMSL) Notchback
Connector 36: | Cigar Lighter/Ashtray Lamp
Connector 37: | Clock
Connector 38: | Clutch Start Switch
Connector 39: | Clutch Switch (M/T)
Connector 40: | Coolant Temperature Sensor (C68)
Connector 41: | Cooling Fan - Auxiliary
Connector 42: | Cooling Fan - Main
Connector 43: | Cooling Fan Control Relay
Connector 44: | Cooling Fan Resistor
Connector 45: | Crankshaft Position Sensor (CKP) Sensor (L95, LXT)
Connector 46: | Crankshaft Position (CKP) Sensor (L79)
Connector 47: | Crankshaft Position (CKP) Sensor (LDA)
Connector 48: | Crankshaft Position (CKP) Sensor (w/Throttle Actuator Control) (L34)
Connector 49: | Crankshaft Position (CKP) Sensor (w/o Throttle Actuator Control) (L34)
Connector 50: | Crankshaft Position (CKP) Sensor (LMN)
Connector 51: | Cruise Control Module
Connector 52: | Data Link Connector (DLC)
Connector 53: | Daytime Running Lamp (DRL) Module (T61-Except North America)
Connector 54: | Daytime Running Lamp (DRL) Module (T61-North America)
Connector 55: | Daytime Running Lamp (DRL) Relay (T61-Except North America)
Connector 56: | Daytime Running Lamp (DRL) Relay 1 (T61-Except North America)
Connector 57: | Daytime Running Lamp (DRL) Relay 2 (T61-Except North America)
Connector 58: | Diesel Particulate Filter Pressure Sensor (LMN)
Connector 59: | Dome Lamp (TC0)
Connector 60: | Dome Lamp (w/o TC0)
Connector 61: | Door Ajar Switch - Left Front
Connector 62: | Door Ajar Switch - Left Rear
Connector 63: | Door Ajar Switch - Right Front
Connector 64: | Door Ajar Switch - Right Rear
Connector 65: | Door Lock Actuator - Driver
Connector 66: | Door Lock Actuator - Front Passenger
Connector 67: | Door Lock Actuator - Left Rear
Connector 68: | Door Lock Actuator - Right Rear
Connector 69: | Door Lock Relay
Connector 70: | Door Lock Switch (Optional)
Connector 71: | Door Tamper Switch - Driver
Connector 72: | Door Tamper Switch - Passenger
Connector 73: | Electronic Brake Control Module (EBCM) w/TCS
Connector 74: | Electronic Brake Control Module (EBCM) w/o TCS
Connector 75: | Engine Control Module (ECM) X1 (LMN)
Connector 76: | Engine Control Module (ECM) X2 (LMN)
Connector 77: | Engine Control Module (ECM) (L95, LXT)
Connector 78: | Engine Control Module (ECM) X1 (HV-240) (L79)
Connector 79: | Engine Control Module (ECM) X2 (HV-240) (L79)
Connector 80: | Engine Control Module (ECM) X1 (MR-140) (LDA)
Connector 81: | Engine Control Module (ECM) X2 (MR-140) (LDA)
Connector 82: | Engine Control Module (ECM) X1 (L34) w/Throttle Actuator Control
Connector 83: | Engine Control Module (ECM) X2 (L34) w/Throttle Actuator Control
Connector 84: | Engine Control Module (ECM) X1 (MR-140) (L34) w/o Throttle Actuator Control
Connector 85: | Engine Control Module (ECM) X2 (MR-140) (L34) w/o Throttle Actuator Control
Connector 86: | Engine Coolant Temperature (ECT) Sensor (L95, LXT)
Connector 87: | Engine Coolant Temperature (ECT) Sensor (L79)
Connector 88: | Engine Coolant Temperature (ECT) Sensor (LDA)
Connector 89: | Engine Coolant Temperature (ECT) Sensor (w/Throttle Actuator Control) (L34)
Connector 90: | Engine Coolant Temperature (ECT) Sensor (w/o Throttle Actuator Control) (L34)
Connector 91: | Engine Coolant Temperature (ECT) Sensor (LMN)
Connector 92: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve (L95, LXT)
Connector 93: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve (L79)
Connector 94: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve (LDA)
Connector 95: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve (w/Throttle Actuator Control) (L34)
Connector 96: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve (w/o Throttle Actuator) (L34)
Connector 97: | Evaporative Emission (EVAP) Canister Vent Solenoid Valve (LDA)
Connector 98: | Evaporative Emission (EVAP) Canister Vent Solenoid (w/Throttle Actuator Control) (L34)
Connector 99: | Evaporative Emission (EVAP) Canister Vent Solenoid Valve (w/o Throttle Actuator Control) (L34)
Connector 100: | Exhaust Gas Recirculation (EGR) Valve (ECE 83 Emissions) (L95, LXT)
Connector 101: | Exhaust Gas Recirculation (EGR) Valve (Euro III Emissions) (L95, LXT)
Connector 102: | Exhaust Gas Recirculation (EGR) Valve (Euro IV Emissions) (L95, LXT)
Connector 103: | Exhaust Gas Recirculation (EGR) Valve (LDA)
Connector 104: | Exhaust Gas Recirculation (EGR) Valve (w/Throttle Actuator Control) (L34)
Connector 105: | Exhaust Gas Recirculation (EGR) Valve (w/o Throttle Actuator Control) (L34)
Connector 106: | Exhaust Gas Recirculation (EGR) Valve (LMN)
Connector 107: | Exhaust Gas Temperature Sensor 1 - (LMN)
Connector 108: | Exhaust Gas Temperature Sensor 2 (LMN)
Connector 109: | Fog Lamp - Left Front
Connector 110: | Fog Lamp - Left Rear (T79)
Connector 111: | Fog Lamp - Right Front
Connector 112: | Fog Lamp - Right Rear (T79)
Connector 113: | Fuel Filter Heater/Temperature Sensor (LMN)
Connector 114: | Fuel Injector 1 (LMN)
Connector 115: | Fuel Injector 2 (LMN)
Connector 116: | Fuel Injector 3 (LMN)
Connector 117: | Fuel Injector 4 (LMN)
Connector 118: | Fuel Injectors (L95, LXT)
Connector 119: | Fuel Injectors (L79)
Connector 120: | Fuel Injectors (LDA)
Connector 121: | Fuel Injectors (L34)
Connector 122: | Fuel Injectors (w/o Throttle Actuator Control) (L34)
Connector 123: | Fuel Pump/Sender
Connector 124: | Fuel Pump (L79)
Connector 125: | Fuel Pump (LDA)
Connector 126: | Fuel Pump (w/o Throttle Actuator Control) (L34)
Connector 127: | Fuel Pump/Sender (L95, LXT)
Connector 128: | Fuel Pump/Sender (w/Throttle Actuator Control) (L34)
Connector 129: | Fuel Pump Module (LMN)
Connector 130: | Fuel Rail Pressure Control Valve (LMN)
Connector 131: | Fuel Rail Pressure Sensor (LMN)
Connector 132: | Fuel Tank Pressure Sensor (w/Throttle Actuator Control) (L34)
Connector 133: | Generator
Connector 134: | Glow Plug Control Unit (LMN)
Connector 135: | Hazard Switch
Connector 136: | Headlamp - High Beam - Left
Connector 137: | Headlamp - High Beam - Right
Connector 138: | Headlamp - Low Beam - Left
Connector 139: | Headlamp - Low Beam - Right
Connector 140: | Headlamp Leveling Switch (TR6)
Connector 141: | Headlamp Switch
Connector 142: | Heated Oxygen Sensor 1 (HO2S1) (LDA)
Connector 143: | Heated Oxygen Sensor 1 (HO2S1) (w/o Throttle Actuator Control) (L34)
Connector 144: | Heated Oxygen Sensor 2 (HO2S2) (LDA)
Connector 145: | Heated Oxygen Sensor 2 (HO2S2) (w/o Throttle Actuator Control) (L34)
Connector 146: | Heated Oxygen Sensor 2 (HO2S2) (Mexico, Japan) (LDA)
Connector 147: | Heated Oxygen Sensor 2 (HO2S2) (Mexico, Japan) (w/o Throttle Actuator Control) (L34)
Connector 148: | Heated Oxygen Sensor (HO2S) 1 (L95, LXT)
Connector 149: | Heated Oxygen Sensor (HO2S) 1 (w/Throttle Actuator Control) (L34)
Connector 150: | Heated Oxygen Sensor (HO2S) 2 (L95, LXT)
Connector 151: | Heated Oxygen Sensor (HO2S) 2 (w/Throttle Actuator Control) (L34)
Connector 152: | High Pressure Pump (LMN)
Connector 153: | High Speed Blower Motor Relay (C68)
Connector 154: | Hold Mode Switch (M98)
Connector 155: | Hood Ajar Switch
Connector 156: | Horn
Connector 157: | HVAC Control Module X1 (C68)
Connector 158: | HVAC Control Module X2 (C68)
Connector 159: | HVAC Control Module (C60)
Connector 160: | I/P Compartment Lamp
Connector 161: | I/P Compartment Lamp Switch
Connector 162: | I/P Dimmer Switch
Connector 163: | Idle Air Control (IAC) Valve (L79)
Connector 164: | Idle Air Control (IAC) Valve (LDA)
Connector 165: | Idle Air Control (IAC) Valve (w/o Throttle Actuator Control) (L34)
Connector 166: | Ignition Coil (IC) Module (L79)
Connector 167: | Ignition Coil (IC) Module (LDA)
Connector 168: | Ignition Coil (IC) Module (w/Throttle Actuator Control) (L34)
Connector 169: | Ignition Coil (IC) Module (w/o Throttle Actuator Control) (L34)
Connector 170: | Ignition Coil Module (1 and 4) (L95, LXT)
Connector 171: | Ignition Coil Module (2 and 3) (L95, LXT)
Connector 172: | Ignition Lock Cylinder Control Actuator (North America)
Connector 173: | Ignition Key Alarm Switch
Connector 174: | Ignition Key Alarm Switch
Connector 175: | Ignition Key Cylinder Lamp
Connector 176: | Ignition Switch
Connector 177: | Immobilizer
Connector 178: | Inflatable Restraint Front End Discriminating Sensor
Connector 179: | Inflatable Restraint Front Passenger Presence Sensor
Connector 180: | Inflatable Restraint I/P Module (Single Stage) (L95, LXT, LDA, L79)
Connector 181: | Inflatable Restraint I/P Module (Dual Stage) (L34)
Connector 182: | Inflatable Restraint Sensing and Diagnostic Module (SDM) (Except North America)
Connector 183: | Inflatable Restraint Sensing and Diagnostic Module (SDM) (North America)
Connector 184: | Inflatable Restraint Side Impact Module (AJ7)
Connector 185: | Inflatable Restraint Side Impact Sensor (AJ7)
Connector 186: | Inflatable Restraint Steering Wheel Module (Single Stage) (L95, LXT, LDA, L79)
Connector 187: | Inflatable Restraint Steering Wheel Module (Dual Stage) (L34)
Connector 188: | Inflatable Restraint Steering Wheel Module C1 (North America)
Connector 189: | Inflatable Restraint Steering Wheel Module C2 (North America)
Connector 190: | Inflatable Restraint Steering Wheel Module Coil
Connector 191: | Inflatable Restraint Steering Wheel Module Coil - C1 (Single Stage) (L95, LXT, LDA, L79)
Connector 192: | Inflatable Restraint Steering Wheel Module Coil - C1 (Dual Stage) (L34)
Connector 193: | Inflatable Restraint Steering Wheel Module Coil - C2 (w/Cruise)
Connector 194: | Inflatable Restraint Steering Wheel Module Coil - C2 (w/o Cruise)
Connector 195: | Input Shaft Speed (ISS) Sensor (MLQ)
Connector 196: | Input Speed Sensor (M98)
Connector 197: | Inside Air Temperature (C68)
Connector 198: | Instrument Cluster X1
Connector 199: | Instrument Cluster X2
Connector 200: | Instrument Cluster X3
Connector 201: | Intake Air Temperature (IAT) Sensor (L95, LXT)
Connector 202: | Intake Air Temperature (IAT) Sensor (L79)
Connector 203: | Intake Air Temperature (IAT) Sensor (LDA)
Connector 204: | Intake Air Temperature (IAT) Sensor (w/Throttle Actuator Control) (L34)
Connector 205: | Intake Air Temperature (IAT) Sensor (w/o Throttle Actuator Control) (L34)
Connector 206: | Intake Manifold Tuning Valve (L95, LXT)
Connector 207: | Intake Manifold Tuning Valve Solenoid (L79)
Connector 208: | Intake Manifold Tuning Valve Solenoid (LDA)
Connector 209: | Intake Manifold Tuning Valve Solenoid (w/o Throttle Actuator Control) (L34)
Connector 210: | Key Interlock Module (Except North America)
Connector 211: | Key Interlock Module (North America)
Connector 212: | Knock Sensor (KS) (L95, LXT)
Connector 213: | Knock Sensor (KS) (L79)
Connector 214: | Knock Sensor (KS) (LDA)
Connector 215: | Knock Sensor (KS) (w/Throttle Actuator Control) (L34)
Connector 216: | Knock Sensor (KS) (w/o Throttle Actuator Control) (L34)
Connector 217: | Lamp Control Module
Connector 218: | Lamp Driver Module
Connector 219: | License Plate Lamp - Left
Connector 220: | License Plate Lamp - Right
Connector 221: | Manifold Absolute Pressure (MAP) Sensor (L95, LXT)
Connector 222: | Manifold Absolute Pressure (MAP) Sensor (L79)
Connector 223: | Manifold Absolute Pressure (MAP) Sensor (LDA)
Connector 224: | Manifold Absolute Pressure (MAP) Sensor (w/Throttle Actuator Control) (L34)
Connector 225: | Manifold Absolute Pressure (MAP) Sensor (w/o Throttle Actuator Control) (L34)
Connector 226: | Mass Air Flow (MAF) Sensor (LMN)
Connector 227: | Mode Actuator (C68)
Connector 228: | Multifunction Alarm Module
Connector 229: | Octane Selection Switch (L95, LXT)
Connector 230: | Octane Selection Switch (L79)
Connector 231: | Oil Feeding Connector
Connector 232: | Oil Pressure Switch
Connector 233: | Output Speed Sensor (M98)
Connector 234: | Outside Rearview Mirror Driver
Connector 235: | Outside Rearview Mirror Folding Module (Optional)
Connector 236: | Outside Rearview Mirror Passenger
Connector 237: | Outside Rearview Mirror Switch
Connector 238: | Oxygen (O2) Sensor (L95, LXT)
Connector 239: | Oxygen (O2) Sensor (L79)
Connector 240: | Park Neutral Position (PNP) Switch (MLQ)
Connector 241: | Park/Neutral Position Switch (M98)
Connector 242: | Park/Neutral Position (PNP) Switch (MFA)
Connector 243: | Park/Turn Signal Lamp - Left Front (Except North America)
Connector 244: | Park/Turn Signal Lamp - Left Front (North America)
Connector 245: | Park/Turn Signal Lamp - Right Front (Except North America)
Connector 246: | Park/Turn Signal Lamp - Right Front (North America)
Connector 247: | Parking Brake Switch
Connector 248: | Power Steering Control Module
Connector 249: | PTC Heater (LMN)
Connector 250: | Radio (w/RDS) A
Connector 251: | Radio (w/RDS) B
Connector 252: | Radio (w/o RDS)
Connector 253: | Radio Antenna Module (Hatchback)
Connector 254: | Radio Antenna Module (Notchback)
Connector 255: | Reading Lamp (CF5)
Connector 256: | Reading Lamps (w/o CF5)
Connector 257: | Rear Compartment Lamp
Connector 258: | Rear Compartment Latch (Notchback)
Connector 259: | Rear Compartment Lid Release Actuator (Notchback)
Connector 260: | Rear Compartment Lid Release Switch (Notchback)
Connector 261: | Rear Compartment Tamper Switch
Connector 262: | Rear Compartment Tamper Switch (Notchback)
Connector 263: | Rear Fog Lamp Relay (T79)
Connector 264: | Rear Liftgate Latch - C1 (Hatchback)
Connector 265: | Rear Liftgate Latch - C2 (Hatchback)
Connector 266: | Rear Liftgate Latch - C3 (Hatchback)
Connector 267: | Rear Window Defogger X1
Connector 268: | Rear Window Defogger X2
Connector 269: | Recirculation Actuator
Connector 270: | Remote Control Door Lock Receiver/Theft Deterrent Control Module (w/Alarm)
Connector 271: | Remote Control Door Lock Receiver/Theft Deterrent Control Module (w/o Alarm)
Connector 272: | Rough Road Sensor (L95, LXT)
Connector 273: | Rough Road Sensor (LDA)
Connector 274: | Rough Road Sensor (w/o Throttle Actuator Control) (L34)
Connector 275: | Rough Road Sensor (w/o ABS) (w/Throttle Actuator Control) (L34)
Connector 276: | Seat Belt Pretensioner
Connector 277: | Seat Belt Switch
Connector 278: | Security Indicator
Connector 279: | Shift Indicator Lamp
Connector 280: | Shift Program Switch (MLQ)
Connector 281: | Shift Program Switch (MFA)
Connector 282: | Side Marker Lamp - Left Rear
Connector 283: | Side Marker Lamp - Right Rear
Connector 284: | Speaker - Double (DBS)
Connector 285: | Speaker - Tweeters - Front
Connector 286: | Speaker - Tweeters - Rear
Connector 287: | Speakers - Front
Connector 288: | Speakers - Rear
Connector 289: | Steering Wheel Position Sensor
Connector 290: | Stop Lamp Switch
Connector 291: | Sunload Sensor (C68)
Connector 292: | Sunroof Module
Connector 293: | Sunroof Switch/Reading Lamp
Connector 294: | Tail/Stop Lamp - Left Rear Inner (Hatchback)
Connector 295: | Tail/Stop Lamp - Left Rear Outer (Hatchback)
Connector 296: | Tail/Stop Lamp - Right Rear Inner (Hatchback)
Connector 297: | Tail/Stop Lamp - Right Rear Outer (Hatchback)
Connector 298: | Theft Deterrent Alarm
Connector 299: | Throttle Body (L95, LXT)
Connector 300: | Throttle Body Assembly (w/Throttle Actuator Control) (L34)
Connector 301: | Throttle Plate Actuator (LMN)
Connector 302: | Throttle Position (TP) Sensor (L79)
Connector 303: | Throttle Position (TP) Sensor (LDA)
Connector 304: | Throttle Position (TP) Sensor (w/o Throttle Actuator Control) (L34)
Connector 305: | Tire Pressure Monitor System (TPMS) Module
Connector 306: | Transaxle (M98)
Connector 307: | Transmission Connector (MLQ)
Connector 308: | Transmission Connector (MFA)
Connector 309: | Transmission Control Module (TCM) X1 (M98)
Connector 310: | Transmission Control Module (TCM) X1 (MFA)
Connector 311: | Transmission Control Module (TCM) X1 (MLQ)
Connector 312: | Transmission Control Module (TCM) X2 (M98)
Connector 313: | Transmission Control Module (TCM) X2 (MFA)
Connector 314: | Transmission Control Module (TCM) X2 (MLQ)
Connector 315: | Transmission Control Module (TCM) X3 (MFA)
Connector 316: | Turn Signal Lamp - Left Front (Except North America)
Connector 317: | Turn Signal Lamp - Left Rear
Connector 318: | Turn Signal Lamp - Right Front (Except North America)
Connector 319: | Turn Signal Lamp - Right Rear
Connector 320: | Turn Signal Multifunction Switch
Connector 321: | Turn Signal Repeater Lamp - Left
Connector 322: | Turn Signal Repeater Lamp - Right
Connector 323: | Turn Signal/Hazard Flasher Module
Connector 324: | Variable Effort Steering Actuator
Connector 325: | Vehicle Speed Sensor (VSS) (MLQ)
Connector 326: | Vehicle Speed Sensor (VSS) (Manual Transmission)
Connector 327: | Wastegate Solenoid (LMN)
Connector 328: | Water In Fuel Sensor (LMN)
Connector 329: | Wheel Speed Sensor (WSS) - Front
Connector 330: | Wheel Speed Sensor (WSS) - Rear
Connector 331: | Window Motor - Left Front
Connector 332: | Window Motor - Left Rear
Connector 333: | Window Motor - Right Front
Connector 334: | Window Motor - Right Rear
Connector 335: | Window Switch - Driver - Front Power Only
Connector 336: | Window Switch - Left Front - Front/Rear Power
Connector 337: | Window Switch - Left Rear
Connector 338: | Window Switch - Right Front
Connector 339: | Window Switch - Right Rear
Connector 340: | Windshield Washer Fluid Pump (Hatchback)
Connector 341: | Windshield Washer Fluid Pump (Notchback)
Connector 342: | Windshield Wiper Motor (w/CE1)
Connector 343: | Windshield Wiper Motor (w/o CE1)
Connector 344: | Windshield Wiper/Washer Switch A
Connector 345: | Windshield Wiper/Washer Switch B (w/Rear Fog Lamps)
Connector 346: | Windshield Wiper/Washer Switch B (w/o Rear Fog Lamps)
Connector 347: | Wiper Washer Rain Sensor (CE1)
Connector 348: | Wiper Motor Rear

### A/C Compressor Clutch (C60, C68)

#### Connector Part Information

- OEM: PED 12162017
- Description: 2-Way F Metri-Pack 150 Series, Sealed (GY)

#### A/C Compressor Clutch (C60, C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN | 59 | A/C Compressor Clutch Supply Voltage
B | 0.5 BK | 150 | Ground

### A/C Refrigerant Pressure Sensor Manual HVAC (L95, LXT)

#### Connector Part Information

- OEM: PED 12078090
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### A/C Refrigerant Pressure Sensor Manual HVAC (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | 413 | Low Reference
B | L-BU/BK | 1688 | 5-Volt Reference
C | L-BU | 203 | A/C Refrigerant Pressure Sensor Signal

### A/C Refrigerant Pressure Sensor Manual HVAC (LDA, L79, L34)

#### Connector Part Information

- OEM: PED 12078090
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### A/C Refrigerant Pressure Sensor Manual HVAC (LDA, L79, L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU/WH | 632 | Low Reference
B | GY | 605 | 5-Volt Reference
C | L-BU | 380 | A/C Refrigerant Pressure Sensor

### A/C Refrigerant Pressure Sensor - Automatic/HVAC (L95, LXT)

#### Connector Part Information

- OEM: PED 12078090
- Description: 3-Way F Metri-Pack 150 Series (WH)

#### A/C Refrigerant Pressure Sensor - Automatic/HVAC (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BN | 413 | Low Reference
B | 0.5 L-BU/BK | 1688 | 5-Volt Reference
C | 0.5 RD/L-BU | 203 | A/C Refrigerant Pressure Sensor Signal

### A/C Refrigerant Pressure Sensor - Automatic/HVAC (LDA, L79, L34)

#### Connector Part Information

- OEM: PED 12078090
- Description: 3-Way F Metri-Pack 150 Series (WH)

#### A/C Refrigerant Pressure Sensor - Automatic/HVAC (LDA, L79, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU/WH | 632 | Low Reference
B | 0.5 GY | 605 | 5-Volt Reference
C | 0.5 L-BU | 380 | 5-Volt Reference

### A/C Refrigerant Pressure Sensor - Automatic/HVAC (LMN)

#### Connector Part Information

- OEM: PED 12078090
- Description: 3-Way F Metri-Pack 150 Series (WH)

#### A/C Refrigerant Pressure Sensor - Automatic/HVAC (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/WH | 1688 | 5-Volt Reference
2 | 0.5 BN/WH | 413 | Low Reference
3 | 0.5 BN/BK | 203 | A/C Refrigerant Pressure Sensor Signal

### A/C Refrigerant Pressure Sensor (LMN)

#### Connector Part Information

- OEM: PED 12078090
- Description: 3-Way F Metri-Pack 150 Series (WH)

#### A/C Refrigerant Pressure Sensor (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN/WH | 605 | 5-Volt Reference
B | BK/WH | 632 | Low Reference
C | BN/BK | 380 | A/C Refrigerant Pressure Sensor Signal

### Accelerator Pedal Position (APP) Sensor (L34)

#### Connector Part Information

- OEM: AMP 174923
- Description: 6-Way F (BK)

#### Accelerator Pedal Position (APP) Sensor (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 WH | 791 | APP Sensor 2 Signal
2 | 0.5 PU | 1550 | Low Reference
3 | 0.5 D-BU | 790 | APP Sensor 1 Signal
4 | 0.5 L-BU | 1450 | Low Reference
5 | 0.5 BN | 488 | 5-Volt Reference 1
6 | 0.5 BN/BK | 543 | 5-Volt Reference 2

### Accelerator Pedal Position Sensor (LMN)

#### Connector Part Information

- OEM: PED 15326830
- Description: 6-Way F GT 150 Series Unsealed

#### Accelerator Pedal Position Sensor (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | -- | Accelerator Pedal Position Signal 2
2 | PU | -- | Accelerator Pedal Position Low Reference 2
3 | BU | -- | Accelerator Pedal Position Signal 1
4 | L-BU | -- | Accelerator Pedal Position Low Reference 1
5 | BN | -- | Accelerator Pedal Position 5-Volt Reference 1
6 | BN/BK | -- | Accelerator Pedal Position 5-Volt Reference 2

### Air Temperature Actuator (C68)

#### Connector Part Information

- OEM: KET MG 610203
- Description: 7-Way F 118 (PA) Series (BK)

#### Air Temperature Actuator (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.3 BK | 1199 | Air Temperature Door Control
3 | 0.3 BN | 1812 | Low Reference
4 | -- | -- | Not Used
5 | 0.3 YE | 1791 | Low Reference
6 | 0.3 YE/BK | 1814 | Lower Mode Door Position Signal
7 | 0.3 L-BU | 1316 | Air Temperature Door Control

### Ambient Air Temperature Sensor (C68)

#### Connector Part Information

- OEM: KET MG 610489
- Description: 2-Way F NMWP 04F-B Ass'y

#### Ambient Air Temperature Sensor (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE | 61 | Low Reference
2 | 0.5 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal

### Ashtray Lamp

#### Connector Part Information

- OEM:
- Description: 2-Way F (BK)

#### Ashtray Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | 309 | Ashtray Lamp Supply Voltage
2 | D-GN | 44 | Ground

### Automatic Transmission Shift Lever (Except North America)

#### Connector Part Information

- OEM: KET MG 610396
- Description: 4-Way F Series Sealed (WH)

#### Automatic Transmission Shift Lever (Except North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 1050 | Ground
2 | 0.5 L-GN | 275 | Park/Neutral Position (PNP) Switch Signal
3 | 0.5 L-GN | 275 | Park/Neutral Position (PNP) Switch Signal
4 | 0.5 D-GN | 286 | Automatic Transmission Shift Lock Solenoid Supply Voltage

### Automatic Transmission Shift Lever (North America)

#### Connector Part Information

- OEM: KET MG 610396
- Description: 4-Way F SDL Series (WH)

#### Automatic Transmission Shift Lever (North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.50 BK | 1050 | Ground
2 | 0.5 L-GN | 275 | Park/Neutral Position (PNP) Switch Signal
3 | 0.5 L-GN | 275 | Shift Lock Control Solenoid
4 | PK | 239 | Ignition 1 Voltage

### Auxiliary Power Outlet

#### Connector Part Information

- OEM: KET MG 630685-5
- Description: 2-Way F 250 Series (BK)

#### Auxiliary Power Outlet

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.85 YE | 243 | Ignition 1 and 2 Voltage
2 | 0.85 BK | 1050 | Ground

### Back Up Lamp - Left

#### Connector Part Information

- OEM: 0001338
- Description: 2-Way F CE-F22.2 Series (WH)

#### Back Up Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | 24 | Backup Lamps Supply Voltage
B | BK/WH | 750 | Ground

### Back Up Lamp - Right

#### Connector Part Information

- OEM:
- Description: 2-Way F CE-F22.2 Series (WH)

#### Back Up Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | 24 | Backup Lamps Supply Voltage
B | BK/WH | 750 | Ground

### Backup Lamp Switch (M/T)

#### Connector Part Information

- OEM: PED 12052641
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Backup Lamp Switch (M/T)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 839 | Ignition 1 Voltage
2 | L-GN | 24 | Backup Lamp Supply Voltage

### Battery Saver (ER1)

#### Connector Part Information

- OEM: KET MG 651050
- Description: 8-Way F

#### Battery Saver (ER1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | WH | 1080 | Light Switch Signal
3 | WH | 1080 | Illumination Relay Control
4 | OG | 1540 | Ignition 1 Voltage
5 | BK | 1050 | Ground
6 | PU | 128 | Door Ajar Signal
7 | L-GN | 80 | Key in Ignition Signal
8 | -- | -- | Not Used

### Blower Motor

#### Connector Part Information

- OEM: KET MG 610043
- Description: 2-Way F 250 Series (WH)

#### Blower Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3 YE | 744 | Automatic HVAC - Blower Motor Supply Voltage
3 PU | 65 | Manual HVAC - Blower Motor Feed
2 | 3 PU | 743 | Automatic HVAC - Blower Motor Speed Signal
3 BK | 1050 | Manual HVAC - Ground

### Blower Motor Control Module (C68)

#### Connector Part Information

- OEM: KET MG 610269
- Description: 6-Way F 250 D/L Series

#### Blower Motor Control Module (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.25 D-BU | 188 | Blower Motor Resistor Assembly Supply Voltage
2 | -- | -- | Not Used
3 | 3 BK | 350 | Ground
4 | 0.3 GY/BK | 754 | Blower Motor Speed Control
5 | -- | -- | Not Used
6 | 3 PU | 743 | Blower Motor Speed Signal

### Blower Motor Relay (C68)

#### Connector Part Information

- OEM: AK 36409
- Description: 4-Way F Relay

#### Blower Motor Relay (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
30 | 3 BK | 350 | Battery Positive Voltage
85 | 0.5 D-BU/BK | 247 | Ground
86 | 0.85 BN | 41 | Blower Motor High Control
87 | 3 PU | 743 | Blower Motor Feed

### Blower Motor Relay (C60)

#### Connector Part Information

- OEM: AK 36409
- Description: 4-Way F Relay (GY)

#### Blower Motor Relay (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
30 | RD | 742 | Battery Positive Voltage
85 | BK | 250 | Ground
86 | OG | 52 | Blower Motor High Control
87 | PU | 65 | Blower Motor Feed

### Blower Motor Resistor (C60)

#### Connector Part Information

- OEM: KET MG 610047
- Description: 4-Way F 250 Series (WH)

#### Blower Motor Resistor (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 72 | Medium 2 Blower Motor Control
2 | PU | 63 | Blower Motor Medium 1 Control
3 | PU | 65 | Blower Motor Feed
4 | YE | 60 | Blower Motor Low Control

### Blower Switch (C60)

#### Connector Part Information

- OEM: AMP 178004-1
- Description: 4-Way F 250 Series Dbl Lock Plug 4P (WH)

#### Blower Switch (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
B1 | L-BU | 72 | Medium 2 Blower Motor Control
B2 | PU | 63 | Blower Motor Medium 1 Control
B3 | BN | 41 | Ignition 1 Voltage
B4 | YE | 60 | Blower Motor Low Control

### Boost Pressure Sensor (LMN)

#### Connector Part Information

- OEM: TYCO 368162-1
- Description: 4-Way F JPT Sealed

#### Boost Pressure Sensor (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BU | -- | Ground
2 | L-GN | -- | Intake Air Temperature Signal
3 | WH/BK | -- | 5-Volt Reference
4 | GY/BK | -- | Boost Pressure Signal

### Brake Fluid Level Switch

#### Connector Part Information

- OEM: KET MG 610320
- Description: 2-Way F SWP Series (BK)

#### Brake Fluid Level Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PU/WH | 33 | Brake Warning Indicator Control
2 | 0.5 BK | 1150 | Ground

### Camshaft Position (CMP) Sensor (L95, LXT)

#### Connector Part Information

- OEM: AMP 85205-1
- Description: 3-Way F JR Power Timer 3P Hsg Ass'y (BK)

#### Camshaft Position (CMP) Sensor (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
2 | 0.5 L-GN | 632 | Low Reference
3 | 0.5 BN/WH | 633 | Camshaft Position (CMP) Sensor Signal

### Camshaft Position (CMP) Sensor (L79)

#### Connector Part Information

- OEM: KET AMP 85205-1
- Description: 3-Way F ITC (Injector Connector) Series

#### Camshaft Position (CMP) Sensor (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 PK/BK | 1846 | Ignition 1 Voltage
2 | 0.5 BK/WH | 252 | Ground
3 | 0.5 BN/WH | 633 | Camshaft Position (CMP) Sensor Signal

### Camshaft Position (CMP) Sensor (LDA)

#### Connector Part Information

- OEM: KET MG 640541
- Description: 3-Way F ITC (Injector Connector) Series

#### Camshaft Position (CMP) Sensor (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
2 | 0.5 BK/WH | 251 | Ground
3 | 0.5 PU (BN/WH) | 633 | Camshaft Position (CMP) Sensor Signal

### Camshaft Position (CMP) Sensor (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 85205-1
- Description: 3-Way F ITC (Injector Connector) Series (BK)

#### Camshaft Position (CMP) Sensor (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
2 | 0.5 BK/WH | 251 | Ground
3 | 0.5 PU | 633 | Camshaft Position (CMP) Sensor Signal

### Camshaft Position (CMP) Sensor (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: KET MG 640541
- Description: 3-Way F ITC (Injector Connector) Series

#### Camshaft Position (CMP) Sensor (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
2 | 0.5 BK/WH | 251 | Ground
3 | 0.5 PU (BN/WH) | 633 | Camshaft Position (CMP) Sensor Signal

### Camshaft Position (CMP) Sensor (LMN)

#### Connector Part Information

- OEM: TYCO 85205-1
- Description: 3-Way F JPT Sealed

#### Camshaft Position (CMP) Sensor (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN/BK | -- | Signal
2 | BU/WH | -- | Ground
3 | PK/WH | -- | Battery Positve Voltage

### Center High Mounted Stop Lamp (CHMSL) Hatchback

#### Connector Part Information

- OEM: KET MG 610392
- Description: 2-Way F SDL Series (WH)

#### Center High Mounted Stop Lamp (CHMSL) Hatchback

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 750 | Ground
2 | L-BU | 20 | Stop Lamp Switch Signal

### Center High Mounted Stop Lamp (CHMSL) Notchback

#### Connector Part Information

- OEM: KET MG 630679
- Description: 2-Way F SDL Series (WH)

#### Center High Mounted Stop Lamp (CHMSL) Notchback

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 20 | Stop Lamp Switch Signal
2 | BK | 1250 | Ground

### Cigar Lighter/Ashtray Lamp

#### Connector Part Information

- OEM: KET MG 620046
- Description: 4-Way M 250 Series (WH)

#### Cigar Lighter/Ashtray Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 44 | Instrument Panel Lamps Dimmer Switch Signal
2 | BN/WH | 309 | Right Park Lamp Supply Voltage
3 | YE | 143 | Accessory Voltage
4 | BK | 1050 | Ground

### Clock

#### Connector Part Information

- OEM: MOLEX 5557-06R
- Description: 6-Way F Mini Fit Conn. Rec. Housing (WH)

#### Clock

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN/WH | 1358 | Passenger Presence Indicator
2 | 0.3 OG | 1140 | Battery Positive Voltage
3 | 0.3 BK | 1050 | Ground
4 | 0.5 PK | 939 | Ignition 1 Voltage
5 | 0.3 YE | 43 | Accessory Voltage
6 | 0.3 BN/WH | 309 | Right Park Lamp Supply Voltage

### Clutch Start Switch

#### Connector Part Information

- OEM: PED 12010649
- Description: 2-Way F 56 Series (WH)

#### Clutch Start Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 5 | Crank Voltage
2 | GY | 48 | Clutch Start Switch Signal

### Clutch Switch (M/T)

#### Connector Part Information

- OEM: PED 02977373
- Description: 2-Way F 56 Series, Unsealed (GY)

#### Clutch Switch (M/T)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 250 | Ignition 1 Voltage
2 | 0.5 BN/WH | 379 | Cruise Control Clutch Pedal Switch Output

### Coolant Temperature Sensor (C68)

#### Connector Part Information

- OEM: KET MG 610070
- Description: 2-Way F 090 (2.3 mm) Series

#### Coolant Temperature Sensor (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE | 61 | Low Reference
2 | 0.5 GY/BK | 1596 | Coolant Temperature Sensor Signal

### Cooling Fan - Auxiliary

#### Connector Part Information

- OEM: KUM PB 045-02027
- Description: 2-Way F WWP02F-B Assembly (BK)

#### Cooling Fan - Auxiliary

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 BK | 150 | Ground
2 | 2 PU | 532 | Cooling Fan Motor Supply Voltage

### Cooling Fan - Main

#### Connector Part Information

- OEM: AMP 176146-2
- Description: 2-Way F 187 Series Sealed Connector 2 Pos Plug Hsg Assembly (BK)

#### Cooling Fan - Main

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 L-BU | 504 | Cooling Fan Low Reference (North America)
2 BK | 50 | Ground
2 | 2 L-BU | 409 | Cooling Fan Motor Supply Voltage (North America)
2 PU | 532 | Cooling Fan Motor Supply Voltage

### Cooling Fan Control Relay

#### Connector Part Information

- OEM: PED 12110539
- Description: 9-Way F Metri-Pack 280 Series Sealed (BK)

#### Cooling Fan Control Relay

Pin | Wire | Circuit | Function
--- | --- | --- | ---
30 | 2 L-BU | 504 | Cooling Fan Low Reference
85 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
86 | 0.5 GY | 473 | High Speed Cooling Fan Relay Control
87 | 2 BK | 50 | Ground
87A | 2 PU | 532 | Cooling Fan Motor Supply Voltage

### Cooling Fan Resistor

#### Connector Part Information

- OEM: AMP 176143-2
- Description: 2-Way F WWP02F-B Assembly (BK)

#### Cooling Fan Resistor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 L-BU | 409 | Cooling Fan Motor Supply Voltage
2 | 2 PU | 532 | Cooling Fan Motor Supply Voltage

### Crankshaft Position Sensor (CKP) Sensor (L95, LXT)

#### Connector Part Information

- OEM: AMP 85205-1
- Description: 3-Way F JR Power Timer 3P Hsg Ass'y (BK)

#### Crankshaft Position Sensor (CKP) Sensor (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE/BK | 1868 | Low Reference
2 | 0.5 D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
3 | 0.5 BK/WH | 51 | Ground

### Crankshaft Position (CKP) Sensor (L79)

#### Connector Part Information

- OEM: AMP 85205-1
- Description: 3-Way JR Power Timer 3P Hsg Ass'y (BK)

#### Crankshaft Position (CKP) Sensor (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
2 | 0.5 YE/BK | 1868 | Low Reference
3 | 0.5 BK/WH | 51 | Ground

### Crankshaft Position (CKP) Sensor (LDA)

#### Connector Part Information

- OEM: AMP 85205-1
- Description: 3-Way JR Power Timer 3P Hsg Ass'y (BK

#### Crankshaft Position (CKP) Sensor (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
2 | 0.5 YE/BK | 1868 | Low Reference
3 | 0.5 BK/WH | 51 | Ground

### Crankshaft Position (CKP) Sensor (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 85205-1
- Description: 3-Way JR Power Timer 3P Hsg Assembly (BK)

#### Crankshaft Position (CKP) Sensor (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
2 | 0.5 YE/BK | 1868 | Low Reference
3 | 0.5 BK/WH | 51 | Ground

### Crankshaft Position (CKP) Sensor (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 85205-1
- Description: 3-Way JR Power Timer 3P Hsg Ass'y (BK)

#### Crankshaft Position (CKP) Sensor (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
2 | 0.5 YE/BK | 1868 | Low Reference
3 | 0.5 BK/WH | 51 | Ground

### Crankshaft Position (CKP) Sensor (LMN)

#### Connector Part Information

- OEM: TYCO 85205-1
- Description: 3-Way F JPT Sealed

#### Crankshaft Position (CKP) Sensor (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Signal
2 | GY | -- | Low Reference
3 | YE/BK | -- | Ground

### Cruise Control Module

#### Connector Part Information

- OEM: PED 12065425
- Description: 10-Way F Metri-Pack 150 Series, Sealed (BK)

#### Cruise Control Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN/WH | 817 | Vehicle Speed Sensor (VSS) Signal
B | 0.5 GY | 397 | Cruise Control Switch Signal
C | 0.5 L-BU | 20 | Stop Lamp Switch Signal
D | 0.3 GY/BK | 87 | Cruise Control Release Signal
E | 0.5 BK | 250 | Ground
F | 0.5 BN/WH | 379 | Cruise Control Clutch Pedal Switch Signal
0.5 OG/BK | 434 | Automatic Transmission Park/Neutral Position (PNP) Signal
G | 0.5 D-BU | 84 | Cruise Control SET/COAST Switch Signal
H | 0.5 PK | 739 | Ignition 1 Voltage
J | 0.3 GY | 121 | Engine Speed Signal
K | 0.5 WH | 85 | Cruise Control Engage Signal

### Data Link Connector (DLC)

#### Connector Part Information

- OEM: 12110250
- Description: 16-Way F Metri-Pack 150 Series (BK)

#### Data Link Connector (DLC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | D-BU | 555 | Serial Data
4 | BK | 250 | Ground
5 | BK | 250 | Ground
6 | -- | -- | Not Used (Gasoline)
PU | -- | CAN High (Diesel)
7 | PU | 2000 | Serial Data
8 | L-GN | 483 | Serial Data
9-11 | -- | -- | Not Used
12 | D-BU/WH | 774 | Serial Data
13 | L-BU | 327 | Serial Data
14 | -- | -- | Not Used (Gasoline)
YE | -- | CAN Low (Diesel)
15 | -- | -- | Not Used
16 | OG | 1840 | Battery Positive Voltage

### Daytime Running Lamp (DRL) Module (T61-Except North America)

#### Connector Part Information

- OEM: F8-4
- Description: 8-Way M Connector (BK)

#### Daytime Running Lamp (DRL) Module (T61-Except North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 140 | Battery Voltage
2 | BN/WH | 309 | Park Lamp Signal
3 | D-BU | 2641 | Daytime Running Lamp (DRL) Relay Control
4 | PU | 12 | Headlamp Low Beam Supply Voltage
5 | BK | 1050 | Ground
6 | PK | 239 | Ignition Voltage
7 | BN/WH | 309 | Park Lamp Signal
8 | PU/WH | 231 | Oil Pressure Signal

### Daytime Running Lamp (DRL) Module (T61-North America)

#### Connector Part Information

- OEM: PED 12064998
- Description: 8-Way F Connector (BK)

#### Daytime Running Lamp (DRL) Module (T61-North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG | 140 | Battery Voltage
B | L-GN | 11 | Headlamp High Beam Supply Voltage
C | PU | 12 | Headlamp Low Beam Supply Voltage
D | PU/WH | 33 | Brake Warning Indicator Control
E | BK | 1050 | Ground
F | BN | 141 | Ignition 3 Voltage
G | WH | 629 | Daytime Running Lamp (DRL) Indicator Control
H | -- | -- | Not Used

### Daytime Running Lamp (DRL) Relay (T61-Except North America)

#### Connector Part Information

- OEM: AK 83803
- Description: 9-Way F Relay (BK)

#### Daytime Running Lamp (DRL) Relay (T61-Except North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
30 | BN/WH | 309 | Right Park Lamp Supply Voltage
85 | BK | 250 | Ground
86 | L-GN | 11 | Headlamp High Beam Supply Voltage
87 | PU | 12 | Headlamp Low Beam Supply Voltage

### Daytime Running Lamp (DRL) Relay 1 (T61-Except North America)

#### Connector Part Information

- OEM: AK 838033
- Description: 9-Way F Relay

#### Daytime Running Lamp (DRL) Relay 1 (T61-Except North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
30 | D-BU | 2641 | Daytime Running Lamp (DRL) Relay Control
85 | OG | 140 | Battery Positive Voltage
86 | WH | 1080 | Park Lamp Relay Control
87 | OG | 140 | Battery Positive Voltage

### Daytime Running Lamp (DRL) Relay 2 (T61-Except North America)

#### Connector Part Information

- OEM: AK 36409
- Description: 9-Way F Relay

#### Daytime Running Lamp (DRL) Relay 2 (T61-Except North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
30 | L-BU/BK | 2346 | Flash to Pass Signal
85 | BN | 141 | Battery Positive Voltage
86 | GY/BK | 1798 | Headlamp Relay Control
87 | L-BU | 1346 | Headlamp Relay Supply Voltage/Headlamp Control

### Diesel Particulate Filter Pressure Sensor (LMN)

#### Connector Part Information

- OEM: FEP 1J0973703
- Description: 3-Way F Sealed

#### Diesel Particulate Filter Pressure Sensor (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | -- | 5-Volt Reference
2 | L-BU | -- | Low Reference
3 | YE/BK | -- | Signal

### Dome Lamp (TC0)

#### Connector Part Information

- OEM: KET MG 610398
- Description: 6-Way F SDL Series (WH)

#### Dome Lamp (TC0)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 640 | Battery Positive Voltage
2 | -- | -- | Not Used
3 | PK | 839 | Ignition 1 Voltage
4 | BK | 850 | Ground
5 | PU | 156 | Courtesy Lamp Control
6 | D-GN/WH | 900 | Key Cylinder Lamp Control

### Dome Lamp (w/o TC0)

#### Connector Part Information

- OEM: KET MG 610396
- Description: 4-Way F SDL Series (WH)

#### Dome Lamp (w/o TC0)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BK | 850 | Ground
3 | PU | 156 | Courtesy Lamp Control
4 | OG | 640 | Battery Positive Voltage

### Door Ajar Switch - Left Front

#### Connector Part Information

- OEM: KET MG 630063
- Description: 2-Way 250 Series (BK)

#### Door Ajar Switch - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 156 | Courtesy Lamp Control

### Door Ajar Switch - Left Rear

#### Connector Part Information

- OEM: KET MG 630063
- Description: 2-Way 250 Series (BK)

#### Door Ajar Switch - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 156 | Courtesy Lamp Control

### Door Ajar Switch - Right Front

#### Connector Part Information

- OEM: KET MG 630063
- Description: 2-Way 250 Series (BK)

#### Door Ajar Switch - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 156 | Courtesy Lamp Control

### Door Ajar Switch - Right Rear

#### Connector Part Information

- OEM: KET MG 630063
- Description: 2-Way 250 Series (BK)

#### Door Ajar Switch - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 156 | Courtesy Lamp Control

### Door Lock Actuator - Driver

#### Connector Part Information

- OEM: PED 15300027
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Door Lock Actuator - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU/WH | 294 | Door Lock Actuator Unlock Control
B | GY | 295 | Door Lock Actuator Lock Control

### Door Lock Actuator - Front Passenger

#### Connector Part Information

- OEM: PED 15300027
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Door Lock Actuator - Front Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU/WH | 294 | Door Lock Actuator Unlock Control
B | GY | 295 | Door Lock Actuator Lock Control

### Door Lock Actuator - Left Rear

#### Connector Part Information

- OEM: PED 15300027
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Door Lock Actuator - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 294 | Door Lock Actuator Unlock Control
B | GY | 295 | Door Lock Actuator Lock Control

### Door Lock Actuator - Right Rear

#### Connector Part Information

- OEM: PED 15300027
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Door Lock Actuator - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 294 | Door Lock Actuator Unlock Control
B | WH | 295 | Door Lock Actuator Lock Control

### Door Lock Relay

#### Connector Part Information

- OEM: KET MG 610896
- Description: 8-Way F PCB Connector SDL-II PCB Hsg (WH)

#### Door Lock Relay

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN/WH | 355 | Driver Door Lock Relay Lock Control
2 | GY | 295 | Door Lock Actuator Lock Control
3 | PU | 294 | Door Lock Actuator Unlock Control
4 | WH | 194 | Door Unlock Control
5 | OG/BK | 1340 | Battery Positive Voltage
6 | L-BU/BK | 195 | Door Lock Control
7 | YE | 356 | Driver Door Lock Relay Unlock Control
8 | BK | 350 | Ground

### Door Lock Switch (Optional)

#### Connector Part Information

- OEM: KET MG 610394
- Description: 3-Way F SDL Series (WH)

#### Door Lock Switch (Optional)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN/WH | 355 | Driver Door Lock Relay Lock Control
2 | BK | 1150 | Ground
3 | WH | 356 | Driver Door Lock Relay Unlock Control

### Door Tamper Switch - Driver

#### Connector Part Information

- OEM: AK 32421
- Description: 4-Way F Connector (GY)

#### Door Tamper Switch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU/BK | 195 | Door Lock Control
B | BK | 1150 | Ground
C | WH | 194 | Door Unlock Control
D | L-GN | 1370 | Driver Door Lock Cylinder Signal

### Door Tamper Switch - Passenger

#### Connector Part Information

- OEM: AK 32421
- Description: 4-Way F Connector (GY)

#### Door Tamper Switch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 1371 | Passenger Door Lock Cylinder Signal
B | -- | -- | Not Used
C | BK | 350 | Ground
D | -- | -- | Not Used

### Electronic Brake Control Module (EBCM) w/TCS

#### Connector Part Information

- OEM: AMP 1376600-1
- Description: 47-Way M

#### Electronic Brake Control Module (EBCM) w/TCS

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 4 RD | 42 | B+
2 | 0.5 D-BU | 774 | Serial Data
3 | -- | -- | Not Used
4 | 0.5 BN | 739 | Ignition 1 Voltage
5-9 | -- | -- | Not Used
10 | 0.5 WH/YE | 866 | Rough Road Signal
11-12 | -- | -- | Not Used
13 | 0.5 PU/WH | 33 | Brake Oil Pressure Switch
14 | 0.5 L-BU | 876 | Rough Road Signal
15 | -- | -- | Not Used
16 | 3 BK/WH | 2051 | Ground
17-31 | -- | -- | Not Used
32 | 4 RD | 42 | B+
33 | 0.5 WH | 833 | Right Front Wheel Speed Sensor Signal
34 | 0.5 GY | 872 | Right Front Wheel Speed Sensor Return
35 | 0.5 D-GN | 905 | TCS Warning Lamp Indicator Control
36 | 0.5 BK | 884 | Left Rear Wheel Speed Sensor Return
37 | 0.5 RD | 885 | Left Rear Wheel Speed Sensor Signal
38-40 | -- | -- | Not Used
41 | 0.5 L-BU | 20 | Stop Lamp Switch Signal
42 | 0.5 WH | 883 | Right Rear Wheel Speed Sensor Return
43 | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal
44 | 0.5 L-GN/BK | 867 | ABS Warning Lamp
45 | 0.5 L-BU | 830 | Left Front Wheel Speed Sensor Return
46 | 0.5 BN | 873 | Left Front Wheel Speed Sensor Signal
47 | 4 BK | 2050 | Ground

### Electronic Brake Control Module (EBCM) w/o TCS

#### Connector Part Information

- OEM: AMP 1612683-1
- Description: 26-Way F

#### Electronic Brake Control Module (EBCM) w/o TCS

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 4 RD | 42 | B+
2 | 0.5 BK | 884 | Left Rear Wheel Speed Sensor Return
3 | 0.5 RD | 885 | Left Rear Wheel Speed Sensor Signal
4 | 0.5 L-GN/BK | 867 | ABS Warning Lamp
5 | 0.5 WH | 833 | Right Front Wheel Speed Sensor Signal
6 | 0.5 GY | 872 | Right Front Wheel Speed Sensor Return
7 | -- | -- | Not Used
8 | 0.5 L-BU | 830 | Left Front Wheel Speed Sensor Return
9 | 0.5 BN | 873 | Left Front Wheel Speed Sensor Signal
10 | 0.5 PU/WK | 33 | Brake Oil Pressure Switch
11 | 0.5 WH | 883 | Right Rear Wheel Speed Sensor Return
12 | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal
13 | 3 BK/WH | 2051 | Ground
14 | 4 RD | 42 | B+
15 | -- | -- | Not Used
16 | 0.5 L-BU | 20 | Stop Lamp Switch Signal
17 | 0.5 WH/YE | 866 | Rough Road Signal
18 | 0.5 D-BU | 774 | Serial Data
19 | 0.5 L-GN | 876 | Rough Road Signal
20 | 0.5 BN | 739 | Ignition 1 Voltage
21-25 | -- | -- | Not Used
26 | 4 BK | 2050 | Ground

### Engine Control Module (ECM) X1 (LMN)

#### Connector Part Information

- OEM: AMP 2-1355123-3
- Service: N/A
- Description: 60-Way F 60POS Receptacle Hsg Assembly (BK)

#### Engine Control Module (ECM) X1 (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | Fuel Injector 3 Control (w/ Immobilizer)
YE/BK | -- | Fuel Injector 1 Control (w/o Immobilizer)
2 | L-GN/BK | -- | Fuel Injector 2 Control (w/ Immobilizer)
GN | -- | Fuel Injector 4 Control (w/ Immobilizer)
3 | -- | -- | Not Used
4 | BN/WH | -- | Fuel Rail Pressure Regulator Supply Voltage
5 | -- | -- | Not Used
6 | PU | -- | Cruise Switch Ground
7 | WH/BK | -- | CKP Shield Ground
8 | GN/WH | -- | Fuel Rail Pressure Sensor Low Reference
9-11 | -- | -- | Not Used
12 | GY | -- | CKP Low Reference
13 | WH/BK | -- | Boost Pressure Sensor 5 Volt Reference
14-15 | -- | -- | Not Used
16 | YE/BK | -- | Fuel Injector 1 Control (w/ Immobilizer)
L-BU | -- | Fuel Injector 3 Control (w/ Immobilizer)
17 | GN | -- | Fuel Injector 4 Control (w/ Immobilizer)
L-GN/BK | -- | Fuel Injector 2 Control (w/o Immobilizer)
18 | -- | -- | Not Used
19 | PU/WH | -- | Fuel Injection Pump Supply Voltage
20 | BU/WH | -- | CMP Low Reference
21-22 | -- | -- | Not Used
23 | YE/BU | -- | Boost Pressure Sensor Low Reference
24-26 | -- | -- | Not Used
27 | BN/WH | -- | CKP Signal
28 | L-BU | -- | Fuel Rail Pressure Sensor 5-Volt Reference
29-30 | -- | -- | Not Used
31 | PU | -- | Fuel Injector 2 Low Reference (w/ Immobilizer)
WH/BK | -- | Fuel Injector 4 Low Reference (w/o Immobilizer)
32 | -- | -- | Not Used
33 | WH/BK | -- | Fuel Injector 4 Low Reference (w/ Immobilizer)
PU | -- | Fuel Injector 2 Low Reference (w/o Immobilizer)
34 | L-BU/BK | -- | Fuel Rail Pressure Regulator Control
35-36 | -- | -- | Not Used
37 | BU/WH | -- | IAT Signal
38-39 | -- | -- | Not Used
40 | GY/BK | -- | Boost Pressure Sensor Signal
41 | -- | -- | Not Used
42 | PU/WH | -- | MAF Signal
43 | GY/BK | -- | Fuel Rail Pressure Sensor Signal
44 | YE/BK | -- | IAT, MAF Low Reference
45 | WH | -- | Cruise Indicator Control
46 | BN/WH | -- | Fuel Injector 3 Low Reference (w/ Immobilizer)
WH | -- | Fuel Injector 1 Low Reference (w/o Immobilizer)
47 | WH | -- | Fuel Injector 1 Low Reference (w/ Immobilizer)
BN/WH | -- | Fuel Injector 3 Low Reference (w/o Immobilizer)
48 | -- | -- | Not Used
49 | GN | -- | Fuel Injection Pump Control
50 | L-GN/BK | -- | CMP Signal
51 | -- | -- | Not Used
52 | GN | -- | Throttle Plate Actuator Feedback Signal
53 | L-GN | -- | IAT Signal
54-55 | -- | -- | Not Used
56 | GN/WH | -- | Cruise Switch Signal
57-58 | -- | -- | Not Used
59 | WH | -- | Throttle Plate Actuator Control
60 | GN/WH | -- | EGR Control

### Engine Control Module (ECM) X2 (LMN)

#### Connector Part Information

- OEM: AMP 3-1355136-3
- Service: N/A
- Description: 94-Way F 94POS Receptacle Hsg Assembly (BK)

#### Engine Control Module (ECM) X2 (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Battery Positive Voltage
2 | BK | -- | Ground
3 | PK | -- | Battery Positive Voltage
4 | BK | -- | Ground
5 | PK | -- | Battery Positive Voltage
6 | BK | -- | Ground
7 | -- | -- | Not Used
8 | BN/WH | -- | APP Sensor Low Reference (2)
9 | GN | -- | APP Sensor Signal (1)
10 | YE/BK | -- | Fuel Temperature Sensor Low Reference
11 | L-GN/BK | -- | Fuel Temperature Signal
12 | BK/WH | -- | A/C Refrigerant Pressure Sensor Low Reference
13 | BN/BK | -- | A/C Refrigerant Pressure Sensor Signal
14-16 | -- | -- | Not Used
17 | YE | -- | Stop Lamp Switch Signal
18 | GY/BK | -- | ECT Low Reference
19 | BN | -- | Generator Voltage Signal
20 | GN/WH | -- | Fuel Pump Relay Control
21 | L-BU/WH | -- | Change Oil Soon Indicator Control
22 | BN/WH | -- | A/C Refrigerant Pressure Sensor 5-Volt Reference
23-25 | -- | -- | Not Used
26 | L-GN/BK | -- | ECT Gauge Signal
27 | -- | -- | Not Used
28 | PK/BK | -- | Ignition 1 Voltage
29 | PU/WH | -- | A/C Compressor Relay Control
30 | L-BU | -- | APP Sensor Low Reference (1)
31 | YE | -- | APP Sensor Signal (2)
32 | L-BU/BK | -- | Exhaust Gas Temperature Sensor Signal 2
33 | YE/WH | -- | Exhaust Gas Temperature Sensor 2 Low Reference
34 | PU/WH | -- | Exhaust Gas Temperature Sensor Signal 1
35 | BU/WH | -- | Exhaust Gas Temperature Sensor 1 Low Reference
36 | -- | -- | Not Used
37 | L-BU | -- | Diesel Particulate Filter Pressure Sensor Low Reference
38-43 | -- | -- | Not Used
44 | PU/WH | -- | Diesel Particulate Filter Pressure Sensor 5-Volt Reference
45 | GY/BK | -- | APP Sensor 5-Volt Reference (1)
46 | WH | -- | APP Sensor 5-Volt Reference (2)
47 | BN | -- | Serial Data
48 | BU/WH | -- | Engine Speed Signal
49 | BN | -- | Charge Indicator Control
50-51 | -- | -- | Not Used
52 | WH | -- | Glow Plug Diagnosis
53 | -- | -- | Not Used
54 | BN | -- | Brake Pedal Switch Signal
55-56 | -- | -- | Not Used
57 | GN/WH | -- | PTC Request Signal
58-63 | -- | -- | Not Used
64 | YE/BK | -- | Diesel Particulate Filter Pressure Sensor Signal
65 | -- | -- | Not Used
66 | BN | -- | ECT Sensor Signal
67 | GY/BK | -- | ECT Indicator Control
68 | BU | -- | Fuel Heater Relay Control
69 | GN | -- | Cooling Fan Low Speed Relay Control
70 | YE/BK | -- | Diesel Particulate Filter Indicator Control
71 | PU/WH | -- | MIL Control
72 | GY/BK | -- | Engine Main Relay Coil Control
73 | GN/BK | -- | Wastegate Solenoid Control
74 | PK/BK | -- | Vehicle Speed Signal (VSS) (M/T)
75 | BU/WH | -- | Generator Field Duty Cycle Signal
76-78 | -- | -- | Not Used
79 | GN/WH | -- | A/C Request Signal
80 | GN/WH | -- | Cruise Control Clutch Switch Signal
81-82 | -- | -- | Not Used
83 | L-GN | -- | CAN Low
84 | L-BU | -- | CAN High
85-88 | -- | -- | Not Used
89 | PU | -- | Fuel Warning Signal
90 | BU | -- | Cooling Fan High Speed Relay Control
91 | L-GN/WH | -- | PTC Relay 2,3 Control
92 | L-BU | -- | Glow Plug Indicator Control
93 | WH/RD | -- | Glow Plug Control
94 | YE | -- | PTC Relay 1 Control

### Engine Control Module (ECM) (L95, LXT)

#### Connector Part Information

- OEM: 211PC902S0008
- Description: 90-Way F Connector (BK)

#### Engine Control Module (ECM) (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 1.25 BK/WH | 251 | Ground
4 | -- | -- | Ground
5 | 0.5 GY | 435 | Exhaust Gas Recirculation (EGR) Solenoid Low Control
6 | 0.5 D-GN/WH | 465 | Fuel Pump Relay Control
7 | 0.5 D-BU/WH | 471 | Main Relay Control
8 | 0.5 D-GN | 135 | Engine Coolant Temperature (ECT) Gage Signal
9 | 0.5 D-BU | 473 | High Speed - Cooling Fan Relay Control
10 | 0.5 D-GN | 335 | Low Speed - Cooling Fan Relay Control
11 | 0.5 BK/WH | 51 | Shield Ground
12 | 0.5 D-BU/WH | 1876 | Low Reference
13 | 0.5 OG/BK | 469 | Heated Oxygen Sensor (HO2S) 1 Heater Control
14 | 0.5 PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Low Reference
15 | -- | -- | Not Used
16 | 0.5 BN | 413 | Heated Oxygen Sensor (HO2S) 2 Heater Control
17 | 0.5 L-GN | 632 | Low Reference
18 | -- | -- | Not Used
19 | 0.5 BK/YE | 808 | Low Reference
20 | 0.5 L-BU | 203 | A/C Refrigerant Pressure Sensor Signal
21 | 0.5 D-BU | 1936 | Fuel Level Sensor Signal
22 | 0.5 BN/WH | 633 | Camshaft Position (CMP) Sensor Signal
23 | -- | -- | Not Used
24 | 1.25 BK/WH | 251 | Ground
25 | 0.5 BK/WH | 51 | Shield Ground
26 | -- | -- | Not Used
27 | 0.5 L-BU | 772 | Octane Switch Signal (Non-OBD)
1.25 BK/WH | 251 | Ground (Euro Emissions)
28 | 1.25 BK/WH | 251 | Ground
29 | 0.85 PK | 539 | Ignition 1 Voltage
30 | 0.5 OG | 440 | Battery Positive Voltage
31 | 0.85 WH | 423 | Ignition Coil (IC) Timing Control (2 and 3)
32 | 0.85 OG | 406 | Ignition Coil (IC) Timing Control (1 and 4)
33 | 1.25 BK/WH | 251 | Ground
34 | -- | -- | Not Used
35 | 0.5 BN/WH | 1666 | Heated Oxygen Sensor (HO2S) 1 Signal
36 | -- | -- | Not Used
37 | 0.5 WH/BK | 962 | Intake Manifold Tuning Valve Solenoid Control
38 | -- | -- | Not Used
39 | 0.5 BN/WH | 419 | Multifunction Indicator Lamp (MIL) Control
40 | 0.5 PU | 30 | Fuel Level Sensor Signal
41 | 0.5 PU | 67 | A/C Compressor Clutch Coil Supply Voltage
42 | 0.5 YE/BK | 496 | Knock Sensor (KS) Signal
43 | 0.5 D-GN | 534 | High Idle Switch Signal
44 | 0.5 PU/WH | 1665 | Heated Oxygen Sensor (HO2S) 1 Low Reference (OBD)
O2 Sensor Signal (Non OBD)
45 | 0.5 BN | 1456 | Exhaust Gas Recirculation (EGR) Valve Position Signal
46 | 0.5 GY | 605 | Low Reference
47-49 | -- | -- | Not Used
50 | 0.5 L-BU/BK | 1688 | 5-Volt Reference
51 | 0.5 D-GN/WH | 817 | Vehicle Speed Signal (Manual Transmission)
52 | 0.5 D-GN/WH | 762 | A/C Request Signal
53 | 0.5 WH | 873 | Rough Road Sensor Signal
0.5 D-BU | 876 | Rough Road Sensor Signal w/ABS
54 | 0.5 YE/BK | 1868 | Low Reference
55 | 0.5 PK | 427 | Idle Speed Control Motor Switch Signal
56 | 0.5 PU | 2000 | Keyword Serial Data
57 | 0.5 YE | 710 | CAN Serial Data Low (Automatic Transmission)
58 | -- | -- | Not Used
59 | 0.5 BK | 1744 | Fuel Injector 1 Control
60 | 0.5 PK/BK | 1746 | Fuel Injector 3 Control
61 | 0.5 D-BU | 426 | Idle Motor Return
62 | 0.5 L-BU | 425 | Idle Motor Feed
63 | -- | -- | Not Used
64 | 0.5 BN/WH | 1671 | Heated Oxygen Sensor (HO2S) 2 Signal
65 | 0.5 D-GN/WH | 428 | EVAP Canister Purge Solenoid Control
66 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
67 | 1.25 BK/WH | 251 | Ground
68 | 0.5 WH | 121 | Engine Speed Signal
69 | 0.5 GY | 435 | Exhaust Gas Recirculation (EGR) Solenoid Low Control (Non OBD)
70-73 | -- | -- | Not Used
74 | 0.5 D-BU | 417 | Throttle Position (TP) Sensor Signal
75 | 0.5 L-GN | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
76 | 0.5 YE | 410 | Engine Coolant Temperature (ECT) Sensor Signal
77 | -- | -- | Not Used
78 | 0.5 BN | 472 | Intake Air Temperature (IAT) Sensor Signal
79 | 0.5 GY | 416 | 5-Volt Reference
80 | -- | -- | Not Used
81 | 0.5 PU | 773 | Octane Switch Signal
0.5 BK/WH | 251 | Ground
82 | -- | -- | Not Used
83 | 0.5 BN | 990 | Power Steering Pressure Switch Signal
84 | 0.5 OG | 830 | 5-Volt Reference
85 | 0.5 D-BU/WH | 1869 | Crankshaft Position Sensor Signal
86-87 | -- | -- | Not Used
88 | 0.5 PU | 1807 | CAN Serial Data High
89 | 0.5 L-BU/BK | 844 | Fuel Injector 4 Control
90 | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control

### Engine Control Module (ECM) X1 (HV-240) (L79)

#### Connector Part Information

- OEM: PED 12129231
- Description: 32-Way Retainer Lock (GY)

#### Engine Control Module (ECM) X1 (HV-240) (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK/WH | 51 | Ground
2 | 0.5 BK/WH | 51 | Ground
3 | 0.5 YE/BK | 496 | Knock Sensor Signal
4 | D-GN | 411 | Exhaust Gas Recirculation (EGR) Valve Control
5 | -- | -- | Not Used
6 | 0.5 YE/BK | 1868 | Low Reference
7 | 0.5 D-BU | 417 | Throttle Position (TP) Sensor Signal
8 | 0.5 PK/BK | 1746 | Fuel Injector 3 Control
9 | 0.5 BK | 1744 | Fuel Injector 1 Control
10 | BK/WH | 252 | Low Reference
11 | 0.5 YE | 410 | Engine Coolant Temperature (ECT) Sensor Signal
12 | D-GN/RD | 1665 | Oxygen (O2) Sensor 1 Low Reference (Unleaded Only)
13 | 0.5 PU/WH | 1749 | Idle Air Control (IAC) Coil B High Control
14 | -- | -- | Not Used
15 | 0.5 GY | 416 | 5-Volt Reference
16 | 0.5 OG/BK | 469 | Low Reference
17 | 0.5 BK/WH | 51 | Ground
18 | 0.5 L-BU | 406 | Ignition Coil (IC) 1 and 4 Control
19 | 0.5 D-GN/WH | 423 | Ignition Coil (IC) 2 and 3 Control
20 | 0.5 D-GN/WH | 428 | Evaporative Emissions (EVAP) Canister Purge Solenoid Control
21 | 0.5 D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
22 | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control
23 | 0.5 BN | 472 | Intake Air Temperature (IAT) Sensor 5-Volt Reference
24 | 0.5 L-GN | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
25 | 0.5 BN/WH | 633 | Camshaft Position (CMP) Sensor Signal
26 | 0.5 L-BU/BK | 844 | Fuel Injector 4 Control
27 | 0.5 GY | 1653 | Oxygen (O2) Sensor 1 Signal (Unleaded Only)
28 | 0.5 BN | 1747 | Idle Air Control (IAC) Coil A High Control
29 | 0.5 WH | 444 | Idle Air Control (IAC) B Low Control
30 | 0.5 YE/WH | 1748 | Idle Air Control (IAC) A Low Control
31 | 0.5 L-BU/BK | 1688 | 5-Volt Reference Voltage
32 | 0.5 BK/YE | 808 | Low Reference

### Engine Control Module (ECM) X2 (HV-240) (L79)

#### Connector Part Information

- OEM: PED 12129232
- Description: 32-Way Retainer Lock (WH)

#### Engine Control Module (ECM) X2 (HV-240) (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PU/WH | 632 | Low Reference
2 | 0.5 OG | 440 | Battery Positive Voltage
3 | 0.5 PK/D-BU | 539 | Ignition 1 Voltage
4-6 | -- | -- | Not Used
7 | 0.5 L-BU | 380 | A/C Refrigerant Pressure (ACP) Sensor Signal
8 | 0.5 L-BU | 722 | Octane Switch Signal
9 | 0.5 GY | 121 | Engine Speed Signal
10 | 0.5 D-GN/WH | 762 | A/C Request Signal
11 | -- | -- | Not Used
12 | 0.5 D-BU | 473 | High Speed Cooling Fan Relay Control
13 | WH/BK | -- | Intake Manifold Tuning Valve Solenoid Control
14 | 0.5 PU | 1807 | CAN Serial Data High
15 | 0.5 PU | 2000 | Keyword Serial Data
16 | -- | -- | Not Used
17 | 0.5 GY | 605 | 5-Volt Reference
18 | 0.5 OG | 440 | Battery Positive Voltage
19 | 0.5 GY | 1936 | Fuel Gage
20-21 | -- | -- | Not Used
22 | 0.5 PU | 723 | Octane Switch Signal
23 | 0.5 D-GN/WH | 817 | Vehicle Speed Signal (Manual Transmission)
24 | 0.5 D-GN | 135 | Engine Coolant (ECT) Sensor Gage Signal
25 | -- | -- | Not Used
26 | 0.5 D-GN/WH | 465 | Fuel Pump Relay Control
27 | 0.5 D-GN/WH | 335 | Low Speed Cooling Fan Relay Control
28 | 0.5 D-GN | 67 | A/C Compressor Clutch Coil Supply Voltage
29 | -- | -- | Not Used
30 | 0.5 YE | 710 | CAN Serial Data Low
31 | 0.5 WH | 30 | Fuel Level Sensor Signal
32 | 0.5 BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control

### Engine Control Module (ECM) X1 (MR-140) (LDA)

#### Connector Part Information

- OEM: AMP 0-368434-2
- Description: 64-Way F ECU 64P Conn Ass'y (32-bit-B)

#### Engine Control Module (ECM) X1 (MR-140) (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG | 440 | Battery Positive Voltage
2-4 | -- | -- | Not Used
5 | 0.5 BK/WH | 51 | Ground
6 | 0.5 D-GN/WH | 817 | Vehicle Speed Signal (Manual Transmission)
7 | 0.5 D-BU | 876 | Rough Road Signal - W/ABS
8-11 | -- | -- | Not Used
12 | 0.5 D-BU | 473 | High Speed Cooling Fan Relay Control
13 | WH/BK | 962 | Intake Manifold Tuning Valve Solenoid Control
14 | 0.5 PU | 1807 | CAN Serial Data High
15 | 0.5 YE | 710 | CAN Serial Data Low
16 | BN/WH | 1669 | Heated Oxygen Sensor (HO2S) 1 Heater Control
17 | 0.5 OG | 440 | Battery Positive Voltage
18 | 0.5 PK/BU | 539 | Ignition 1 Voltage
19-20 | -- | -- | Not Used
21 | 0.5 D-GN | 602 | Rough Road Sensor Signal
22 | 0.5 L-BU | 380 | A/C Refrigerant Pressure (ACP) Sensor Signal
23 | -- | -- | Not Used
24 | 0.5 D-GN | 135 | Engine Coolant Temperature (ECT) Sensor Gage Signal
25 | 0.5 GY (WH) | 121 | Engine Speed Signal
26-27 | -- | -- | Not Used
28 | 0.5 D-GN/WH (D-GN) | 335 | Low Speed Cooling Fan Relay Control
29 | 0.5 D-GN (PU) | 67 | A/C Compressor Clutch Coil Supply Voltage
30 | 0.5 WH | 30 | Fuel Level Sensor Signal
31 | -- | -- | Not Used
32 | 0.5 PU | 2000 | Keyword Serial Data
33 | -- | -- | Not Used
34 | 0.5 PU/WH | 632 | Low Reference
35 | 0.5 D-GN/WH | 762 | A/C Request Signal
36 | 0.5 PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal
37-49 | -- | -- | Not Used
50 | 0.5 GY | 605 | 5-Volt Reference
51 | 0.5 GY | 1936 | Fuel Level Sensor Signal
52 | 0.5 YE/D-GN | 890 | Fuel Tank Pressure Sensor Signal
53 | 0.5 L-GN | 413 | Heated Oxygen Sensor (HO2S) 2 Low Reference
54 | 0.5 L-GN (D-GN/WH) | 465 | Fuel Pump Relay Control
55-63 | -- | -- | Not Used
64 | 0.5 BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control

### Engine Control Module (ECM) X2 (MR-140) (LDA)

#### Connector Part Information

- OEM: AMP 1-368434-1
- Description: 64-Way F ECU 64P Conn Ass'y (32-bit-B)

#### Engine Control Module (ECM) X2 (MR-140) (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU | 406 | Ignition Coil (IC) Timing Control 1 and 4
2 | 0.5 BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control
3 | 0.5 GY | 120 | Fuel Pump Supply Voltage
4 | 0.5 WH | 428 | Evaporative Emissions (EVAP) Canister Purge Solenoid Control
5 | 0.5 YE/BK | 1868 | Low Reference
6 | 0.5 GY (D-BU) | 417 | Throttle Position (TP) Sensor Signal
7 | 0.5 GY (BN) | 472 | Intake Air Temperature (IAT) Sensor Signal
8 | 0.5 D-BU/WH (L-GN) | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
9 | 0.5 WH/BK | 1456 | Exhaust Gas Recirculation (EGR) Valve Position Signal
10 | -- | -- | Not Used
11 | 0.5 D-GN/WH (L-BU/BK) | 844 | Fuel Injector 4 Control
12 | GY | 1653 | Heated Oxygen Sensor (HO2S) 1 Signal
13 | 0.5 BN | 1747 | Idle Air Control (IAC) A High Control
14 | 0.5 WH | 444 | Idle Air Control (IAC) B Low Control
15 | 0.5 YE/WH | 1748 | Idle Air Control (IAC) A Low Control
16 | 0.5 L-BU/BK | 1688 | 5-Volt Reference
17 | -- | -- | Not Used
18 | 0.5 YE/BK | 496 | Knock Sensor Signal
19 | 0.5 D-GN | 435 | Exhaust Gas Recirculation (EGR) Solenoid Low Control
20 | -- | -- | Not Used
21 | 0.5 D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
22 | 0.5 BN/WH (L-GN/BK) | 1745 | Fuel Injector 2 Control
23 | -- | -- | Not Used
24 | 0.5 D-GN/BK (PK/BK) | 1746 | Fuel Injector 3 Control
25 | 0.5 YE/D-BU (BK) | 1744 | Fuel Injector 1 Control
26 | 0.5 PU (BN/WH) | 633 | Camshaft Position (CMP) Sensor Signal
27 | -- | -- | Not Used
28 | 0.5 L-GN (YE) | 410 | Engine Coolant Temperature (ECT) Sensor Signal
29 | D-GN/RD | 1665 | Heated Oxygen Sensor (HO2S) 1 Low Reference
30 | 0.5 PU/WH | 1749 | Idle Air Control (IAC) Coil B High Control
31 | -- | -- | Not Used
32 | 0.5 D-GN/WH (D-GN/YE) | 416 | 5-Volt Reference
33 | 0.5 L-BU | 406 | Ignition Coil (IC) Timing Control (1 and 4)
34 | -- | -- | Not Used
35 | 0.5 D-GN/WH | 423 | Ignition Coil (IC) Timing Control (2 and 3)
36 | -- | -- | Not Used
37 | 0.5 BK/WH | 51 | Ground
38 | 0.5 BK/WH | 51 | Ground
39 | 0.5 BK/WH | 51 | Ground
40 | 0.5 BK/WH | 51 | Ground
41 | 0.5 BK/WH | 51 | Ground
42-47 | -- | -- | Not Used
48 | 0.5 OG/BK | 469 | Low Reference
49-50 | -- | -- | Not Used
51 | 0.5 D-GN/WH | 423 | Ignition Coil (IC) Timing Control (2 and 3)
52 | 0.5 D-GN | 435 | Exhaust Gas Recirulation (EGR) Low Control
53-63 | -- | -- | Not Used
64 | 0.5 BK (BK/YE) | 808 | Low Reference

### Engine Control Module (ECM) X1 (L34) w/Throttle Actuator Control

#### Connector Part Information

- OEM: AMP 0-368434-1
- Description: 64-Way F ECU 64P Conn Assembly (32-bit-B) (BK)

#### Engine Control Module (ECM) X1 (L34) w/Throttle Actuator Control

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/BK | 543 | 5-Volt Reference
2 | 0.5 GY | 605 | 5-Volt Reference
3 | 0.5 PU | 1550 | Low Reference
4 | 0.5 L-GN | 413 | Low Reference
5 | 0.5 PU/WH | 632 | Low Reference
6 | 0.5 BN | 488 | 5-Volt Reference
7-8 | -- | -- | Not Used
9 | 0.5 L-BU | 1450 | Low Reference
10-11 | -- | -- | Not Used
12 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
13 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
14 | -- | -- | Not Used
15 | 0.5 BN/WH | 379 | CPP Switch Signal (M/T)
16 | -- | -- | Not Used
17 | 0.5 OG | 440 | Battery Positive Voltage
18 | 0.5 OG | 440 | Battery Positive Voltage
19 | 0.5 BK/WH | 51 | Ground
20 | 0.5 BK/WH | 51 | Ground
21 | 0.5 BK/WH | 51 | Ground
22 | 0.5 BK/WH | 51 | Ground
23-24 | -- | -- | Not Used
25 | D-GN/WH | 762 | A/C Request Signal
26 | L-BU | 20 | Stop Lamp Switch Output
27 | -- | -- | Not Used
28 | BN | 17 | Stop Lamp Switch Output
29 | 0.5 WH | 791 | APP Sensor 2 Signal
30 | L-BU | 380 | A/C Pressure Sensor Signal
31 | 0.5 PU | 2000 | Serial Data
32 | -- | -- | Not Used
33 | 0.5 PK/D-BU | 539 | Ignition 1 Voltage
34 | 0.5 BK/WH | 51 | Ground
35 | D-GN | 67 | A/C Clutch Relay Control
36 | 0.5 BK | 441 | Main Relay Control
37 | WH | 183 | Cruise Indicator Control
38 | D-GN/WH | 817 | Vehicle Speed Signal (M/T)
39-40 | -- | -- | Not Used
41 | 0.5 GY | 121 | Engine Speed Signal
42 | 0.5 L-GN | 465 | Fuel Pump Relay Control
43 | 0.5 GY | 1936 | Fuel Level Sensor Signal
44 | 0.5 D-BU | 790 | APP Sensor 1 Signal
45 | 0.5 D-BU/WH | 397 | Cruise Control Switch Signal
46 | 0.5 PU | 1807 | CAN Serial Data High
47 | 0.5 YE/D-GN | 890 | Fuel Tank Pressure Sensor Signal
48 | 0.5 D-GN | 602 | Rough Road Sensor Signal w/o ABS
49 | 0.5 BN/WH | 419 | MIL Control
50 | D-GN/WH | 355 | Low Speed Cooling Fan Relay Control
51-55 | -- | -- | Not Used
56 | D-GN | 135 | Engine Coolant Temperature Gauge Control
57 | 0.5 BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control
58-60 | -- | -- | Not Used
61 | 0.5 WH | 30 | Fuel Gauge Control
62 | 0.5 PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal
63 | 0.5 YE | 710 | CAN Serial Data Low
64 | D-BU | 876 | Rough Road Signal w/ABS

### Engine Control Module (ECM) X2 (L34) w/Throttle Actuator Control

#### Connector Part Information

- OEM: AMP 1-368434-2
- Description: 64-Way F ECU 64P Conn Assembly (32-bit-B) (BN)

#### Engine Control Module (ECM) X2 (L34) w/Throttle Actuator Control

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.5 L-BU | 406 | Ignition Coil (IC) Timing Control 1 and 4
4 | 0.5 D-GN/WH | 423 | Ignition Coil (IC) Timing Control 2 and 3
5-6 | -- | -- | Not Used
7 | YE | 45 | Intake Manifold Tuning Valve Sensor Signal
8 | YE | 492 | Intake Manifold Tuning Valve Control
9-14 | -- | -- | Not Used
15 | 0.5 D-BU/RD | 581 | Electronic Throttle Control (ETC) (-)
16 | 0.5 D-BU/RD | 581 | Electronic Throttle Control (ETC) (-)
17-18 | -- | -- | Not Used
19 | 0.5 L-BU | 406 | Ignition Coil (IC) Timing Control 1 and 4
20 | 0.5 D-GN/WH | 423 | Ignition Coil (IC) Timing Control 2 and 3
21 | 0.5 D-BU/WH | 808 | Low Reference
22 | 0.5 YE/BK | 496 | Knock Sensor Signal
23-24 | -- | -- | Not Used
25 | 0.5 L-GN | 410 | Engine Coolant Temperature (ECT) Sensor Signal
26 | 0.5 D-GN/RK | 1665 | Heated Oxygen Sensor (HO2S) 1 Low Reference
27 | -- | -- | Not Used
28 | 0.5 D-BU/WH | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
29 | 0.5 GY | 534 | Throttle Position (TP) Sensor 2 Signal
30 | 0.5 GY | 471 | Intake Air Temperature (IAT) Sensor Signal
31 | 0.5 L-BU/WH | 582 | Electronic Throttle Control (ETC) (+)
32 | 0.5 L-BU/WH | 582 | Electronic Throttle Control (ETC) (+)
33 | 0.5 L-BU/BK | 1688 | 5-Volt Reference
34 | 0.5 GY | 1653 | Heated Oxygen Sensor (HO2S) 1Signal
35 | 0.5 OG/BK | 469 | Low Reference
36 | 0.6 D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
37 | 0.5 YE/BK | 1868 | Low Reference
38-40 | -- | -- | Not Used
41 | 0.5 D-GNWH | 417 | Throttle Position (TP) Sensor 1 Signal
42 | 0.5 WH/BK | 1456 | Exhaust Gas Recirculation (EGR) Valve Position Sensor Signal
43-45 | -- | -- | Not Used
46 | 0.5 PU | 633 | Camshaft Position (CMP) Sensor Signal
47-48 | -- | -- | Not Used
49 | 0.5 BN/WH | 1669 | Heated Oxygen Sensor (HO2S) 1 Heater Control
50 | 0.5 D-BU/YE | 474 | 5-Volt Reference
51 | 0.5 BK | 808 | Low Reference
52 | 0.5 BN | 426 | Low Reference
53 | 0.5 D-GN | 435 | Exhaust Gas Recirculation (EGR) Solenoid Valve Control
54 | 0.5 PK | 139 | Ignition 1 Voltage
55 | 0.5 D-GN/BK | 1746 | Fuel Injector 3 Control
56 | 0.5 BN/WH | 1745 | Fuel Injector 2 Control
57-60 | -- | -- | Not Used
61 | 0.5 L-BU/BK | 1986 | Evaporative Emissions (EVAP) Canister Vent Solenoid Control
62 | 0.5 WH | 428 | Evaporative Emissions (EVAP) Canister Purge Solenoid Control
63 | 0.5 YE/D-BU | 1744 | Fuel Injector 1 Control
64 | 0.5 D-GN/WH | 844 | Fuel Injector 4 Control

### Engine Control Module (ECM) X1 (MR-140) (L34) w/o Throttle Actuator Control

#### Connector Part Information

- OEM: AMP 0-368434-2
- Description: 64-Way F ECU 64P Conn Ass'y (32-bit-B)

#### Engine Control Module (ECM) X1 (MR-140) (L34) w/o Throttle Actuator Control

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG | 440 | Battery Positive Voltage
2-4 | -- | -- | Not Used
5 | 0.5 BK/WH | 51 | Ground
6 | 0.5 D-GN/WH | 817 | Vehicle Speed Signal (Manual Transmission)
7 | 0.5 D-BU | 876 | Rough Road Signal - W/ABS
8-11 | -- | -- | Not Used
12 | 0.5 D-BU | 473 | High Speed Cooling Fan Relay Control
13 | WH/BK | 962 | Intake Manifold Tuning Valve Solenoid Control
14 | 0.5 PU | 1807 | CAN Serial Data High
15 | 0.5 YE | 710 | CAN Serial Data Low
16 | BN/WH | 1669 | Heated Oxygen Sensor (HO2S) 1 Heater Control
17 | 0.5 OG | 440 | Battery Positive Voltage
18 | 0.5 PK/BU | 539 | Ignition 1 Voltage
19-20 | -- | -- | Not Used
21 | 0.5 D-GN | 602 | Rough Road Sensor Signal
22 | 0.5 L-BU | 380 | A/C Refrigerant Pressure (ACP) Sensor Signal
23 | -- | -- | Not Used
24 | 0.5 D-GN | 135 | Engine Coolant Temperature (ECT) Sensor Gage Signal
25 | 0.5 GY (WH) | 121 | Engine Speed Signal
26-27 | -- | -- | Not Used
28 | 0.5 D-GN/WH (D-GN) | 335 | Low Speed Cooling Fan Relay Control
29 | 0.5 D-GN (PU) | 67 | A/C Compressor Clutch Coil Supply Voltage
30 | 0.5 WH | 30 | Fuel Level Sensor Signal
31 | -- | -- | Not Used
32 | 0.5 PU | 2000 | Keyword Serial Data
33 | -- | -- | Not Used
34 | 0.5 PU/WH | 632 | Low Reference
35 | 0.5 D-GN/WH | 762 | A/C Request Signal
36 | 0.5 PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal
37-49 | -- | -- | Not Used
50 | 0.5 GY | 605 | 5-Volt Reference
51 | 0.5 GY | 1936 | Fuel Level Sensor Signal
52 | 0.5 YE/D-GN | 890 | Fuel Tank Pressure Sensor Signal
53 | 0.5 L-GN | 413 | Heated Oxygen Sensor (HO2S) 2 Low Reference
54 | 0.5 L-GN (D-GN/WH) | 465 | Fuel Pump Relay Control
55-63 | -- | -- | Not Used
64 | 0.5 BN/WH | 419 | Multifunction Indicator Lamp (MIL) Control

### Engine Control Module (ECM) X2 (MR-140) (L34) w/o Throttle Actuator Control

#### Connector Part Information

- OEM: AMP 1-368434-1
- Description: 64-Way F ECU 64P Conn Ass'y (32-bit-B)

#### Engine Control Module (ECM) X2 (MR-140) (L34) w/o Throttle Actuator Control

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU | 406 | Ignition Coil (IC) Timing Control 1 and 4
2 | 0.5 BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control
3 | 0.5 GY | 120 | Fuel Pump Supply Voltage
4 | 0.5 WH | 428 | Evaporative Emissions (EVAP) Canister Purge Solenoid Control
5 | 0.5 YE/BK | 1868 | Low Reference
6 | 0.5 GY (D-BU) | 417 | Throttle Position (TP) Sensor Signal
7 | 0.5 GY (BN) | 472 | Intake Air Temperature (IAT) Sensor Signal
8 | 0.5 D-BU/WH (L-GN) | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
9 | WH/BK | 1456 | Exhaust Gas Recirculation (EGR) Valve Position Signal
10 | -- | -- | Not Used
11 | 0.5 D-GN/WH (L-BU/BK) | 844 | Fuel Injector 4 Control
12 | GY | 1653 | Heated Oxygen Sensor (HO2S) 1 Signal
13 | 0.5 BN | 1747 | Idle Air Control (IAC) A High Control
14 | 0.5 WH | 444 | Idle Air Control (IAC) B Low Control
15 | 0.5 YE/WH | 1748 | Idle Air Control (IAC) A Low Control
16 | 0.5 L-BU/BK | 1688 | 5-Volt Reference
17 | -- | -- | Not Used
18 | 0.5 YE/BK | 496 | Knock Sensor Signal
19 | 0.5 D-GN | 435 | Exhaust Gas Recirculation (EGR) Solenoid Low Control
20 | -- | -- | Not Used
21 | 0.5 D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
22 | 0.5 BN/WH (L-GN/BK) | 1745 | Fuel Injector 2 Control
23 | -- | -- | Not Used
24 | 0.5 D-GN/BK (PK/BK) | 1746 | Fuel Injector 3 Control
25 | 0.5 YE/D-BU (BK) | 1744 | Fuel Injector 1 Control
26 | 0.5 PU (BN/WH) | 633 | Camshaft Position (CMP) Sensor Signal
27 | -- | -- | Not Used
28 | 0.5 L-GN (YE) | 410 | Engine Coolant Temperature (ECT) Sensor Signal
29 | D-GN/RD | 1665 | Heated Oxygen Sensor (HO2S) 1 Low Reference
30 | 0.5 PU/WH | 1749 | Idle Air Control (IAC) Coil B High Control
31 | -- | -- | Not Used
32 | 0.5 D-GN/WH (D-GN/YE) | 416 | 5-Volt Reference
33 | 0.5 L-BU | 406 | Ignition Coil (IC) Timing Control (1 and 4)
34 | -- | -- | Not Used
35 | 0.5 D-GN/WH | 423 | Ignition Coil (IC) Timing Control (2 and 3)
36 | -- | -- | Not Used
37 | 0.5 BK/WH | 51 | Ground
38 | 0.5 BK/WH | 51 | Ground
39 | 0.5 BK/WH | 51 | Ground
40 | 0.5 BK/WH | 51 | Ground
41 | 0.5 BK/WH | 51 | Ground
42-47 | -- | -- | Not Used
48 | 0.5 OG/BK | 469 | Low Reference
49-50 | -- | -- | Not Used
51 | 0.5 D-GN/WH | 423 | Ignition Coil (IC) Timing Control (2 and 3)
52 | 0.5 D-GN | 435 | Exhaust Gas Recirulation (EGR) Low Control
53-63 | -- | -- | Not Used
64 | 0.5BK (BK/YE) | 808 | Low Reference

### Engine Coolant Temperature (ECT) Sensor (L95, LXT)

#### Connector Part Information

- OEM: PED 12040753
- Description: 2-Way F Metri-Pack 150 Series, Sealed, Pull To Seat (BK)

#### Engine Coolant Temperature (ECT) Sensor (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE | 410 | Engine Coolant Temperature (ECT) Sensor Signal
2 | 0.5 BK/YE | 808 | Low Reference

### Engine Coolant Temperature (ECT) Sensor (L79)

#### Connector Part Information

- OEM: PED 12040753
- Description: 2-Way F Metri-Pack 150 Series Sealed, Pull To Seat (BK)

#### Engine Coolant Temperature (ECT) Sensor (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK/YE | 808 | Low Reference
B | 0.5 YE | 410 | Engine Coolant Temperature (ECT) Sensor Signal

### Engine Coolant Temperature (ECT) Sensor (LDA)

#### Connector Part Information

- OEM: PED 12040753
- Description: 2-Way F Metri-Pack 150 Series Sealed, Pull To Seat (BK)

#### Engine Coolant Temperature (ECT) Sensor (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK (BK/YE) | 808 | Low Reference
B | 0.5 L-GN (YE) | 410 | Engine Coolant Temperature (ECT) Sensor Signal

### Engine Coolant Temperature (ECT) Sensor (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12040753
- Description: 2-Way F Metri-Pack 150 Series Sealed, Pull To Seat (BK)

#### Engine Coolant Temperature (ECT) Sensor (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 410 | Engine Coolant Temperature (ECT) Sensor Signal
2 | 0.5 BK | 808 | Low Reference

### Engine Coolant Temperature (ECT) Sensor (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12040753
- Description: 2-Way F Metri-Pack 150 Series Sealed, Pull To Seat (BK)

#### Engine Coolant Temperature (ECT) Sensor (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK (BK/YE) | 808 | Low Reference
B | 0.5 L-GN (YE) | 410 | Engine Coolant Temperature (ECT) Sensor Signal

### Engine Coolant Temperature (ECT) Sensor (LMN)

#### Connector Part Information

- OEM: PED 12040753
- Description: 2-Way F 150 Series Sealed

#### Engine Coolant Temperature (ECT) Sensor (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | -- | Signal
2 | BN | -- | Ground

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (L95, LXT)

#### Connector Part Information

- OEM: AMP 85202-1
- Description: 2-Way F JR Power Timer 2P Hsg Ass'y (BK)

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
2 | 0.5 D-GN/WH | 428 | EVAP Canister Purge Solenoid Control

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (L79)

#### Connector Part Information

- OEM: PED 12052643
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
2 | D-GN/WH | 428 | Evaporative Emission (EVAP) Canister Purge Solenoid Control

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (LDA)

#### Connector Part Information

- OEM: PED 12052643
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
2 | 0.5 WH | 428 | Evaporative Emission (EVAP) Canister Purge Solenoid Control

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12052643
- Description: 2-Way F Metri-Pack 150 Series Sealed (BN)

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
2 | 0.5 WH | 428 | Evaporative Emission (EVAP) Canister Purge Solenoid Control

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (w/o Throttle Actuator) (L34)

#### Connector Part Information

- OEM: PED 12052643
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 1846 | Ignition 1 Voltage
B | 0.5 WH | 428 | Evaporative Emission (EVAP) Canister Purge Solenoid Control

### Evaporative Emission (EVAP) Canister Vent Solenoid Valve (LDA)

#### Connector Part Information

- OEM: PED 12052643
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Evaporative Emission (EVAP) Canister Vent Solenoid Valve (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
2 | L-BU/PU | 428 | Evaporative Emission (EVAP) Canister Vent Solenoid Control

### Evaporative Emission (EVAP) Canister Vent Solenoid (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12052643
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Evaporative Emission (EVAP) Canister Vent Solenoid (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU/PU | 1986 | Evaporative Emission (EVAP) Canister Vent Solenoid Control
2 | 0.5 PK/BK | 1846 | Ignition 1 Voltage

### Evaporative Emission (EVAP) Canister Vent Solenoid Valve (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12052643
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Evaporative Emission (EVAP) Canister Vent Solenoid Valve (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | 1846 | Ignition 1 Voltage
2 | L-BU/PU | 428 | Evaporative Emission (EVAP) Canister Vent Solenoid Control

### Exhaust Gas Recirculation (EGR) Valve (ECE 83 Emissions) (L95, LXT)

#### Connector Part Information

- OEM: AMP 368530
- Description: 2-Way M Econoseal J Mark II + Connector Plug Housing (BK)

#### Exhaust Gas Recirculation (EGR) Valve (ECE 83 Emissions) (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY | 435 | Exhaust Gas Recirculation (EGR) Solenoid Control
2 | 0.5 PK | 139 | Ignition 1 Voltage

### Exhaust Gas Recirculation (EGR) Valve (Euro III Emissions) (L95, LXT)

#### Connector Part Information

- OEM: AMP 368530-1
- Description: 6-Way F Econoseal J-Mark II + 6P (BK)

#### Exhaust Gas Recirculation (EGR) Valve (Euro III Emissions) (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 416 | 5-Volt Reference Voltage
2 | BK/YE | 808 | Sensor Ground
3 | BN | 1456 | Exhaust Gas Recirculation (EGR) Signal
4 | PK | 139 | Ignition 1 Voltage
5 | -- | -- | Not Used
6 | GY | 435 | Exhaust Gas Recirculation (EGR) Solenoid Low Control

### Exhaust Gas Recirculation (EGR) Valve (Euro IV Emissions) (L95, LXT)

#### Connector Part Information

- OEM: AMP 368530-1
- Description: 6-Way F Econoseal J-Mark II + 6P (BK)

#### Exhaust Gas Recirculation (EGR) Valve (Euro IV Emissions) (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY | 435 | Exhaust Gas Recirculation (EGR) Solenoid Low Control
2 | 0.5 BK/YE | 808 | Sensor Ground
3 | 0.5 BN | 1456 | Exhaust Gas Recirculation (EGR) Signal
4 | 0.5 GY | 416 | 5-Volt Reference Voltage
5 | 0.5 PK | 139 | Ignition 1 Voltage
6 | -- | -- | Not Used

### Exhaust Gas Recirculation (EGR) Valve (LDA)

#### Connector Part Information

- OEM: PED 12186139
- Description: 5-Way F Metri-Pack 150 Series Sealed, Pull To Seat (L-GY)

#### Exhaust Gas Recirculation (EGR) Valve (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 435 | Exhaust Gas Recirulation (EGR) Solenoid Low Control
2 | 0.5 OG/BK | 469 | Low Reference
3 | 0.5 WH/BK | 1456 | Exhaust Gas Recirulation (EGR) Valve Position Signal
4 | 0.5 L-BU/BK | 1688 | 5-Volt Reference
5 | 0.5 GY | 120 | Fuel Pump Supply Voltage

### Exhaust Gas Recirculation (EGR) Valve (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12186139
- Description: 5-Way F Metri-Pack 150 Series Sealed, Pull To Seat (L-GY)

#### Exhaust Gas Recirculation (EGR) Valve (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 435 | Exhaust Gas Recirulation (EGR) Solenoid Low Control
2 | 0.5 OG/BK | 469 | Low Reference
3 | 0.5 WH | 1456 | Exhaust Gas Recirulation (EGR) Valve Position Signal
4 | 0.5 L-BU/BK | 1688 | 5-Volt Reference
5 | 0.5 PK | 120 | Supply Voltage

### Exhaust Gas Recirculation (EGR) Valve (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12186139
- Description: 5-Way F Metri-Pack 150 Series Sealed, Pull To Seat (L-GY)

#### Exhaust Gas Recirculation (EGR) Valve (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN | 435 | Exhaust Gas Recirulation (EGR) Solenoid Low Control
B | 0.5 OG/BK | 469 | Low Reference
C | 0.5 WH/BK | 1456 | Exhaust Gas Recirulation (EGR) Valve Position Signal
D | 0.5 L-BU/BK | 1688 | 5-Volt Reference
E | 0.5 GY | 120 | Fuel Pump Supply Voltage

### Exhaust Gas Recirculation (EGR) Valve (LMN)

#### Connector Part Information

- OEM: TYCO 827551-3
- Description: 2-Way F Timmer Sealed

#### Exhaust Gas Recirculation (EGR) Valve (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GN/WH | -- | EGR Solenoid Control
2 | PK/WH | -- | Battery Positive Voltage

### Exhaust Gas Temperature Sensor 1 - (LMN)

#### Connector Part Information

- OEM: 621-02020
- Description: 2-Way F

#### Exhaust Gas Temperature Sensor 1 (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | -- | Signal
2 | BU/WH | -- | Ground

### Exhaust Gas Temperature Sensor 2 (LMN)

#### Connector Part Information

- OEM: 621-02020
- Description: 2-Way F

#### Exhaust Gas Temperature Sensor 2 (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/BK | -- | Signal
2 | YE/WH | -- | Ground

### Fog Lamp - Left Front

#### Connector Part Information

- OEM: PED 12020599
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Fog Lamp - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 34 | Front Fog Lamp Supply Voltage
B | BK | 50 | Ground

### Fog Lamp - Left Rear (T79)

#### Connector Part Information

- OEM: 12092379
- Description: 3-Way F Lamp Socket Wedge Base W3 (BK)

#### Fog Lamp - Left Rear (T79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | 122 | Rear Fog Lamp Supply Voltage
B | -- | -- | Not Used
G | BK/WH | 70 | Ground

### Fog Lamp - Right Front

#### Connector Part Information

- OEM: PED 12020599
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Fog Lamp - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 34 | Front Fog Lamp Supply Voltage
B | BK | 150 | Ground

### Fog Lamp - Right Rear (T79)

#### Connector Part Information

- OEM: 12092379
- Description: 3-Way F Lamp Socket Wedge Base W3 (BK)

#### Fog Lamp - Right Rear (T79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | 122 | Rear Fog Lamp Supply Voltage
B | -- | -- | Not Used
G | BK/WH | 70 | Ground

### Fuel Filter Heater/Temperature Sensor (LMN)

#### Connector Part Information

- OEM: FCI 17260406A
- Description: 6-Way F 150/280 Series Sealed

#### Fuel Filter Heater/Temperature Sensor (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | BK | -- | Ground
4 | PU | -- | Fuel Filter Heater Supply Voltage
5 | L-GN/BK | -- | Fuel Temperature Signal
6 | YE/BK | -- | Fuel Temperature Ground

### Fuel Injector 1 (LMN)

#### Connector Part Information

- OEM: BOSCH 1928403874
- Description: 2-Way F Sealed

#### Fuel Injector 1 (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BK | -- | Control
2 | WH | -- | Low Reference

### Fuel Injector 2 (LMN)

#### Connector Part Information

- OEM: BOSCH 1928403874
- Description: 2-Way F Sealed

#### Fuel Injector 2 (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN/BK | -- | Control
2 | PU | -- | Low Reference

### Fuel Injector 3 (LMN)

#### Connector Part Information

- OEM: BOSCH 1928403874
- Description: 2-Way F Sealed

#### Fuel Injector 3 (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | Control
2 | BN/WH | -- | Low Reference

### Fuel Injector 4 (LMN)

#### Connector Part Information

- OEM: BOSCH 1928403874
- Description: 2-Way F Sealed

#### Fuel Injector 4 (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GN | -- | Control
2 | WH/BK | -- | Low Reference

### Fuel Injectors (L95, LXT)

#### Connector Part Information

- OEM: AMP 85202-1
- Description: 2-Way F JR Power Timer 2P Hsg Ass'y (BK)

#### Fuel Injectors (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK | 139 | Ignition 1 Voltage
2 | 0.5 BK | 1744 | Fuel Injector 1 Control
0.5 L-GN/BK | 1745 | Fuel Injector 2 Control
0.5 PK/BK | 1746 | Fuel Injector 3 Control
0.5 L-BU/BK | 844 | Fuel Injector 4 Control

### Fuel Injectors (L79)

#### Connector Part Information

- OEM: PED 15326181
- Description: 2-Way F Micro-Pack 064 Series Sealed (BK)

#### Fuel Injectors (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK | 139 | Ignition 1 Voltage
B | BK | 1744 | Fuel Injector 1 Control
L-GN/BK | 1745 | Fuel Injector 2 Control
PK/BK | 1746 | Fuel Injector 3 Control
L-BU/BK | 844 | Fuel Injector 4 Control

### Fuel Injectors (LDA)

#### Connector Part Information

- OEM: PED 15326181
- Description: 2-Way F Micro-Pack 064 Series Sealed (BK)

#### Fuel Injectors (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK | 139 | Ignition 1 Voltage
B | YE/BU (BK) | 1744 | Fuel Injector 1 Control
BN/WH (L-GN/BK) | 1745 | Fuel Injector 2 Control
D-GN/BK (PK/BK) | 1746 | Fuel Injector 3 Control
D-GN/WH(L-BU/BK) | 844 | Fuel Injector 4 Control

### Fuel Injectors (L34)

#### Connector Part Information

- OEM: PED 15305086
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Fuel Injectors (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 139 | Ignition 1 Voltage
B | 0.5 YE/D-BU | 1744 | Fuel Injector 1 Control
0.5 BN/WH | 1745 | Fuel Injector 2 Control
0.5 D-GN/BK | 1746 | Fuel Injector 3 Control
0.5 D-GN/WH | 844 | Fuel Injector 4 Control

### Fuel Injectors (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 15326181
- Description: 2-Way F Micro-Pack 064 Series Sealed (BK)

#### Fuel Injectors (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK | 139 | Ignition 1 Voltage
B | 0.5 YE/BU (BK) | 1744 | Fuel Injector 1 Control
0.5 BN/WH (L-GN/BK) | 1745 | Fuel Injector 2 Control
0.5 D-GN/BK (PK/BK) | 1746 | Fuel Injector 3 Control
0.5 D-GN/WH (L-BU/BK | 844 | Fuel Injector 4 Control

### Fuel Pump/Sender

#### Connector Part Information

- OEM: AMP 936039
- Description: 6-Way F Fuel Pump 6POS Conn'r Ass'y (BN)

#### Fuel Pump/Sender

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 1936 | Fuel Level Sensor Signal
2 | BK | 1250 | Ground
PU/BK | 632 | Low Reference (Diesel)
3 | GY | 120 | Fuel Pump Supply Voltage
4 | BK | 1250 | Ground
5 | PU | 172 | Low Fuel Indicator Control
6 | PU/BK | 632 | Low Reference

### Fuel Pump (L79)

#### Connector Part Information

- OEM: AMP 936039
- Description: 6-Way Fuel Pump 6POS CONN'R ASS'Y

#### Fuel Pump (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-BU | 1936 | Fuel Level Sensor Signal
2 | 1.25 BK | 1250 | Ground
3 | 0.5 GY | 120 | Fuel Pump Supply Voltage
4 | 0.5 BK | 1250 | Ground
5 | 0.5 PU | 172 | Low Fuel Indicator Control
6 | 0.5 PU/BK | 632 | Low Reference

### Fuel Pump (LDA)

#### Connector Part Information

- OEM: AMP 936039
- Description: 6-Way Fuel Pump 6POS CONN'R ASS'Y

#### Fuel Pump (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 1936 | Fuel Level Sensor Signal
2 | BK | 1250 | Ground
3 | GY | 120 | Fuel Pump Supply Voltage
4 | BK | 1250 | Ground
5 | PU | 172 | Low Fuel Indicator Control
6 | PU/BK | 632 | Low Reference

### Fuel Pump (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 936039
- Description: 6-Way Fuel Pump 6POS CONN'R ASS'Y

#### Fuel Pump (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 1936 | Fuel Level Sensor Signal
2 | 1.25 BK | 1250 | Ground
3 | 1.25 GY | 120 | Fuel Pump Supply Voltage
4 | BK | 1250 | Ground
5 | PU | 172 | Low Fuel Indicator Control
6 | PU/BK | 632 | Low Reference

### Fuel Pump/Sender (L95, LXT)

#### Connector Part Information

- OEM: AMP 936039
- Description: 6-Way F Fuel Pump 6POS Conn'r Ass'y (BN)

#### Fuel Pump/Sender (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-BU | 1936 | Fuel Level Sensor Signal
2 | 1.25 BK | 1250 | Ground
3 | 0.5 GY | 120 | Fuel Pump Supply Voltage
4 | 0.5 BK | 1250 | Ground
5 | 0.5 PU | 172 | Low Fuel Indicator Control
6 | 0.5 PU/BK | 632 | Low Reference

### Fuel Pump/Sender (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 936039
- Description: 6-Way F Fuel Pump 6POS Connector Assembly (BN)

#### Fuel Pump/Sender (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 1936 | Fuel Level Sensor Signal
2 | 1.25 BK | 1250 | Ground
3 | 1.25 GY | 120 | Fuel Pump Supply Voltage
4 | BK | 1250 | Ground
5 | PU | 172 | Low Fuel Indicator Control
6 | PU/BK | 632 | Low Reference

### Fuel Pump Module (LMN)

#### Connector Part Information

- OEM: KET MG641521
- Description: 5-Way F 090II Sealed

#### Fuel Pump Module (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BU | -- | Fuel Level +
2 | PU/BK | -- | Fuel Level -
3 | -- | -- | Not Used
4 | BK | -- | Ground
5 | GY | -- | Fuel Pump Supply Voltage

### Fuel Rail Pressure Control Valve (LMN)

#### Connector Part Information

- OEM: BOSCH 1928403874
- Description: 2-Way F Sealed

#### Fuel Rail Pressure Control Valve (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/BK | -- | Control
2 | BN/WH | -- | 12V

### Fuel Rail Pressure Sensor (LMN)

#### Connector Part Information

- OEM: BOSCH 1928403968
- Description: 2-Way F Sealed

#### Fuel Rail Pressure Sensor (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GN/WH | -- | Ground
2 | GY/BK | -- | Signal
3 | L-BU | -- | 5-Volt Reference

### Fuel Tank Pressure Sensor (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12059595
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Fuel Tank Pressure Sensor (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK/WH | 632 | Low Reference
2 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
3 | 0.5 GY | 605 | 5-Volt Reference

### Generator

#### Connector Part Information

- OEM: PED 12186568
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Generator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | BN | 25 | Charge Indicator Control/Signal
C | PK/D-BU | 539 | Ignition 1 Voltage
D | -- | -- | Not Used

### Glow Plug Control Unit (LMN)

#### Connector Part Information

- OEM: FCI 60432001
- Description: 11-Way F Sealed

#### Glow Plug Control Unit (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Glow Plug 4 Supply Voltage
2 | PU | -- | Glow Plug 3 Supply Voltage
3 | PU | -- | Glow Plug 2 Supply Voltage
4 | PU | -- | Glow Plug 1 Supply Voltage
5 | -- | -- | Not Used
6 | PK | -- | Ignition Voltage
7 | BK | -- | Ground
8 | -- | -- | Not Used
9 | WH | -- | Diagnosis
10 | RD/WH | -- | Battery Positive Voltage
11 | WH/RD | -- | Glow Plug Control

### Hazard Switch

#### Connector Part Information

- OEM: KET MG 651056
- Description: 10-Way F 090-II Series (WH)

#### Hazard Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | D-GN | 44 | Instrument Panel Lamps Dimmer Switch
3 | BN/WH | 309 | Right Park Lamp Supply Voltage
4 | BN | 27 | Hazard Flasher Signal (Optional)
5 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
6 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
7 | L-BU | 1508 | Turn Signal Switch Signal
8 | OG | 1040 | Battery Positive Voltage
9 | PK | 16 | Turn Signal Flasher Signal
10 | PK | 339 | Ignition 1 Voltage

### Headlamp - High Beam - Left

#### Connector Part Information

- OEM: 12033701
- Description: 2-Way F Metri-Pack 480 Series, Sealed (BK)

#### Headlamp - High Beam - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | RD | 711 | Left Headlamp High Beam Supply Voltage
B | BK/WH | 1250 | Ground

### Headlamp - High Beam - Right

#### Connector Part Information

- OEM: 12033701
- Description: 2-Way F Metri-Pack 480 Series, Sealed (BK)

#### Headlamp - High Beam - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | RD | 311 | Right Headlamp High Beam Supply Voltage
B | BK/WH | 1250 | Ground

### Headlamp - Low Beam - Left

#### Connector Part Information

- OEM: 12033701
- Description: 2-Way F Metri-Pack 480 Series, Sealed (BK)

#### Headlamp - Low Beam - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-GN | 712 | Left Headlamp Low Beam Supply Voltage
B | BK/WH | 250 | Ground

### Headlamp - Low Beam - Right

#### Connector Part Information

- OEM: 12033701
- Description: 2-Way F Metri-Pack 480 Series, Sealed (BK)

#### Headlamp - Low Beam - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 312 | Right Headlamp Low Beam Supply Voltage
B | BK/WH | 250 | Ground

### Headlamp Leveling Switch (TR6)

#### Connector Part Information

- OEM: MOLEX 5557-06R
- Description: 6-Way F Mini Fit Conn. Rec. Housing (WH)

#### Headlamp Leveling Switch (TR6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.3 BN/WH | 309 | Right Park Lamp Supply Voltage
2 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage
3 | PU | 12 | Headlamp Low Beam Supply Voltage
4 | D-GN | 44 | Instrument Panel Lamps Dimming Control
5 | -- | -- | Not Used
6 | BK | 250 | Ground

### Headlamp Switch

#### Connector Part Information

- OEM: MOLEX 5559-06P
- Description: 6-Way Mini Fit Conn. Crimp Pin Housing (BK)

#### Headlamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | 309 | Right Park Lamp Supply Voltage (w/o North America DRL)
PU | 12 | Headlamp Low Beam Supply Voltage (w/North America DRL)
2 | GY/BK | 1798 | Headlamp Relay Control
3 | BK | 250 | Ground
4 | -- | -- | Not Used
5 | YE | 317 | Front Fog Relay Coil Supply Voltage
6 | WH | 1080 | Park Lamp Relay Control

### Heated Oxygen Sensor 1 (HO2S1) (LDA)

#### Connector Part Information

- OEM: PED 12162144
- Description: 4-Way F Metri-Pack 150 Series Sealed (BK)

#### Heated Oxygen Sensor 1 (HO2S1) (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/RD | 1665 | Heated Oxygen Sensor (HO2S) 1 Low Reference
2 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
3 | GY | 1653 | Heated Oxygen Sensor (HO2S) 1 Signal
4 | BN/WH | 1669 | Heated Oxygen Sensor (HO2S) 1 Heater Control

### Heated Oxygen Sensor 1 (HO2S1) (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12162144
- Description: 4-Way F Metri-Pack 150 Series Sealed (BK)

#### Heated Oxygen Sensor 1 (HO2S1) (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/RD | 1665 | Heated Oxygen Sensor (HO2S) 1 Low Reference
2 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
3 | GY | 1653 | Heated Oxygen Sensor (HO2S) 1 Signal
4 | BN/WH | 1669 | Heated Oxygen Sensor (HO2S) 1 Heater Control

### Heated Oxygen Sensor 2 (HO2S2) (LDA)

#### Connector Part Information

- OEM: AMP 174257-2
- Description: 4-Way F 070 Series Econoseal-J MK-2 Cap Hsg 4P (BK)

#### Heated Oxygen Sensor 2 (HO2S2) (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal
2 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
3 | 0.5 L-GN | 413 | Heated Oxygen Sensor (HO2S) 2 Low Reference
4 | 0.5 BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control

### Heated Oxygen Sensor 2 (HO2S2) (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 174257-2
- Description: 4-Way F 070 Series Econoseal-J MK-2 Cap Hsg 4P (BK)

#### Heated Oxygen Sensor 2 (HO2S2) (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal
2 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
3 | 0.5 L-GN | 413 | Heated Oxygen Sensor (HO2S) 2 Low Reference
4 | 0.5 BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control

### Heated Oxygen Sensor 2 (HO2S2) (Mexico, Japan) (LDA)

#### Connector Part Information

- OEM: AMP 174257-2
- Description: 4-Way F 070 Series Econoseal-J MK-2 Cap Hsg 4P (BK)

#### Heated Oxygen Sensor 2 (HO2S2) (Mexico, Japan) (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
2 | 0.5 PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal
3 | 0.5 BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control
4 | 0.5 L-GN | 413 | Heated Oxygen Sensor (HO2S) 2 Low Reference

### Heated Oxygen Sensor 2 (HO2S2) (Mexico, Japan) (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 174257-2
- Description: 4-Way F 070 Series Econoseal-J MK-2 Cap Hsg 4P (BK)

#### Heated Oxygen Sensor 2 (HO2S2) (Mexico, Japan) (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
2 | 0.5 PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal
3 | 0.5 BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control
4 | 0.5 L-GN | 413 | Heated Oxygen Sensor (HO2S) 2 Low Reference

### Heated Oxygen Sensor (HO2S) 1 (L95, LXT)

#### Connector Part Information

- OEM: AMP 174257-2
- Description: 4-Way M 070 Series Econoseal J MK-2 Plug Ass'y 4P (BK)

#### Heated Oxygen Sensor (HO2S) 1 (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1665 PU/WH | 1665 | Heated Oxygen Sensor (HO2S) 1 Low Reference
2 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
3 | 0.5 OG/BK | 469 | Heated Oxygen Sensor (HO2S) 1 Heater Control
4 | 0.5 BN/WH | 1666 | Heated Oxygen Sensor (HO2S) 1 Signal

### Heated Oxygen Sensor (HO2S) 1 (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12162144
- Description: 4-Way F Metri-Pack 150 Series Sealed (BK)

#### Heated Oxygen Sensor (HO2S) 1 (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN/RD | 1665 | Heated Oxygen Sensor (HO2S) 1 Low Reference
2 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
3 | 0.5 GY | 1653 | Heated Oxygen Sensor (HO2S) 1 Signal
4 | 0.5 BN/WH | 1669 | Heated Oxygen Sensor (HO2S) 1 Heater Control

### Heated Oxygen Sensor (HO2S) 2 (L95, LXT)

#### Connector Part Information

- OEM: AMP 174257-2
- Description: 4-Way M 070 Series Econoseal J MK-2 Plug Ass'y 4P (BK)

#### Heated Oxygen Sensor (HO2S) 2 (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Low Reference
2 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
3 | 0.5 L-GN | 413 | Heated Oxygen Sensor (HO2S) 2 Heater Control
4 | 0.5 BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Signal

### Heated Oxygen Sensor (HO2S) 2 (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 174259-2
- Description: 4-Way F 070 Series Econoseal-J MK-2 Cap Hsg 4P (BK)

#### Heated Oxygen Sensor (HO2S) 2 (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Signal
2 | 0.5 PK/BK | 1846 | Ignition 1 Voltage
3 | 0.5 L-GN | 413 | Low Reference
4 | 0.5 BN/BK | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control

### High Pressure Pump (LMN)

#### Connector Part Information

- OEM: BOSCH 1928403874
- Description: 2-Way F Sealed

#### High Pressure Pump (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | -- | Signal
2 | GN | -- | Control

### High Speed Blower Motor Relay (C68)

#### Connector Part Information

- OEM: AK 36409
- Description: 4-Way F (GY)

#### High Speed Blower Motor Relay (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
30 | 3 BK | 350 | Ground
85 | 0.5 D-BU/BK | 247 | High Speed Blower Relay Control
86 | 0.85 BN | 41 | Ignition 2 Voltage
87 | 3 PU | 743 | Blower Motor Speed Control

### Hold Mode Switch (M98)

#### Connector Part Information

- OEM: KET MG652999
- Description: 4-Way F 040 Unsealed

#### Hold Mode Switch (M98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GN/WH | -- | Hold Mode Switch Signal
2 | BN/WH | -- | Illumination Supply Voltage
3 | GN | -- | Illumination Control
4 | BK | -- | Ground

### Hood Ajar Switch

#### Connector Part Information

- OEM: KET MG 610392
- Description: 2-Way F SDL Series (WH)

#### Hood Ajar Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 109 | Hood Ajar Switch Signal
2 | 0.5 OG | 1240 | Battery Positive Voltage

### Horn

#### Connector Part Information

- OEM: KET MG 641156
- Description: 2-Way F 090 WP Series (GY)

#### Horn

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 50 | Ground (Signal Horn)
0.5 BK | 150 | Ground (Dual Horn)
2 | 0.5 D-GN | 29 | Horn Control (Signal Horn)
0.5 BK/WH | 29 | Horn Control (Dual Horn)

### HVAC Control Module X1 (C68)

#### Connector Part Information

- OEM: MOLEX 51155-1615
- Description: 16-Way F

#### HVAC Control Module X1 (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 350 | Ground
2 | 0.3 L-BU | 1316 | Air Temperature Door Control
3 | 0.3 D-GN | 44 | Instrument Panel Lamps Dimmer Switch Signal
4 | 0.3 BN/WH | 309 | Right Park Lamp Voltage
5 | 0.5 BN | 41 | Ignition 2 Voltage
6-7 | -- | -- | Not Used
8 | 0.3 YE | 1791 | Low Reference
9 | -- | -- | Not Used
10 | 0.5 D-BU/BK | 247 | High Speed Blower Relay Control
11 | 0.5 D-GN/WH | 762 | A/C Request Signal
12 | 0.3 WH | 193 | Rear Defog Relay Control
13 | 0.5 YE | 61 | Low Reference
14 | 0.3 OG | 1140 | Battery Positive Voltage
15 | -- | -- | Not Used
16 | 0.3 D-GN | 1910 | Inside Air Temperature Sensor Signal

### HVAC Control Module X2 (C68)

#### Connector Part Information

- OEM: MOLEX 51155-2015
- Description: 20-Way F

#### HVAC Control Module X2 (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.3 GY/BK | 754 | Blower Motor Speed Signal
2 | 0.5 D-GN/RD | 817 | Vehicle Speed Signal
3 | -- | -- | Not Used
4 | 0.3 BN | 1812 | Low Reference
5 | 0.3 YE/BK | 1814 | Lower Mode Door Position Signal
6 | 0.3 BK | 1199 | Air Temperature Door Control
7 | 0.5 D-GN | 95 | Windshield Washer Switch Signal
8 | 0.5 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
9 | 0.5 GY/BK | 1596 | Coolant Temperature Sensor Signal
10 | 0.5 L-BU/BK | 590 | Sunload Sensor Signal
11 | 0.5 BK | 350 | Ground
12 | 1.25 D-BU | 188 | Blower Motor Resistor Assembly Supply Voltage
13 | 0.3 PK/WH | 1648 | Recirculation Door Control A
14 | 0.3 D-GN/BK | 1647 | Recirculation Door Control B
15 | -- | -- | Not Used
16 | 0.3 D-GN/BK | 1395 | Upper Mode Valve Solenoid Control
17 | 0.3 PK | 1396 | Defrost Mode Valve Solenoid Control
18 | 0.3 YE/BU | 1397 | Lower Mode Valve Solenoid Control
19 | 0.3 WH/BK | 1398 | Mode Valve Signal
20 | PK/BK | 1399 | Mode Valve Signal

### HVAC Control Module (C60)

#### Connector Part Information

- OEM: KET MG 610376
- Description: 12-Way F PCB 040 Series (WH)

#### HVAC Control Module (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | PK | 239 | Ignition 1 Voltage
A2 | WH | 193 | Rear Defog Relay Control
A3 | BK | 1050 | Ground
A4 | L-GN/BK | 1647 | Recirculation Door Control B
A5 | PK/WH | 1648 | Recirculation Door Control A
A6 | OG | 1140 | Battery Positive Voltage
A7 | OG | 52 | Blower Motor High Control
A8 | D-GN/WH | 762 | A/C Request Signal
A9 | BN/WH | 309 | Right Park Lamp Supply Voltage
A10 | D-GN | 44 | Instrument Panel Lamps Dimming Control
A11-A12 | -- | -- | Not Used

### I/P Compartment Lamp

#### Connector Part Information

- OEM: AK 36277
- Description: 2-Way F SWP Series (BK)

#### I/P Compartment Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | 175 | I/P Compartment Lamp Signal
2 | BK | 1050 | Ground

### I/P Compartment Lamp Switch

#### Connector Part Information

- OEM: F2-14
- Description: 2-Way F SWP Series (BK)

#### I/P Compartment Lamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 1540 | Battery Positive Voltage (w/Rear Fog Lamps) (w/Lamp Driver Control Module)
2 | PU | 175 | I/P Compartment Lamp Signal

### I/P Dimmer Switch

#### Connector Part Information

- OEM: KET MG 610045
- Description: 3-Way F 250 Series (WH)

#### I/P Dimmer Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 44 | Instrument Panel Lamps Dimmer Switch
2 | BK | 250 | Ground
3 | BN/WH | 309 | Right Park Lamp Supply Voltage

### Idle Air Control (IAC) Valve (L79)

#### Connector Part Information

- OEM: PED 12040754
- Description: 4-Way F Black Metri-Pack 150 Series (BK)

#### Idle Air Control (IAC) Valve (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | 444 | Idle Air Control (IAC) Coil B Low Control
B | 0.5 PU/WH | 1749 | Idle Air Control (IAC) Coil B High Control
C | 0.5 YE/WH | 1748 | Idle Air Control (IAC) Coil A Low Control
D | 0.5 BN | 1747 | Idle Air Control (IAC) Coil A High Control

### Idle Air Control (IAC) Valve (LDA)

#### Connector Part Information

- OEM: PED 12040754
- Description: 4-Way F Black Metri-Pack 150 Series (BK)

#### Idle Air Control (IAC) Valve (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | 444 | Idle Air Control (IAC) Coil B Low Control
B | 0.5 PU/WH | 1749 | Idle Air Control (IAC) Coil B High Control
C | 0.5 YE/WH | 1748 | Idle Air Control (IAC) Coil A Low Control
D | 0.5 BN | 1747 | Idle Air Control (IAC) Coil A High Control

### Idle Air Control (IAC) Valve (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12040754
- Description: 4-Way F Black Metri-Pack 150 Series (BK)

#### Idle Air Control (IAC) Valve (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | 444 | Idle Air Control (IAC) Coil B Low Control
B | 0.5 PU/WH | 1749 | Idle Air Control (IAC) Coil B High Control
C | 0.5 YE/WH | 1748 | Idle Air Control (IAC) Coil A Low Control
D | 0.5 BN | 1747 | Idle Air Control (IAC) Coil A High Control

### Ignition Coil (IC) Module (L79)

#### Connector Part Information

- OEM: PED 12059595
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Ignition Coil (IC) Module (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 406 | Ignition Coil (IC) Timing Control (1 and 4)
B | 0.5 PK | 739 | Ignition 1 Voltage
C | 0.5 D-GN/WH | 423 | Ignition Coil (IC) Timing Control (2 and 3)

### Ignition Coil (IC) Module (LDA)

#### Connector Part Information

- OEM: PED 12059595
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Ignition Coil (IC) Module (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | 406 | Ignition Coil (IC) Timing Control (1 and 4)
B | PK | 739 | Ignition 1 Voltage
C | D-GN/WH | 423 | Ignition Coil (IC) Timing Control (2 and 3)

### Ignition Coil (IC) Module (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12059595
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Ignition Coil (IC) Module (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 406 | Ignition Coil Control (1 and 4)
B | 0.5 PK/BK | 739 | Ignition 1 Voltage
C | 0.5 D-GN/WH | 423 | Ignition Coil Control (2 and 3)

### Ignition Coil (IC) Module (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12059595
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Ignition Coil (IC) Module (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 406 | Ignition Coil (IC) Timing Control (1 and 4)
B | 0.5 PK | 739 | Ignition 1 Voltage
C | 0.5 D-GN/WH | 423 | Ignition Coil (IC) Timing Control (2 and 3)

### Ignition Coil Module (1 and 4) (L95, LXT)

#### Connector Part Information

- OEM: KET MG 641789-4
- Description: 2-Way F 090-II WP Series

#### Ignition Coil Module (1 and 4) (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.85 OG | 406 | Ignition Coil Control (1 and 4)
2 | 0.85 PK | 739 | Ignition 1 Voltage

### Ignition Coil Module (2 and 3) (L95, LXT)

#### Connector Part Information

- OEM: KET MG 641637-5
- Description: 2-Way F 090-II WP Series (BK)

#### Ignition Coil Module (2 and 3) (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.85 WH | 423 | Ignition Coil Control (2 and 3)
2 | 0.85 PK | 739 | Ignition 1 Voltage

### Ignition Lock Cylinder Control Actuator (North America)

#### Connector Part Information

- OEM: KET MG 610392
- Description: 2-Way F SDL Series (WH)

#### Ignition Lock Cylinder Control Actuator (North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE | 1075 | Ignition Lock Cylinder Actuator Control
0.5 OG (North America)
2 | 0.5 YE | 43 | Accessory Voltage
0.5 D-GN/WH (North America)

### Ignition Key Alarm Switch

#### Connector Part Information

- OEM: KET MG 610070
- Description: 2-Way 090 (2.3 mm) Series (WH)

#### Ignition Key Alarm Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 640 | Battery Positive Voltage
OG | 640 | Battery Positive Voltage
2 | L-GN | 80 | Key In Ignition Switch Signal
L-GN | 80 | Key In Ignition Switch Signal

### Ignition Key Alarm Switch

#### Connector Part Information

- OEM: KET MG 610070
- Description: 2-Way 090 (2.3 mm) Series (WH)

#### Ignition Key Alarm Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 640 | Battery Positive Voltage
OG | 640 | Battery Positive Voltage
2 | L-GN | 80 | Key In Ignition Switch Signal
L-GN | 80 | Key In Ignition Switch Signal

### Ignition Key Cylinder Lamp

#### Connector Part Information

- OEM: KET MG 610207
- Description: 2-Way F 118 (PA) Series (WH)

#### Ignition Key Cylinder Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 640 | Battery Positive Voltage
2 | D-GN/WH | 900 | Key Cylinder Lamp Control

### Ignition Switch

#### Connector Part Information

- OEM: KET MG 650887
- Description: 6-Way F 250 III Series (WH)

#### Ignition Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 300 | Ignition 3 Voltage
2 | RD | 642 | Battery Positive Voltage
3 | D-BU | 5 | Crank Voltage
4 | PK | 3 | Ignition 1 Voltage
5 | RD | 1642 | Battery Positive Voltage
6 | BN | 4 | Accessory Voltage

### Immobilizer

#### Connector Part Information

- OEM: MOLEX 35508-0700
- Description: 7-Way F Wire-to-Board Housing

#### Immobilizer

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK | 639 | Ignition 1 Voltage
2 | 0.5 OG | 240 | Battery Positive Voltage
3 | -- | -- | Not Used
4 | 0.5 BK | 1050 | Ground
5 | 0.5 PU | 2000 | Serial Data
6 | 0.5 PU | 800 | Serial Data
7 | 0.5 YE | 749 | Theft Deterrent Control Unit Signal

### Inflatable Restraint Front End Discriminating Sensor

#### Connector Part Information

- OEM: YAZAKI 7283-6507-70
- Description: 2-Way F Connector (YE)

#### Inflatable Restraint Front End Discriminating Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN/RD | 2106 | Front End Sensor - Left Signal
0.5 D-GN/WH | 2104 | Front End Sensor - Right Signal
2 | 0.5 BN/BK | 2105 | Front End Sensor - Left Voltage
0.5 PU | 2103 | Front End Sensor - Right Signal

### Inflatable Restraint Front Passenger Presence Sensor

#### Connector Part Information

- OEM: AMP 1-0967640-1
- Description: 4-Way F Connector (BK)

#### Inflatable Restraint Front Passenger Presence Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK | 939 | Ignition 1 Voltage
2 | 0.5 YE/WH | 1415 | Communication
3 | 0.5 BK | 252 | Ground
BK/WH (North America)
4 | -- | -- | Not Used

### Inflatable Restraint I/P Module (Single Stage) (L95, LXT, LDA, L79)

#### Connector Part Information

- OEM: FCI60201704
- Description: 2-Way Connector (YE)

#### Inflatable Restraint I/P Module (Single Stage) (L95, LXT, LDA, L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK/D-BU | 1403 | I/P Module - High Control (LHD)
0.5WH/BK | I/P Module - High Control (RHD)
2 | 0.5 OG/D-BU | 1404 | I/P Module - Low Control (LHD)
0.5 D-GN/WH | I/P Module - Low Control (RHD)

### Inflatable Restraint I/P Module (Dual Stage) (L34)

#### Connector Part Information

- OEM: FCI54550400
- Description: 4-Way F Connector (YE)

#### Inflatable Restraint I/P Module (Dual Stage) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG/D-BU | 1404 | IP Module - Low Control
2 | 0.5 BK/D-BU | 1403 | IP Module - High Control
3 | 0.5 D-GN/D-BU | 1411 | IP - Stage 2 - High Control
4 | 0.5 BK/D-GN | 1412 | IP Module - Stage 2 - Low Control

### Inflatable Restraint Sensing and Diagnostic Module (SDM) (Except North America)

#### Connector Part Information

- OEM: AMP 368233-1
- Description: 50-Way Air Bag 50P Plug Ass'y (BK)

#### Inflatable Restraint Sensing and Diagnostic Module (SDM) (Except North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 1186 | Seat Belt Pretensioner - Passenger High Control
2 | 0.5 D-BU/WH | 1187 | Seat Belt Pretensioner - Passenger Low Control
3 | 0.5 PK | 1184 | Seat Belt Pretensioner - Driver Low Control
4 | 0.5 D-BU | 1185 | Seat Belt Pretensioner - Driver High Control
5 | 0.5 YE | 1139 | Ignition 1 Voltage
6 | 0.5 BK/WH | 251 | Ground
7 | 0.5 D-GN | 358 | Air Bag Indicator Control
8 | -- | -- | Not Used
9 | 0.5 L-BU | 327 | Serial Data
10 | 0.5 BN | 347 | Steering Wheel Module - Low Control
11 | 0.5 BU | 348 | Steering Wheel Module - Low Control
12 | 0.5 BN/WH | 238 | Seat Belt Switch - Left
13 | 0.5 BK/D-BU | 1403 | I/P Module - High Control (LHD)
0.5 WH/BK | I/P Module - High Control (RHD)
14 | 0.5 OG/D-BU | 1404 | I/P Module - Low Control (LHD)
0.5 D-GN/WH | I/P Module - Low Control (RHD)
15 | -- | -- | Not Used
16 | 0.5 WH/YE | 1180 | Side Impact Module - Right - Low Control
17 | 0.5 D-GN/YE | 1181 | Side Impact Module - Right - High Control
18 | 0.5 D-GN/D-BU | 1183 | Side Impact Module - Driver High Control
19 | 0.5 WH/D-BU | 1182 | Side Impact Module - Driver Low Control
20 | 0.5 RD/YE | 753 | Side Impact Sensor - Driver - Voltage (LHD)
0.5 PK/WH | 714 | Side Impact Sensor - Passenger Voltage (RHD)
21 | 0.5 PK/WH | 714 | Side Impact Sensor - Passenger Voltage (LHD)
0.5 RD/YE | 753 | Side Impact Sensor - Driver Voltage (RHD)
22-44 | -- | -- | Not Used
45 | 0.5 BK | 754 | Side Impact Sensor - Driver Signal (LHD)
BN/WH | 715 | Side Impact Sensor - Passenger Signal (RHD)
46 | 0.5 BN/WH | 715 | Side Impact Sensor - Passenger Signal (LHD)
BK | 754 | Side Impact Sensor - Driver Signal (RHD)
47-50 | -- | -- | Not Used

### Inflatable Restraint Sensing and Diagnostic Module (SDM) (North America)

#### Connector Part Information

- OEM: AMP 0-1393359-2
- Description: 75-Way F Connector (OG)

#### Inflatable Restraint Sensing and Diagnostic Module (SDM) (North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2-25 | -- | -- | Not Used (Shorting Bar)
26 | 0.5 YE | 1139 | Ignition 1 Voltage
27 | 0.5 D-GN | 358 | Air Bag Indicator Control
28 | 0.5 BK/WH | 251 | Ground
29 | 0.5 D-BU | 348 | Steering Wheel Module - Low Control
30 | 0.5 BN | 347 | Steering Wheel Module - High Control
31 | 0.5 BK/D-BU | 1403 | I/P Module - High Control
32 | 0.5 OG/D-BU | 1404 | I/P Module - Low Control
33 | 0.5 D-BU | 1185 | Seat Belt Pretensioner - Driver - High Control
34 | 0.5 PK | 1184 | Seat Belt Pretensioner - Driver - Low Control
35 | 0.5 PK/BK | 1186 | Seat Belt Pretensioner - Passenger - High Control
36 | 0.5 D-BU/WH | 1187 | Seat Belt Pretensioner - Passenger - Low Control
37 | 0.5 D-BU/WH | 1182 | Side Impact Module - Driver High Control
38 | 0.5 D-GN/D-BU | 1183 | Side Impact Module - Driver Low Control
39 | 0.5 D-GN/YE | 1181 | Side Impact Module - Passenger Low Control
40 | 0.5 WH/YE | 1180 | Side Impact Module - Passenger High Control
41 | 0.5 YE | 1409 | Steering Wheel Module - High Control
42 | 0.5 YE/BK | 1410 | Steering Wheel Module - High Control
43 | 0.5 D-GN/D-BU | 1411 | IP Module - Stage 2 - High Control
44 | 0.5 BK/D-GN | 1412 | IP Module - Stage 2 - Low Control
45-53 | -- | -- | Not Used
54 | 0.5 L-BU | 327 | Serial Data
55 | -- | -- | Not Used
56 | 0.5 D-GN/WH | 1358 | Driver Information Center (DIC) Switch Signal
57-60 | -- | -- | Not Used
61 | 0.5 BN/WH | 238 | Seat Belt Switch - Left
62-63 | -- | -- | Not Used
64 | 0.5 YE/WH | 1415 | Communication
65-67 | -- | -- | Not Used
68 | 0.5 BN/WH | 715 | Side Impact Sensor - Passenger Signal
69 | 0.5 PK/WH | 714 | Side Impact Sensor - Passenger Voltage
70 | 0.5 RD/YE | 753 | Side Impact Sensor - Driver Voltage
71 | 0.5 BK | 754 | Side Impact Sensor - Driver Signal
72 | 0.5 D-GN/WH | 2104 | Discriminating Sensor - Right - Signal
73 | 0.5 PU | 2103 | Discriminating Sensor - Right - Signal
74 | 0.5 BN/BK | 2105 | Discriminating Sensor - Left - Signal
75 | 0.5 L-GN/RD | 2106 | Discriminating Sensor - Left - Signal

### Inflatable Restraint Side Impact Module (AJ7)

#### Connector Part Information

- OEM: Yazaki 7C83-5524-70
- Description: 2-Way Connector (YE)

#### Inflatable Restraint Side Impact Module (AJ7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 WH/D-BU | 1182 | Side Impact Module - Driver Low Control
WH/YE | 1180 | Side Impact Module - Passenger Low Control
2 | D-GN/D-BU | 1183 | Side Impact Module - Driver High Control
0.5 D-GN/YE | 1181 | Side Impact Module - Passenger High Control

### Inflatable Restraint Side Impact Sensor (AJ7)

#### Connector Part Information

- OEM: V23540-M5602-Y120
- Description: 2-Way

#### Inflatable Restraint Side Impact Sensor (AJ7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK/WH | 754 | Side Impact Sensor - Driver Signal
BN/WH | 715 | Side Impact Sensor - Passenger Signal
2 | 0.5 PK | 753 | Side Impact Sensor - Driver Voltage
0.5 PK/WH | 714 | Side Impact Sensor - Passenger Voltage

### Inflatable Restraint Steering Wheel Module (Single Stage) (L95, LXT, LDA, L79)

#### Connector Part Information

- OEM: PED 12162794
- Description: 2-Way M Metri-Pack 280 Series, Unsealed (YE)

#### Inflatable Restraint Steering Wheel Module (Single Stage) (L95, LXT, LDA, L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 348 | Steering Wheel Module - Low Control
2 | BN | 347 | Steering Wheel Module - High Control

### Inflatable Restraint Steering Wheel Module (Dual Stage) (L34)

#### Connector Part Information

- OEM: FC I54550400
- Description: 4-Way Connector (YE)

#### Inflatable Restraint Steering Wheel Module (Dual Stage) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BK | 1410 | Trailer ABS Failure Indicator Control
2 | YE | 1409 | Discriminating Sensor - Right Signal
3 | BN | 347 | Steering Wheel Module - High Control
4 | D-BU | 348 | Steering Wheel Module - Low Control

### Inflatable Restraint Steering Wheel Module C1 (North America)

#### Connector Part Information

- OEM: 54550267
- Description: 2-Way F ABX-3 Code B (WH)

#### Inflatable Restraint Steering Wheel Module C1 (North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | 347 | Steering Wheel Module - High Control
B | D-GN/WH | 348 | Steering Wheel Module - Low Control

### Inflatable Restraint Steering Wheel Module C2 (North America)

#### Connector Part Information

- OEM: 54550271
- Description: 2-Way F ABX-3 Code G (BK)

#### Inflatable Restraint Steering Wheel Module C2 (North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU/RD | 1410 | Steering Wheel Module - High Control
B | BK/WH | 1409 | Steering Wheel Module - Low Control

### Inflatable Restraint Steering Wheel Module Coil

#### Connector Part Information

- OEM: KET MG 641032
- Description: 3-Way

#### Inflatable Restraint Steering Wheel Module Coil

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 1796 | Radio Control Steering Column Signal
2 | BK/WH | 372 | Remote Radio Return Audio
3 | BK | 28 | Horn Relay Control

### Inflatable Restraint Steering Wheel Module Coil - C1 (Single Stage) (L95, LXT, LDA, L79)

#### Connector Part Information

- OEM: PED 12162794
- Description: 2-Way M Metri-Pack 280 Series, Unsealed (YE)

#### Inflatable Restraint Steering Wheel Module Coil - C1 (Single Stage) (L95, LXT, LDA, L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 348 | Steering Wheel Module - Low Control
2 | BN | 347 | Steering Wheel Module - High Control

### Inflatable Restraint Steering Wheel Module Coil - C1 (Dual Stage) (L34)

#### Connector Part Information

- OEM: FC 154550400
- Description: 4-Way F Connector (YE)

#### Inflatable Restraint Steering Wheel Module Coil - C1 (Dual Stage) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BK | 1410 | Steering Wheel Module - High Control
2 | YE | 1409 | Steering Wheel Module - High Control
3 | BN | 347 | Steering Wheel Module - High Control
4 | D-BU | 348 | Steering Wheel Module - Low Control

### Inflatable Restraint Steering Wheel Module Coil - C2 (w/Cruise)

#### Connector Part Information

- OEM: KET MG 651050
- Description: 8-Way F 090-II Series (WH)

#### Inflatable Restraint Steering Wheel Module Coil - C2 (w/Cruise)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 1796 | Radio Control - Steering Column Signal
2 | BK/WH | 372 | Remote Radio Return - Audio
3 | BK | 28 | Horn Relay Control
4 | GY | 397 | Cruise Control Switch Signal
5 | GY/BK | 87 | Cruise Control Release Signal
6 | D-BU | 84 | Cruise Control SET/Coast Switch Signal
7 | OG | 1540 | Battery Positive Voltage
8 | -- | -- | Not Used

### Inflatable Restraint Steering Wheel Module Coil - C2 (w/o Cruise)

#### Connector Part Information

- OEM: KET MG 641032
- Description: 3-Way F

#### Inflatable Restraint Steering Wheel Module Coil - C2 (w/o Cruise)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 1796 | Radio Control - Steering Column Signal
2 | BK/WH | 372 | Remote Radio Return - Audio
3 | BK | 28 | Horn Relay Control

### Input Shaft Speed (ISS) Sensor (MLQ)

#### Connector Part Information

- OEM: YAZAKI 7283-8125-90
- Description: 2-Way F Connector (GN)

#### Input Shaft Speed (ISS) Sensor (MLQ)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE/BK | 1297 | Input Shaft Speed Sensor Low Signal
2 | 0.5 D-BU/WH | 1296 | Input Shaft Speed Sensor High Signal

### Input Speed Sensor (M98)

#### Connector Part Information

- OEM: YZK 7283-8125-30
- Description: 2-Way F 090II Type Sealed

#### Input Speed Sensor (M98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BU/WH | -- | Input Shaft Speed Sensor Low
2 | YE/BK | -- | Input Shaft Speed Sensor High

### Inside Air Temperature (C68)

#### Connector Part Information

- OEM: KET MG 620074
- Description: 2-Way M 090 Connector (2.3 mm)

#### Inside Air Temperature (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.3 D-GN | 1910 | Inside Air Temperature Sensor Signal
2 | 0.5 YE | 61 | Low Reference

### Instrument Cluster X1

#### Connector Part Information

- OEM: KET MG 651563
- Description: 23-Way F PCB 050 Series (WH)

#### Instrument Cluster X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PU/WH | 33 | Brake Warning Indicator Control
2 | 0.5 BN | 25 | Charge Indicator Control/Charge Indicator Signal
3 | 0.5 YE | 1481 | Hold Mode Indicator Control
4 | 0.5 BN | 956 | Speed Sensitive Power Steering (SSPS) Warning Lamp Control
5 | 0.5 D-BU | 744 | Trunk Open Signal (Optional)
6 | -- | -- | Not Used
7 | 0.3 PU/WH | 821 | Engine Overspeed Indicator Control
8-9 | -- | -- | Not Used
10 | 0.5 BK | 250 | Ground
11 | 0.3 BK/WH | 238 | Seat Belt Switch - Left
12 | 0.5 WH | 156 | Courtesy Lamp Control
13 | 0.3 L-GN | 867 | ABS Indicator Failure Control
14 | 0.5 WH | 905 | Traction Control Warning
15 | 0.5 BN/WH | 1084 | Tire Pressure Monitoring System
16 | 0.5 L-BU | -- | Glow Plug Indicator (Diesel)
-- | -- | Not Used (Gasoline)
17 | 0.5 L-BU | 14 | Left Turn Signal Lamps Supply Voltage
18 | 0.3 OG | 640 | Battery Positive Voltage
19 | 0.5 PK | 239 | Ignition 1 Voltage
20 | -- | -- | Not Used (Gasoline)
L-BU | -- | Change Oil Soon Indicator (Diesel)
21 | -- | -- | Not Used (Gasoline)
0.5 PU | -- | Fuel Warning Signal (Diesel)
22 | 0.3 BN/WH | 309 | Right Park Lamp Supply Voltage
23 | 0.3 D-GN | 44 | Instrument Panel Lamps Dimmer Switch Signal

### Instrument Cluster X2

#### Connector Part Information

- OEM: KET MG 610363
- Description: 20-Way F PCB 040 Series (WH)

#### Instrument Cluster X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 250 | Ground
2 | 0.3 D-GN | 135 | Engine Coolant Temperature (ECT) Sensor Gage Signal
0.3 L-GN/BK | 135 | Engine Coolant Temperature (ECT) Sensor Gage Signal (Diesel)
3 | 0.5 WH | 30 | Fuel Level Sensor Signal
0.5 PU/BK | 632 | Low Reference (Diesel)
4 | 0.5 GY | 121 | Engine Speed Signal
5 | 0.5 D-GN/WH | 817 | Vehicle Speed Sensor (VSS) Signal
6 | 0.5 BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control
7 | 0.5 BN | 358 | Air Bag Indicator Control
8 | 0.5 PU/WH (2.0L) | 231 | Oil Pressure Indicator Control
0.5 PU/BK
9 | 0.5 L-GN | 11 | Headlamp High Beam Supply Voltage
10 | 0.5 WH | 85 | Cruise Control Engage Signal (w/Cruise Control)
11 | 0.5 D-BU | 15 | Right Turn Signal Lamps Supply Voltage
12 | -- | -- | Not Used (Gasoline)
0.5 BU | 1936 | Low Fuel Signal (Diesel)
13 | -- | -- | Not Used (Gasoline)
0.5 YE/BK | 3070 | Diesel Particulate Filter Indicator (Diesel)
14 | 0.5 PU | 172 | Low Fuel Indicator Control
15 | 0.5 PK | 239 | Ignition 1 Voltage (Gasoline)
0.5 GY/BK | 3067 | Coolant Temperature Indicator (Diesel)
16 | -- | -- | Not Used (Gasoline)
0.5 BN/WH | 3058 | Water In Fuel Indicator (Diesel)
17 | 0.5 BN | 27 | Hazard Flasher Signal (Optional)
18 | 0.5 WH | 629 | DRL Indicator Control (w/DRL)
19 | 0.5 YE | 317 | Fog Lamp Relay Coil Supply Voltage
20 | 0.5 RD | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps)

### Instrument Cluster X3

#### Connector Part Information

- OEM: KET MG 610896
- Description: 8-Way F PCB Connector SDL-II PCB Hsg (WH)

#### Instrument Cluster X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.5 D-BU/RD | 3010 | Park/Neutral Position (PNP) Switch L1 Signal
4 | 0.5 GY | 2380 | Park/Neutral Position (PNP) Switch Low Gear Signal
-- | -- | Not Used (North America)
5 | 0.5 D-GN | 2384 | Park/Neutral Position (PNP) Switch 2nd Gear Signal
-- | -- | Not Used (North America)
6 | 0.5 L-GN/BK | 3013 | Park/Neutral Position (PNP) Switch L4 Signal
7 | 0.5 L-GN/RD | 3012 | Park/Neutral Position (PNP) Switch L3 Signal
8 | 0.5 L-GN/RD | 3011 | Park/Neutral Position (PNP) Switch L2 Signal

### Intake Air Temperature (IAT) Sensor (L95, LXT)

#### Connector Part Information

- OEM: AMP 85202-1
- Description: 2-Way F JR Power Timer 2P Hsg Ass'y (BK)

#### Intake Air Temperature (IAT) Sensor (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 472 | Intake Air Temperature (IAT) Sensor Signal
2 | 0.5 OG/BK | 469 | Low Reference

### Intake Air Temperature (IAT) Sensor (L79)

#### Connector Part Information

- OEM: AMP 85202-1
- Description: 2-Way JR Power Timer 2P Hsg Ass'y (BK)

#### Intake Air Temperature (IAT) Sensor (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK/YE | 808 | Low Reference
2 | 0.5 BN | 472 | Intake Air Temperature (IAT) Sensor Signal

### Intake Air Temperature (IAT) Sensor (LDA)

#### Connector Part Information

- OEM: AMP 85202-1
- Description: 2-Way JR Power Timer 2P Hsg Ass'y (BK)

#### Intake Air Temperature (IAT) Sensor (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 808 | Low Reference
2 | 0.5 GY (BN) | 472 | Intake Air Temperature (IAT) Sensor Signal

### Intake Air Temperature (IAT) Sensor (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 85202-1
- Description: 2-Way JR Power Timer 2P Hsg Assembly (BK)

#### Intake Air Temperature (IAT) Sensor (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 808 | Low Reference
2 | 0.5 GY | 472 | Intake Air Temperature (IAT) Sensor Signal

### Intake Air Temperature (IAT) Sensor (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 85202-1
- Description: 2-Way JR Power Timer 2P Hsg Ass'y (BK)

#### Intake Air Temperature (IAT) Sensor (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 808 | Low Reference
2 | 0.5 GY (BN) | 472 | Intake Air Temperature (IAT) Sensor Signal

### Intake Manifold Tuning Valve (L95, LXT)

#### Connector Part Information

- OEM: AMP 174352-2
- Description: 2-Way M Econoseal J Mark II + Connector Plug Housing (BK)

#### Intake Manifold Tuning Valve (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 WH/BK | 962 | Intake Manifold Tuning Valve Solenoid Control
2 | 0.5 PK/BU | 539 | Ignition 1 Voltage

### Intake Manifold Tuning Valve Solenoid (L79)

#### Connector Part Information

- OEM: AMP 174352-2
- Description: 2-Way M Econoseal J Mark II + Connector Plug Housing (BK)

#### Intake Manifold Tuning Valve Solenoid (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH/BK | 962 | Intake Manifold Tuning Valve Solenoid Control
2 | PK/D-BU | 539 | Ignition 1 Voltage

### Intake Manifold Tuning Valve Solenoid (LDA)

#### Connector Part Information

- OEM: AMP 174352-2
- Description: 2-Way M Econoseal J Mark II + Connector Plug Housing (BK)

#### Intake Manifold Tuning Valve Solenoid (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH/BK | 962 | Intake Manifold Tuning Valve Solenoid Control
2 | 0.5 PK/D-BU | 539 | Ignition 1 Voltage

### Intake Manifold Tuning Valve Solenoid (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 174352-2
- Description: 2-Way M Econoseal J Mark II + Connector Plug Housing (BK)

#### Intake Manifold Tuning Valve Solenoid (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH/BK | 962 | Intake Manifold Tuning Valve Solenoid Control
2 | 0.5 PK/D-BU | 539 | Ignition 1 Voltage

### Key Interlock Module (Except North America)

#### Connector Part Information

- OEM: AK 36905
- Description: 9-Way F Relay (BK)

#### Key Interlock Module (Except North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | YE | 1075 | Park Neutral Position (PNP) Switch Signal
3 | -- | -- | Not Used
4 | BK | 250 | Ground
5 | D-GN | 286 | Shift Lock Control Solenoid Control
6 | L-GN | 275 | Park Neutral Position (PNP) Switch Signal
7 | OG/BK | 434 | Park Neutral Position (PNP) Switch Signal
8 | L-BU | 20 | Stop Lamp Switch Signal
9 | YE | 434 | Park Neutral Position (PNP) Switch Signal

### Key Interlock Module (North America)

#### Connector Part Information

- OEM: AK 36915
- Description: 9-Way F Relay (BK)

#### Key Interlock Module (North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 YE | 43 | Accessory Voltage
3 | -- | -- | Not Used
4 | 0.5 D-GN | 286 | Shift Lock Control solenoid Control
5 | 0.5 YE | 1075 | Ignition Lock Cylinder Actuator Control
6 | 0.5 BK | 250 | Ground
7 | 0.5 L-BU | 20 | Stop Lamp Switch Signal
8 | 0.5 L-GN | 275 | Park Neutral Position (PNP) Switch Signal
9 | -- | -- | Not Used

### Knock Sensor (KS) (L95, LXT)

#### Connector Part Information

- OEM: AMP 368215-1
- Description: 3-Way F JPT 3P Ass'y for Knock Sensor (GY)

#### Knock Sensor (KS) (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE/BK | 496 | Knock Sensor (KS) Signal
2 | 0.5 D-BU/WH | 1876 | Low Reference
3 | 0.5 BK/WH | 51 | Ground

### Knock Sensor (KS) (L79)

#### Connector Part Information

- OEM: AMP 368215-1
- Description: 3-Way JPT 3P Ass'y for Knock Sensor

#### Knock Sensor (KS) (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE/BK | 496 | Knock Sensor (KS) Signal
2 | 0.5 D-BU/WH | 808 | Low Reference
3 | 0.5 BK/WH | 51 | Ground

### Knock Sensor (KS) (LDA)

#### Connector Part Information

- OEM: AMP 368215-1
- Description: 3-Way JPT 3P Ass'y for Knock Sensor

#### Knock Sensor (KS) (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE/BK | 496 | Knock Sensor (KS) Signal
2 | 0.5 D-BU/WH | 808 | Low Reference
3 | 0.5 BK/WH | 51 | Ground

### Knock Sensor (KS) (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 368215-1
- Description: 3-Way F JPT 3P Assembly for Knock Sensor (GY)

#### Knock Sensor (KS) (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE/BK | 496 | Knock Sensor (KS) Signal
2 | 0.5 D-BU/WH | 808 | Low Reference

### Knock Sensor (KS) (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 368215-1
- Description: 3-Way JPT 3P Ass'y for Knock Sensor

#### Knock Sensor (KS) (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE/BK | 496 | Knock Sensor (KS) Signal
2 | 0.5 D-BU/WH | 808 | Low Reference
3 | 0.5 BK/WH | 51 | Ground

### Lamp Control Module

#### Connector Part Information

- OEM: KET MG 651050
- Description: 8-Way F 090-II Series (WH)

#### Lamp Control Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | WH | 1080 | Park Lamp Relay Control
3 | WH | 1080 | Park Lamp Relay Control
4 | OG | 1540 | Battery Positive Voltage
5 | BK | 1050 | Ground
6 | PU | 126 | Left Front Door Open Switch Signal
7 | L-GN | 80 | Key in Ignition Switch Signal
8 | -- | -- | Not Used

### Lamp Driver Module

#### Connector Part Information

- OEM: AK 36636
- Description: 6-Way M

#### Lamp Driver Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU/WH | 33 | Park Brake Indicator Control
B | BN | 739 | Ignition 1 Voltage
C | L-GN/BK | 867 | ABS Warning Lamp
D | BK | 1150 | Ground
E | GY | 875 | ABS Indicator Control
F | GY/BK | 2147 | Brake Oil Pressure Switch

### License Plate Lamp - Left

#### Connector Part Information

- OEM: 12110053
- Description: 2-Way F Lamp Socket Wedge Base W2 (L-GY)

#### License Plate Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BK (North America) | 709 | Left Park Lamp Supply Voltage
PU
B | WH (North America) | 550 | Ground
BK | 1250 | Ground

### License Plate Lamp - Right

#### Connector Part Information

- OEM: 12110053
- Description: 2-Way F Lamp Socket Wedge Base W2 (L-GY)

#### License Plate Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BK (North America) | 709 | Left Park Lamp Supply Voltage
PU
B | WH (North America) | 550 | Ground
BK | 1250 | Ground

### Manifold Absolute Pressure (MAP) Sensor (L95, LXT)

#### Connector Part Information

- OEM: PED 12129946
- Description: 3-Way F Metri-Pack 150 Series Sealed (GY)

#### Manifold Absolute Pressure (MAP) Sensor (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG/BK | 469 | Low Reference
B | 0.5 L-GN | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
C | 0.5 L-BU/BK | 1688 | 5-Volt Reference

### Manifold Absolute Pressure (MAP) Sensor (L79)

#### Connector Part Information

- OEM: 12059595
- Description: 3-Way F Metri-Pack 150 Series, Sealed (BK)

#### Manifold Absolute Pressure (MAP) Sensor (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG/BK | 469 | Low Reference
B | 0.5 L-GN | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
C | 0.5 L-BU/BK | 1688 | 5-Volt Reference

### Manifold Absolute Pressure (MAP) Sensor (LDA)

#### Connector Part Information

- OEM: AMP 174359-2
- Description: 3-Way F 070 Series Econoseal Mark-2 Cap 3P (BK)

#### Manifold Absolute Pressure (MAP) Sensor (LDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU/BK | 1688 | 5-Volt Reference
2 | 0.5 D-BU/WH (L-GN) | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
3 | 0.5 OG/BK | 469 | Low Reference

### Manifold Absolute Pressure (MAP) Sensor (w/Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: PED 12059595
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Manifold Absolute Pressure (MAP) Sensor (w/Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU/BK | 1688 | 5-Volt Reference
2 | 0.5 D-BU/WH | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
3 | 0.5 OG/BK | 469 | Low Reference

### Manifold Absolute Pressure (MAP) Sensor (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

- OEM: AMP 174359-2
- Description: 3-Way F 070 Series Econoseal Mark-2 Cap 3P (BK)

#### Manifold Absolute Pressure (MAP) Sensor (w/o Throttle Actuator Control) (L34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU/BK | 1688 | 5-Volt Reference
2 | 0.5 D-BU/WH (L-GN) | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
3 | 0.5 OG/BK | 469 | Low Reference

### Mass Air Flow (MAF) Sensor (LMN)

#### Connector Part Information

- OEM: BOSCH 1928403736
- Description: 4-Way F Sealed

#### Mass Air Flow (MAF) Sensor (LMN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | -- | Ignition 1 Voltage
2 | YE/BK | -- | Ground
3 | BU/WH | -- | IAT Signal
4 | PU/WH | -- | MAF Signal

### Mode Actuator (C68)

#### Connector Part Information

- OEM: KET MG 610203
- Description: 7-Way F 118 (PA) Series (BK)

#### Mode Actuator (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.3 YE/BU | 1397 | Lower Mode Valve Solenoid Control
2 | 0.3 PK | 1396 | Defrost Mode Valve Solenoid Control
3 | 0.3 D-GN/BK | 1395 | Upper Mode Valve Solenoid Control
4 | 0.85 BN | 41 | Ignition 2 Voltage
5 | 0.3 BK | 350 | Ground
6 | 0.3 PK/BK | 1399 | Mode Valve Signal
7 | WH/BK | 1398 | Mode Valve Signal

### Multifunction Alarm Module

#### Connector Part Information

- OEM: KET MG 610896
- Description: 8-Way F PCB Connector SDL-II PCB Hsg (WH)

#### Multifunction Alarm Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK/WH | 238 | Seat Belt Switch Signal - Left
2 | L-GN | 80 | Key In Ignition Switch Signal
3 | PU/WH | 821 | Engine Overspeed Indicator Control
4 | PU | 126 | Left Front Door Open Switch Signal
5 | BK | 1050 | Ground
6 | RD | 709 | Left Park Lamp Supply Voltage
7 | -- | -- | Not Used
8 | PK | 239 | Ignition 1 Voltage

### Octane Selection Switch (L95, LXT)

#### Connector Part Information

- OEM: KET MG 640329
- Description: 3-Way M SWP Series (BK)

#### Octane Selection Switch (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PU | 773 | Octane Switch Signal
2 | 0.5 BK/WH | 251 | Ground
3 | 0.5 L-BU | 772 | Octane Switch Signal

### Octane Selection Switch (L79)

#### Connector Part Information

- OEM: KET MG 640329
- Description: 3-Way M SWP Series

#### Octane Selection Switch (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PU | 723 | Octane Switch Signal
2 | 0.5 BK/WH | 51 | Ground
3 | 0.5 L-BU | 722 | Octane Switch Signal

### Oil Feeding Connector

#### Connector Part Information

- OEM: KET MG 640333
- Description: 4-Way M SWP Series (BK)

#### Oil Feeding Connector

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK/WH | 2051 | Ground
2 | 0.5 BN | 739 | Ignition 1 Voltage
3 | 0.5 D-BU | 774 | Serial Data
4 | 0.5 RD | 42 | Battery Positive Voltage

### Oil Pressure Switch

#### Connector Part Information

- OEM: ZPF1-2
- Description: 1-Way F Metri-Pack 150 Series Sealed (BK)

#### Oil Pressure Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/BK | 231 | Oil Pressure Switch Signal

### Output Speed Sensor (M98)

#### Connector Part Information

- OEM: YZK 7283-8125-30
- Description: 2-Way F 090II Type Sealed

#### Output Speed Sensor (M98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BK | -- | Input Shaft Speed Sensor Low
2 | BU/WH | -- | Input Shaft Speed Sensor High

### Outside Rearview Mirror Driver

#### Connector Part Information

- OEM: AMP 173850
- Description: 8-Way F 070 Series Multilock Plug 8P (NA)

#### Outside Rearview Mirror Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/WH | 2230 | Folding Mirror Motor Retract Control (Optional)
2 | 0.5 L-GN/BK | 2231 | Folding Mirror Motor Extend Control (Optional)
3 | 0.3 OG/WH | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage (Optional)
4 | 0.5 GY | 90 | Passenger Mirror Motor Left Control
5 | -- | -- | Not Used
6 | 0.5 WH | 81 | Driver Mirror Motor Right Control
7 | 0.5 L-GN | 89 | Driver Mirror Motor Up Control
8 | 0.5 BK | 1150 | Ground

### Outside Rearview Mirror Folding Module (Optional)

#### Connector Part Information

- OEM: KET MG 610896
- Description: 8-Way F PCB Connector SDL-II PCB Hsg (WH)

#### Outside Rearview Mirror Folding Module (Optional)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY/RD | 2232 | Folding Mirror Switch Signal
2 | -- | -- | Not Used
3 | 0.5 OG | 640 | Battery Positive Voltage
4 | 0.5 BN | 641 | Ignition 2 Voltage
5 | 0.5 BK | 350 | Ground
6 | -- | -- | Not Used
7 | 0.5 L-GN/BK | 2231 | Folding Mirror Motor Extend Control
8 | 0.5 BN/WH | 2230 | Folding Mirror Motor Retract Control

### Outside Rearview Mirror Passenger

#### Connector Part Information

- OEM: AMP 173850-1
- Description: 8-Way F 070 Series Multilock Plug 8P (WH)

#### Outside Rearview Mirror Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN/BK | 2231 | Folding Mirror Motor Extend Control (Optional)
2 | 0.5 BN/WH | 2230 | Folding Mirror Motor Retract Control (Optional)
3 | 0.3 OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage (Optional)
4 | 0.5 GY/BK | 90 | Passenger Mirror Motor Left Control
5 | -- | -- | Not Used
6 | 0.5 RD/WH | 881 | Passenger Mirror Motor Right Control
7 | 0.5 PU/WH | 889 | Passenger Mirror Motor Down Control
8 | 0.5 BK | 350 | Ground

### Outside Rearview Mirror Switch

#### Connector Part Information

- OEM: AMP 173850
- Description: 8-Way M 070 Series Multilock Plug 8P (BK)

#### Outside Rearview Mirror Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | 89 | Driver Mirror Motor Up Control
2 | GY/BK | 2232 | Folding Mirror Switch (Optional)
3 | PU/WH | 889 | Passenger Mirror Motor Down Control
4 | GY | 90 | Passenger Mirror Motor Left Control
5 | WH | 81 | Driver Mirror Motor Right Control
6 | BK | 1150 | Ground
7 | RD/WH | 881 | Passenger Mirror Motor Right Control
8 | BN | 141 | Ignition 3 Voltage

### Oxygen (O2) Sensor (L95, LXT)

#### Connector Part Information

- OEM: AMP 174352-2
- Description: 2-Way M Econoseal J Mark II + Connector Plug Housing (BK)

#### Oxygen (O2) Sensor (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PU/WH | 1665 | Oxygen (O2) Sensor Signal
2 | 0.5 OG/BK | 469 | Low Reference

### Oxygen (O2) Sensor (L79)

#### Connector Part Information

- OEM: PED 12010501
- Description: 2-Way F Weather Pack Tower, Sealed (BK)

#### Oxygen (O2) Sensor (L79)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 GY | 1653 | Oxygen (O2) Sensor Signal
B | 0.5 D-GN/RD | 1665 | Oxygen (O2) Sensor Low Reference

### Park Neutral Position (PNP) Switch (MLQ)

#### Connector Part Information

- OEM: YAZAKI 7283-1296-40
- Description: 9-Way F

#### Park Neutral Position (PNP) Switch (MLQ)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 2382 | Park Neutral Position (PNP) Switch Park Signal
2 | 0.5 D-GN/WH | 2383 | Park Neutral Position (PNP) Switch Reverse Signal
3 | 0.5 PK | 839 | Ignition 1 Voltage
4 | 0.5 PK | 2384 | Park Neutral Position (PNP) Switch 2nd Gear Signal
5 | 0.5 YE | 2381 | Park Neutral Position (PNP) Switch Neutral Signal
6 | 1.25 BK/WH | 51 | Ground
7 | 0.5 WH | 2377 | Park Neutral Position (PNP) Switch Drive Signal
8 | 0.5 GY | 2380 | Park Neutral Position (PNP) Switch Low Signal
9 | 1.25 OG/BK | 434 | Automatic Transmission Shift Lock Control

### Park/Neutral Position Switch (M98)

#### Connector Part Information

- OEM: YZK 7223-6508-30
- Description: 10-Way F DMS+RV Sealed

#### Park/Neutral Position Switch (M98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | GN/WH | -- | Reverse Signal
3 | BK/WH | -- | Ground
4 | PK | -- | Park/Neutral Signal
5 | GN | -- | C Signal
6 | WH | -- | B Signal
7 | -- | -- | Not Used
8 | PK | -- | PA Signal
9 | PK | -- | Ignition 1 Voltage
10 | WH | -- | A Signal

### Park/Neutral Position (PNP) Switch (MFA)

#### Connector Part Information

- OEM: KET MG 641299
- Description: 10-Way F SSD & 0509 Connector (BK)

#### Park/Neutral Position (PNP) Switch (MFA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK | 439 | Ignition 1 Voltage
2 | 0.5 L-GN/RD | 3011 | Park/Neutral Position (PNP) L2 Signal
3 | 0.5 D-BU/RD | 3010 | Park/Neutral Position (PNP) L1 Signal
4 | 0.5 RD/D-BU | 3012 | Park/Neutral Position (PNP) L3 Signal
5 | 0.5 L-GN/BK | 3013 | Park/Neutral Position (PNP) L4 Signal
6 | -- | -- | Not Used
7 | 0.85 PK | 839 | Ignition 1 Voltage
8 | 0.85 L-GN | 24 | Backup Lamp Supply Voltage
9 | 0.5 OG/BK | 434 | Automatic Transmission Shift Lock Control
10 | 0.5 BK/WH | 251 | Ground

### Park/Turn Signal Lamp - Left Front (Except North America)

#### Connector Part Information

- OEM: KET MG 610327
- Description: 3-Way F SWP Series (GY)

#### Park/Turn Signal Lamp - Left Front (Except North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | 709 | Left Park Lamp Supply Voltage
2 | BK | 50 | Ground
3 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage

### Park/Turn Signal Lamp - Left Front (North America)

#### Connector Part Information

- OEM: KET MG 610327
- Description: 3-Way F SWP Series (BK)

#### Park/Turn Signal Lamp - Left Front (North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 50 | Ground
2 | PU | 709 | Left Park Lamp Supply Voltage
3 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage

### Park/Turn Signal Lamp - Right Front (Except North America)

#### Connector Part Information

- OEM: KET MG 610327
- Description: 3-Way F SWP Series (GY)

#### Park/Turn Signal Lamp - Right Front (Except North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | 309 | Right Park Lamp Supply Voltage
2 | BK | 150 | Ground
3 | L-BU | 15 | Right Turn Signal Lamps Supply Voltage

### Park/Turn Signal Lamp - Right Front (North America)

#### Connector Part Information

- OEM: KET MG 610327
- Description: 3-Way F SWP Series (BK)

#### Park/Turn Signal Lamp - Right Front (North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 150 | Ground
2 | BN/WH | 309 | Right Park Lamp Supply Voltage
3 | L-BU | 15 | Right Turn Signal Lamps Supply Voltage

### Parking Brake Switch

#### Connector Part Information

- OEM: F1-9
- Description: 1-Way F Connector (BK)

#### Parking Brake Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.3 PU/WH | 33 | Brake Warning Indicator Control

### Power Steering Control Module

#### Connector Part Information

OEM: AMP 173852-1
Description: 14-Way F 070 Series Multilock Plug 14P (WH)

#### Power Steering Control Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU | 1738 | Variable Effort Steering Actuator Supply Voltage
2 | 0.5 PU | 1703 | Variable Effort Steering Actuator Control
3 | 0.5 BK/WH | 451 | Steering Wheel Sensor Ground
4 | -- | -- | Not Used
5 | 0.5 GY | 1416 | Battery Positive Voltage
6 | 0.5 D-GN/WH | 817 | Vehicle Speed Sensor (VSS) Signal
7 | -- | -- | Not Used
8 | 0.3 PK | 239 | Ignition 1 Voltage
9 | 0.5 BN | 956 | Speed Sensitive Power Steering (SSPS) Warning Lamp Control
10 | 0.5 BK | 1050 | Ground
11-12 | -- | -- | Not Used
13 | 0.5 D-BU | 555 | Serial Data
14 | 0.5 L-BU | 1533 | Steering Wheel Sensor Signal

### PTC Heater (LMN)

#### Connector Part Information

OEM: PED15326878
Description: 3-Way F GT 280 Series Unsealed

#### PTC Heater (LMN)
Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | PTC Heater Supply Voltage
2 | YE/BK | -- | PTC Heater Supply Voltage
3 | BU/WH | -- | PTC Heater Supply Voltage

### Radio (w/RDS) A

#### Connector Part Information

OEM: ISO 16P REC (SMT-011114-04)
Description: 16-Way

#### Radio (w/RDS) A
Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU | 115 | Right Rear Speaker Output (-)
2 | 0.5 D-BU | 46 | Right Rear Speaker Output (+)
3 | 0.5 D-GN | 117 | Right Front Speaker Output (-)
4 | 0.5 L-GN | 200 | Right Front Speaker Output (+)
5 | 0.5 GY | 118 | Left Front Speaker Output (-)
6 | 0.5 PU | 201 | Left Front Speaker Output (+)
7 | 0.5 YE | 116 | Left Rear Speaker Output (-)
8 | 0.5 BN | 199 | Left Rear Speaker Output (+)
9 | 0.5 BN/WH | 309 | Right Park Lamp Supply Voltage
10-11 | -- | -- | Not Used
12 | 1.25 OG | 40 | Battery Positive Voltage
13 | 0.5 GY | 161 | Antenna Module Signal
14 | 0.3 D-GN | 44 | Instrument Panel Lamps Dimming Control
15 | 0.5 YE | 43 | Accessory Voltage
16 | 1.25 BK/WH | 151 | Ground

### Radio (w/RDS) B

#### Connector Part Information

OEM: ISO 6P REC (SMT-011114-03) ISO 6P REC (SMT-011114-01)
Description: 16-Way

#### Radio (w/RDS) B

Pin

Wire

Circuit

Function

1-10

--

--

Not Used

11

0.3 D-BU

1796

Radio Control - Steering Column Signal

12

0.3 BK/WH

372

Remote Radio Return - Audio

### Radio (w/o RDS)

#### Connector Part Information

OEM: AMP 173853
Description: 18-Way F 070 Series Multilock Plug 18P (WH)

#### Radio (w/o RDS)

Pin

Wire

Circuit

Function

1

0.5 L-GN

200

Right Front Speaker Output (+)

2

0.5 D-BU

46

Right Rear Speaker Output (+)

3

0.5 BN/WH

309

Right Park Lamp Supply Voltage

4

0.5 YE

43

Accessory Voltage

5

1.25 OG

40

Battery Positive Voltage

6

--

--

Not Used

7

0.5 BN

199

Left Rear Speaker Output (+)

8

0.5 PU

201

Left Front Speaker Output (+)

9

0.5 D-GN

117

Right Front Speaker Output (-)

10

0.5 L-BU

115

Right Rear Speaker Output (-)

11

0.5 D-GN

44

Instrument Panel Lamps Dimming Control

12

0.5 GY

161

Antenna Module Signal

13

0.5 BK/WH

372

Remote Radio Return - Audio

14

1.25 BK/WH

151

Ground

15

--

--

Not Used

16

0.3 D-BU

1796

Radio Control - Steering Column Signal

17

0.5 YE

116

Left Rear Speaker Output (-)

18

0.5 GY

118

Left Front Speaker Output (-)

### Radio Antenna Module (Hatchback)

#### Connector Part Information

OEM: KET MG 620040
Description: 1-Way M 250 Series (WH)

#### Radio Antenna Module (Hatchback)

Pin

Wire

Circuit

Function

1

0.5 GY

161

Antenna Enable Signal

### Radio Antenna Module (Notchback)

#### Connector Part Information

OEM: KET MG 612544
Description: 2-Way F (WH)

#### Radio Antenna Module (Notchback)

Pin

Wire

Circuit

Function

1

0.5 GY

161

Antenna Enable Signal

2

2 PU

293

Rear Defog Element Supply Voltage

### Reading Lamp (CF5)

#### Connector Part Information

OEM: KET MG 610402
Description: 8-Way F SDL Series (WH)

#### Reading Lamp (CF5)

Pin

Wire

Circuit

Function

1

BK

850

Ground

2

--

--

Not Used

3

OG

640

Battery Positive Voltage

4

D-GN/WH

133

Sunroof Limit Switch Low Reference

5

BN

641

Ignition 3 Voltage

6

PU

132

Sunroof Limit Switch Soft Stop Signal

7-8

--

--

Not Used

### Reading Lamps (w/o CF5)

#### Connector Part Information

OEM: KET MG 610392
Description: 2-Way F SDL Series (WH)

#### Reading Lamps (w/o CF5)

Pin

Wire

Circuit

Function

1

OG

640

Battery Positive Voltage

2

BK

850

Ground

### Rear Compartment Lamp

#### Connector Part Information

OEM: KET MG 610043
Description: 2-Way F Connector (BK)

#### Rear Compartment Lamp

Pin

Wire

Circuit

Function

1

OG

640

Battery Positive Voltage

2

PK/BK

1303

Rear Compartment Lid Ajar Switch Signal

### Rear Compartment Latch (Notchback)

#### Connector Part Information

OEM: KET MG 651032
Description: 3-Way F 090-II Series (WH)

#### Rear Compartment Latch (Notchback)

Pin

Wire

Circuit

Function

1

BK

1250

Ground

2

BN

253

Trunk Release Relay Control

3

PK/BK

1303

Rear Compartment Lid Ajar Switch Signal

### Rear Compartment Lid Release Actuator (Notchback)

#### Connector Part Information

OEM: KET MG 651032
Description: 3-Way F 090-II Series (WH)

#### Rear Compartment Lid Release Actuator (Notchback)

Pin

Wire

Circuit

Function

1

0.3 BK

1250

Ground

2

0.5 BN

253

Trunk Ajar Switch Signal

3

0.5 PK/BK

1303

Rear Compartment Lid Ajar Switch Signal

### Rear Compartment Lid Release Switch (Notchback)

#### Connector Part Information

OEM: KET MG 651201
Description: 2-Way F 090-II Series

#### Rear Compartment Lid Release Switch (Notchback)

Pin

Wire

Circuit

Function

1

0.5 BN

253

Trunk Release Relay Control

2

0.5 OG

640

Battery Positive Voltage

### Rear Compartment Tamper Switch

#### Connector Part Information

OEM: AMP 174463
Description: 2-Way M 070 Series Multilock 2P (WH)

#### Rear Compartment Tamper Switch

Pin

Wire

Circuit

Function

1

0.5 L-BU

263

Rear Compartment Lid Ajar Switch Signal

2

0.3 BK

1250

Ground

750

### Rear Compartment Tamper Switch (Notchback)

#### Connector Part Information

OEM: AMP 174463
Description: 2-Way M 070 Series Multilock 2P (WH)

#### Rear Compartment Tamper Switch (Notchback)

Pin

Wire

Circuit

Function

1

L-BU

263

Rear Compartment Lid Ajar Switch Signal

2

BK

1250

Ground

### Rear Fog Lamp Relay (T79)

#### Connector Part Information

OEM: AK 36907
Description: 9-Way F Connector (BK)

#### Rear Fog Lamp Relay (T79)

Pin

Wire

Circuit

Function

1

--

--

Not Used

2

PU

1977

Outside Moisture Sensor Signal 1

3

--

--

Not Used

4

OG

1540

Battery Positive Voltage (w/Rear Fog Lamps) (w/Lamp Driver Control Module)

5

YE

317

Front Fog Relay Coil Supply Voltage

6

RD

122

Rear Fog Lamp Supply Voltage

7

L-BU

1346

Headlamp Relay Supply Voltage

8

BK

250

Ground

9

--

--

Not Used

### Rear Liftgate Latch - C1 (Hatchback)

#### Connector Part Information

OEM: KET MG 610047
Description: 4-Way F 250 Series (WH)

#### Rear Liftgate Latch - C1 (Hatchback)

Pin

Wire

Circuit

Function

1

PU

294

Door Lock Actuator Unlock Control

2

--

--

Not Used

3

GY

295

Door Lock Actuator Lock Control

4

--

--

Not Used

### Rear Liftgate Latch - C2 (Hatchback)

#### Connector Part Information

OEM: KET MG 610392
Description: 2-Way F SDL Series (WH)

#### Rear Liftgate Latch - C2 (Hatchback)

Pin

Wire

Circuit

Function

1

PK/BK

1303

Rear Compartment Lid Ajar Switch Signal

2

BK

750

Ground

### Rear Liftgate Latch - C3 (Hatchback)

#### Connector Part Information

OEM: AMP 174463
Description: 2-Way M 070 Series Multilock 2P (WH)

#### Rear Liftgate Latch - C3 (Hatchback)

Pin

Wire

Circuit

Function

1

L-BU

263

Rear Compartment Lid Ajar Switch

2

BK

750

Ground

### Rear Window Defogger X1

#### Connector Part Information

OEM: 12092133
Description: 1-Way F Metri-Pack 630 Series Self Lock (WH)

#### Rear Window Defogger X1

Pin

Wire

Circuit

Function

A

2 PU

293

Rear Defogger Element Supply Voltage

### Rear Window Defogger X2

#### Connector Part Information

OEM: 12092133
Description: 1-Way F Metri-Pack 630 Series Self Lock (WH)

#### Rear Window Defogger X2

Pin

Wire

Circuit

Function

A

0.5 BK

750

Ground

### Recirculation Actuator

#### Connector Part Information

OEM: KET MG 610203
Description: 7-Way F 118 (PA) Series (BK)

#### Recirculation Actuator

Pin

Wire

Circuit

Function

1-3

--

--

Not Used

4

0.85 BN

41

Automatic HVAC - Ignition 2 Voltage

0.5 PK

239

Manual HVAC - Ignition 1 Voltage

5

0.3 PK/WH

1648

Automatic HVAC - Recirculation Door Control A

0.5 L-GN/BK

1648

Manual HVAC - Recirculation Door Control A

6

--

--

Not Used

7

0.3 D-GN/BK

1647

Automatic HVAC - Recirculation Door Control B

0.5 PK/WH

1647

Manual HVAC - Recirculation Door Control B

### Remote Control Door Lock Receiver/Theft Deterrent Control Module (w/Alarm)

#### Connector Part Information

OEM: KET MG 611336
Description: 26-Way F PCB Connector (WH)

#### Remote Control Door Lock Receiver/Theft Deterrent Control Module (w/Alarm)

Pin

Wire

Circuit

Function

1

0.5 YE (North America)

261

Arm Alarm Signal

0.5 YE/D-GN

2

0.5 BK

350

Ground

3

--

--

Not Used

4

0.5 L-BU

263

Rear Compartment Lid Ajar Switch Signal

5

0.5 PK/BK

1303

Rear Compartment Lid Ajar Switch Signal

6

--

--

Not Used

7

0.5 PK/D-BU

109

Hood Ajar Switch Signal

8

0.5 PU

156

Courtesy Lamp Control

9

0.3 L-BU/BK (North America)

195

Door Unlock Control

0.3 L-BU

10

0.5 L-GN/WH

355

Driver Door Lock Relay Lock Control

11

0.5 YE

356

Driver Door Lock Relay Unlock Control

12

0.5 L-GN

1370

Driver Door Lock Switch

13

0.5 D-BU

15

Right Turn Signal Lamp Supply Voltage

14

--

--

Not Used

15

0.5 PK

639

Ignition 1 Voltage

16

--

--

Not Used

17

0.5 L-GN

483

Serial Data

18

0.5 L-GN/RD

80

Key In Ignition Switch Signal

19

0.3 YE/D-GN

749

Security Indicator Control

20

0.5 PU

1371

Door Lock Switch Signal

21-23

--

--

Not Used

24

0.5 BN

253

Trunk Release Relay Control (Notchback)

25

1.25 OG

340

Battery Positive Voltage

26

0.5 L-BU/BK

14

Left Turn Signal Lamps Supply Voltage

L-BU (North America

### Remote Control Door Lock Receiver/Theft Deterrent Control Module (w/o Alarm)

#### Connector Part Information

OEM: 611336
Description: 26-Way F PCB Connector (WH)

#### Remote Control Door Lock Receiver/Theft Deterrent Control Module (w/o Alarm)

Pin

Wire

Circuit

Function

1

--

--

Not Used

2

BK

350

Ground

3-7

--

--

Not Used

8

PU

156

Courtesy Lamp Control

9

--

--

Not Used

10

L-GN/WH

355

Driver Door Lock Relay Lock Control

11

YE

356

Driver Door Lock Relay Unlock Control

12

--

--

Not Used

13

D-BU

15

Right Turn Signal Lamp Supply Voltage

14-16

--

--

Not Used

17

L-GN

483

Serial Data

18

L-GN/RD

80

Key In Ignition Switch Signal

19-23

--

--

Not Used

24

BN

253

Trunk Release Relay Control (Notchback)

25

OG

340

Battery Positive Voltage

26

L-BU/BK

14

Left Turn Signal Lamps Supply Voltage

L-BU

### Rough Road Sensor (L95, LXT)

#### Connector Part Information

OEM: Bosch 2264-420424
Description: 2-Way F Metri-Pack 150 Series, Sealed (GY)

#### Rough Road Sensor (L95, LXT)

Pin

Wire

Circuit

Function

A

0.5 WH

873

Rough Road Sensor Signal

B

0.5 OG

830

5-Volt Reference

### Rough Road Sensor (LDA)

#### Connector Part Information

OEM: PED 12162185
Description: 3-Way Metri-Pack 150.2 Series Sealed, Pull To Seat (BK)

#### Rough Road Sensor (LDA)

Pin

Wire

Circuit

Function

A

0.5 GY

605

5-Volt Reference

B

0.5 D-GN

602

Rough Road Sensor Signal

C

0.5 PU/WH

632

Low Reference

### Rough Road Sensor (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

OEM: PED 12162185
Description: 3-Way Metri-Pack 150.2 Series Sealed, Pull To Seat (BK)

#### Rough Road Sensor (w/o Throttle Actuator Control) (L34)

Pin

Wire

Circuit

Function

A

0.5 GY

605

5-Volt Reference

B

0.5 D-GN

602

Rough Road Sensor Signal

C

0.5 PU/WH

632

Low Reference

### Rough Road Sensor (w/o ABS) (w/Throttle Actuator Control) (L34)

#### Connector Part Information

OEM: PED 12162185
Description: 3-Way F Metri-Pack 150.2 Series Sealed, Pull To Seat (BK)

#### Rough Road Sensor (w/o ABS) (w/Throttle Actuator Control) (L34)

Pin

Wire

Circuit

Function

A

0.5 GY

605

5-Volt Reference

B

0.5 D-GN

602

Rough Road Sensor Signal

C

0.5 PU/WH

632

Low Reference

### Seat Belt Pretensioner

#### Connector Part Information

OEM: V23540-M5302-Y22
Description: 2-Way F Connector (GN)

#### Seat Belt Pretensioner

Pin

Wire

Circuit

Function

1

0.5 PU

1185

Seat Belt Pretensioner - Driver High Control

0.5 RD/BK

1187

Seat Belt Pretensioner - Passenger Low Control

2

0.5 YE/D-BU

1184

Seat Belt Pretensioner - Driver Low Control

0.5 D-BU/WH

1186

Seat Belt Pretensioner - Passenger High Control

### Seat Belt Switch

#### Connector Part Information

OEM: KET MG 610392
Description: 2-Way F Sealed Series (WH)

#### Seat Belt Switch

Pin

Wire

Circuit

Function

1

0.3 BK/WH

238

Seat Belt Switch - Left

2

0.3 BK

350

Ground

### Security Indicator

#### Connector Part Information

OEM: KET MG 610070
Description: 2-Way F 090 (2.3 mm) Series (WH)

#### Security Indicator

Pin

Wire

Circuit

Function

1

0.5 OG

640

Battery Positive Voltage

2

0.3 YE

749

Security Indicator Control

### Shift Indicator Lamp

#### Connector Part Information

OEM: 94797519
Description: 2-Way F (BK)

#### Shift Indicator Lamp

Pin

Wire

Circuit

Function

1

D-GN

44

Instrument Panel Lamps Dimming Control

2

BN/WH

309

Right Park Lamp Supply Voltage

### Shift Program Switch (MLQ)

#### Connector Part Information

OEM: KET MG 610366
Description: 4-Way F PCB 040 Series (WH)

#### Shift Program Switch (MLQ)

Pin

Wire

Circuit

Function

1

0.5 D-GN/WH

1135

Auto Shift Lock Solenoid Supply Voltage

2

BN/WH

309

Right Park Lamp Supply Voltage

3

D-GN

44

Instrument Panel Lamps Dimmer Switch Signal

4

0.5 BK

1050

Ground

### Shift Program Switch (MFA)

#### Connector Part Information

OEM: KET MG 610366
Description: 4-Way F PCB 040 Series (WH)

#### Shift Program Switch (MFA)

Pin

Wire

Circuit

Function

1

0.5 D-GN/WH

1135

Auto Shift Lock Solenoid Supply Voltage

2

BN/WH

309

Right Park Lamp Supply Voltage

3

D-GN

44

Instrument Panel Lamps Dimmer Switch Signal

4

0.5 BK

1050

Ground

### Side Marker Lamp - Left Rear

#### Connector Part Information

OEM: 12110053
Description: 2-Way F Lamp Socket Wedge Base W2 (L-GY)

#### Side Marker Lamp - Left Rear

Pin

Wire

Circuit

Function

A

PU

709

Left Park Lamp Supply Voltage

B

BK

550

Ground

### Side Marker Lamp - Right Rear

#### Connector Part Information

OEM: 12110053
Description: 2-Way F Lamp Socket Wedge Base W2 (L-GY)

#### Side Marker Lamp - Right Rear

Pin

Wire

Circuit

Function

A

WH

309

Right Park Lamp Supply Voltage

B

BK

550

Ground

### Speaker - Double (DBS)

#### Connector Part Information

OEM: KET MG 651038
Description: 4-Way F

#### Speaker - Double (DBS)

Pin

Wire

Circuit

Function

1

PU

201

Left Front Speaker Output (+)

2

GY/WH

118

Left Front Speaker Output (-)

3

PU

1201

Left Front Speaker Output (+)

4

D-GN

1118

Left Front Speaker Output (-)

### Speaker - Tweeters - Front

#### Connector Part Information

OEM: KET MG 610070
Description: 2-Way F 090 (2.3mm) Series (WH)

#### Speaker - Tweeters - Front

Pin

Wire

Circuit

Function

1

0.5 PU

201

Left Front Speaker Output (+)

0.5 L-GN

200

Right Front Speaker Output (+)

2

0.5 GY/WH

118

Left Front Speaker Output (-)

0.5 D-GN

117

Right Front Speaker Output (-)

### Speaker - Tweeters - Rear

#### Connector Part Information

OEM: KET MG 610070
Description: 2-Way F 090 (2.3mm) Series (WH)

#### Speaker - Tweeters - Rear

Pin

Wire

Circuit

Function

1

0.5 BN

199

Left Rear Speaker Output (+)

0.5 BN

46

Right Rear Speaker Output (+)

2

0.5D-GN

116

Left Rear Speaker Output (-)

0.5 D-GN

115

Right Rear Speaker Output (-)

### Speakers - Front

#### Connector Part Information

OEM: KET MG 651026
Description: 2-Way F 090-II Series (WH)

#### Speakers - Front

Pin

Wire

Circuit

Function

1

0.50 PU

201

Left Front Speaker Output (+)

0.5 L-GN

200

Right Front Speaker Output (+)

2

0.5 GY/WH

118

Left Front Speaker Output (-)

0.5 D-GN

117

Right Front Speaker Output (-)

### Speakers - Rear

#### Connector Part Information

OEM: KET MG 651026
Description: 2-Way F 090-II Series (WH)

#### Speakers - Rear

Pin

Wire

Circuit

Function

1

0.5 BN

199

Left Rear Speaker Output (+)

0.5 BN

46

Right Rear Speaker Output (+)

2

0.5 D-GN

116

Left Rear Speaker Output (-)

0.5 D-GN

115

Right Rear Speaker Output (-)

### Steering Wheel Position Sensor

#### Connector Part Information

OEM: PED 12064758
Description: 3-Way F Metri-Pack 150 Series, Unsealed (BK)

#### Steering Wheel Position Sensor

Pin

Wire

Circuit

Function

1

0.5 GY

1416

Battery Positive Voltage

2

0.5 L-BU

1533

Steering Wheel Sensor Signal

3

0.5 BK/WH

451

Ground

### Stop Lamp Switch

#### Connector Part Information

OEM: KET MG 610267
Description: 4-Way F 250 D/L Series (WH)

#### Stop Lamp Switch

Pin

Wire

Circuit

Function

1

OG

239

Ignition 1 Voltage

2

OG/BK

540

Battery Positive Voltage

3

D-GN

286

Automatic Transmission Shift Lock Solenoid Supply Voltage

4

L-BU

20

Stop Lamp Supply Voltage

### Sunload Sensor (C68)

#### Connector Part Information

OEM: KET MG 610489
Description: 2-Way F 090 (2.3 mm) Series

#### Sunload Sensor (C68)

Pin

Wire

Circuit

Function

1

0.5 YE

61

Low Reference

2

0.5 L-BU/BK

590

Sunload Sensor Signal

### Sunroof Module

#### Connector Part Information

OEM: AMP 174923
Description: 6-Way F 070 Multi-Lock Connector (WH)

#### Sunroof Module

Pin

Wire

Circuit

Function

1

0.3 D-GN/WH

133

Sunroof Limit Switch Low Reference

2

--

--

Not Used

3

1.25 BN

641

Ignition 2 Voltage

4

1.25 BK

850

Ground

5

--

--

Not Used

6

0.3 PU

132

Sunroof Limit Switch Soft Stop Signal

### Sunroof Switch/Reading Lamp

#### Connector Part Information

OEM: KET MG 610402
Description: 8-Way F SDL Series (WH)

#### Sunroof Switch/Reading Lamp

Pin

Wire

Circuit

Function

1

0.5 BK

850

Ground

2

--

--

Not Used

3

0.5 OG

640

Battery Positive Voltage

4

D-GN/WH

133

Sunroof Limit Switch Low Reference

5

0.3 BN

641

Ignition 3 Voltage

6

0.3 PU

132

Sunroof Limit Switch Soft Stop Signal

7-8

--

--

Not Used

### Tail/Stop Lamp - Left Rear Inner (Hatchback)

#### Connector Part Information

OEM: 12160394
Description: 3-Way F Lamp Socket Wedge Base W3 Right Angle (WH)

#### Tail/Stop Lamp - Left Rear Inner (Hatchback)

Pin

Wire

Circuit

Function

A

RD

20

Stop Lamp Supply Voltage

B

WH/D-GN

709

Left Park Lamp Supply Voltage

G

BK

450

Ground

### Tail/Stop Lamp - Left Rear Outer (Hatchback)

#### Connector Part Information

OEM: 12092379
Description: 3-Way F Lamp Socket Wedge Base W3 (WH)

#### Tail/Stop Lamp - Left Rear Outer (Hatchback)

Pin

Wire

Circuit

Function

A

RD

20

Stop Lamp Supply Voltage

B

WH/BK

709

Left Park Lamp Supply Voltage

G

BK

250

Ground

### Tail/Stop Lamp - Right Rear Inner (Hatchback)

#### Connector Part Information

OEM: 12160394
Description: 3-Way F Lamp Socket Wedge Base W3 Right Angle (WH)

#### Tail/Stop Lamp - Right Rear Inner (Hatchback)

Pin

Wire

Circuit

Function

A

RD

20

Stop Lamp Supply Voltage

B

WH/D-GN

309

Right Park Lamp Supply Voltage

G

BK

450

Ground

### Tail/Stop Lamp - Right Rear Outer (Hatchback)

#### Connector Part Information

OEM: 12092379
Description: 3-Way F Lamp Socket Wedge Base W3 (WH)

#### Tail/Stop Lamp - Right Rear Outer (Hatchback)

Pin

Wire

Circuit

Function

A

RD

20

Stop Lamp Supply Voltage

B

WH/BK

309

Left Park Lamp Supply Voltage

G

BK

450

Ground

### Theft Deterrent Alarm

#### Connector Part Information

OEM: KUM PB 625-02027
Description: 2-Way F NMWP 04F-B Ass'y (BK)

#### Theft Deterrent Alarm

Pin

Wire

Circuit

Function

1

0.5 YE

261

Arm Alarm Signal

2

0.5 OG

1240

Battery Positive Voltage

### Throttle Body (L95, LXT)

#### Connector Part Information

OEM: AMP 174982-2
Description: 8-Way F 070 Series Econoseal J-Mark II + 8P (BK)

#### Throttle Body (L95, LXT)

Pin

Wire

Circuit

Function

1

0.5 D-BU

426

Idle Motor Return

2

0.5 GY

416

5-Volt Reference

3

--

--

Not Used

4

0.5 D-GN

534

High Idle Switch Signal

5

0.5 L-BU

425

Idle Motor Feed

6

0.5 PK

427

Idle Speed Motor Switch Signal

7

0.5 D-BU

417

Throttle Position (TP) Sensor Signal

8

0.5 BK/YE

808

Low Reference

### Throttle Body Assembly (w/Throttle Actuator Control) (L34)

#### Connector Part Information

OEM: AMP 174982-2
Description: 8-Way M 070 Series Econoseal J-Mark II + 8P (BK)

#### Throttle Body Assembly (w/Throttle Actuator Control) (L34)

Pin

Wire

Circuit

Function

1

0.5 BN

550

Low Reference

2

0.5 D-GN/WH

417

Throttle Position (TP) Sensor 1 Signal

3

0.5 GY

534

Throttle Position (TP) Sensor 2 Signal

4

0.5 D-BU/YE

474

5-Volt Reference

5

0.5 D-BU/RD

426

TAC Motor 1 Control

6-7

--

--

Not Used

8

0.5 L-BU/WH

425

TAC Motor 2 Control

### Throttle Plate Actuator (LMN)

#### Connector Part Information

OEM: FEP 42121400
Description: 4-Way F Sealed

#### Throttle Plate Actuator (LMN)

Pin

Wire

Circuit

Function

1

BK

--

Ground

2

PK/WH

--

Battery Positive Voltage

3

WH/BK

--

Throttle Valve Control

4

GN

--

Feedback Signal

### Throttle Position (TP) Sensor (L79)

#### Connector Part Information

OEM: PED 12065287
Description: 3-Way F Metri-Pack 150 Series (BK)

#### Throttle Position (TP) Sensor (L79)

Pin

Wire

Circuit

Function

A

0.5 GY

416

5-Volt Reference

B

0.5 BK/YE

808

Low Reference

C

0.5 D-BU

417

Throttle Position (TP) Sensor Signal

### Throttle Position (TP) Sensor (LDA)

#### Connector Part Information

OEM: PED 12065287
Description: 3-Way F Metri-Pack 150 Series (BK)

#### Throttle Position (TP) Sensor (LDA)

Pin

Wire

Circuit

Function

A

0.5 D-GN/WH (D-GN/YE)

416

5-Volt Reference

B

0.5 BK

808

Low Reference

C

0.5 GY (D-BU)

417

Throttle Position (TP) Sensor Signal

### Throttle Position (TP) Sensor (w/o Throttle Actuator Control) (L34)

#### Connector Part Information

OEM: PED 12065287
Description: 3-Way F Metri-Pack 150 Series (BK)

#### Throttle Position (TP) Sensor (w/o Throttle Actuator Control) (L34)

Pin

Wire

Circuit

Function

1

0.5 BK

808

Low Reference

2

0.5 D-GN/WH (D-GN/YE)

416

5-Volt Reference

3

0.5 GY (D-BU)

417

Throttle Position (TP) Sensor Signal

### Tire Pressure Monitor System (TPMS) Module

#### Connector Part Information

OEM:
Description: 12-Way F

#### Tire Pressure Monitor System (TPMS) Module

Pin

Wire

Circuit

Function

1

OG

--

Battery Positive Voltage

2

D-GN/WH

--

Vehicle Speed Signal

3

PU

--

Serial Data

4

PU/WH

--

Brake Indicator Signal

5

WH

--

Light Switch

6

--

--

Not Used

7

BN

--

Charge Indicator Signal

8

PK

--

Ignition 2 Voltage

9

BK

--

Horn Relay

10

BN/WH

--

TPMS Indicator Control

11

BK

--

Ground

12

--

--

Not Used

### Transaxle (M98)

#### Connector Part Information

OEM: YZK 7223-6509-40
Description: 14-Way F 050 Sealed

#### Transaxle (M98)

Pin

Wire

Circuit

Function

1

OG/BK

--

Transmission Fluid Temperature Sensor Low Reference

2

BU

--

Clutch Pressure Solenoid Control

3

L-BU

--

L-Up Solenoid Control

4

YE/BK

--

Pressure Solenoid Control

5

--

--

Not Used

6

BN/WH

--

Shift Solenoid 4 Control

7

YE/BK

--

Shift Solenoid 2 Control

8

PU

--

Transmission Fluid Temperature Sensor Signal

9

L-BU

--

Clutch Pressure Solenoid Supply Voltage

10

BU

--

L-Up Solenoid Supply Voltage

11

RD

--

Pressure Solenoid Supply Voltage

12

YE/WH

--

Shift Solenoid 5 Control

13

PK

--

Shift Solenoid 3 Control

14

L-GN

--

Shift Solenoid 1 Control

### Transmission Connector (MLQ)

#### Connector Part Information

OEM: YAZAKI 7283-1407-40
Description: 10-Way F (GY)

#### Transmission Connector (MLQ)

Pin

Wire

Circuit

Function

1

0.5 PU

898

Transmission Fluid Temperature Sensor Signal

2

0.5 PK

1224

Timing Valve Control

3

0.5 RD

1226

Pressure Control Solenoid Control

4

0.5 D-BU

1225

Torque Converter Solenoid Control

5

0.5 L-GN

1222

Shift Solenoid 1 Valve Control

6

0.5 OG/BK

586

Transmission Fluid Temperature Sensor - Low Reference

7

--

--

Not Used

8

0.5 YE/BK

1227

Low Reference

9

--

--

Not Used

10

0.5 YE/BK

1223

Shift Solenoid 2 Valve Control

### Transmission Connector (MFA)

#### Connector Part Information

OEM: KOSTAL 09430010
Description: 16-Way F Connector (BK)

#### Transmission Connector (MFA)

Pin

Wire

Circuit

Function

1

0.5 D-BU/WH

3006

Automatic Transmission Output Shaft Speed (OSS) Sensor - High Signal

2

0.5 YE/BK

3007

Automatic Transmission Output Shaft Speed (OSS) Sensor - Low Signal

3

0.85 L-BU/BK

3688

Voltage Reference

4

0.5 D-GN/WH

3009

Low Reference

5

0.85 OG

2020

Voltage Reference

6

0.85 D-GN/BK

3021

Pressure Control Solenoid (PCS) 3 Control

7

0.85 BN

3022

Pressure Control Solenoid (PCS) 4 Control

8

--

--

Not Used

9

0.5 GY

3008

Transmission Fluid Temperature Sensor Signal

10

0.85 BN/WH

3023

Pressure Control Solenoid (PCS) 5 Control

11

0.85 D-GN/WH

3024

Pressure Control Solenoid (PCS) 6 Control

12

0.85 WH/BK

3025

Shift Solenoid (SS) 1 Control

13

0.85 WH/BN

3026

Shift Solenoid (SS) 2 Control

14

--

--

Not Used

15

0.5 D-BU/WH

3005

Automatic Transmission Input Shaft Speed (ISS) Sensor - Low Signal

16

0.5 YE/BK

3004

Automatic Transmission Input Shaft Speed (ISS) Sensor - High Signal

### Transmission Control Module (TCM) X1 (M98)

#### Connector Part Information

OEM: TYCO 1318756-2
Description: 24-Way F 025/090III Hybrid Unsealed

#### Transmission Control Module (TCM) X1 (M98)

Pin

Wire

Circuit

Function

1

BK/WH

--

Ground

2

YE/BK

--

Pressure Solenoid Control

3

L-BU

--

L-Up Solenoid Control

4

RD

--

Pressure Solenoid Supply Voltage

5

BU

--

L-Up Solenoid Supply Voltage

6

PK

--

Ignition 1 Voltage

7

YE

--

CAN Low

8-10

--

--

Not Used

11

PU

--

Transmission Fluid Temperature Sensor Signal

12

OG/BK

--

Transmission Fluid Temperature Sensor Low Reference

13

BN/WH

--

Shift Solenoid 4 Control

14

PK

--

Shift Solenoid 3 Control

15

YE/BK

--

Shift Solenoid 2 Control

16

L-GN

--

Shift Solenoid 1 Control

17

PU

--

CAN High

18

--

--

Not Used

19

BU

--

Clutch Pressure Solenoid Control

20

--

--

Not Used

21

L-BU

--

Clutch Pressure Solenoid Supply Voltage

22

YE/WH

--

Shift Solenoid 5 Control

23

BK/WH

--

Ground

24

OG

--

Battery Positive Voltage

### Transmission Control Module (TCM) X1 (MFA)

#### Connector Part Information

OEM: KET MG 651804
Description: 16-Way F .060-II Connector (BU)

#### Transmission Control Module (TCM) X1 (MFA)

Pin

Wire

Circu

Function

1

0.85 WH/BN

3026

Shift Solenoid (SS) 2 Control

2

D-GN

3017

Transmission Mode Signal Power

3

0.85 BN

3022

Pressure Control Solenoid (PCS) 4 Control

4

0.5 GY

3008

Transmission Fluid Temperature Sensor Signal

5

0.85 L-BU

20

Stop Lamp Supply Voltage

6

0.5 YE

1481

Hold Mode Indicator Control

7

0.5 BN

2000

Serial Data

8

0.5 PU

1807

CAN Serial Data - High

9

0.85 WH/BK

3025

Shift Solenoid (SS) 1 Control

10

0.85 BN/WH

3023

Pressure Control Solenoid (PCS) 5 Control

11

0.85 D-GN/BK

3021

Pressure Control Solenoid (PCS) 3 Control

12

0.85 D-GN/WH

3024

Pressure Control Solenoid (PCS) 6 Control

13-15

--

--

Not Used

16

0.3 YE

710

CAN Serial Data - Low

### Transmission Control Module (TCM) X1 (MLQ)

#### Connector Part Information

OEM: AMP 1318756-1 A
Description: 24-Way F 025/090 SER 24POS Plug Assembly (WH)

#### Transmission Control Module (TCM) X1 (MLQ)

Pin

Wire

Circuit

Function

1

0.5 BK/WH

51

Ground

2

0.5 YE/BK

1227

Low Reference

3

--

--

Not Used

4

0.5 RD

1226

Pressure Control Solenoid Control

5

0.5 D-BU

1225

Torque Converter Clutch Solenoid Control

6

0.5 PK

839

Ignition 1 Voltage

7

0.5 YE

710

CAN Serial Data Low

8-10

--

--

Not Used

11

0.5 PU

898

Transmission Fluid Temperature Sensor Signal

12

0.5 OG/BK

586

Transmission Fluid Temperature Sensor Signal - Low Reference

13

--

--

Not Used

14

0.5 PK

1224

Timing Valve Control

15

0.5 YE/BK

1223

Shift Solenoid 2 Valve Control

16

0.5 L-GN

1222

Shift Solenoid 1 Valve Control

17

0.5 PU

1807

CAN Serial Data High

18-22

--

--

Not Used

23

0.5 BK/WH

51

Ground

24

0.5 OG

440

Battery Positive Voltage

### Transmission Control Module (TCM) X2 (M98)

#### Connector Part Information

OEM: TYCO 1318757-2
Description: 26-Way F 025/090III Hybrid Unsealed

#### Transmission Control Module (TCM) X2 (M98)

Pin

Wire

Circuit

Function

1-2

--

--

Not Used

3

YE

--

Hold Mode Indicator Control

4

GN/WH

--

Hold Mode Switch Signal

5

YE/BK

--

Output Shaft Speed Sensor Signal Low

6

BU/WH

--

Input Shaft Speed Sensor Signal Low

7

WH

--

B Signal

8

WH

--

A Signal

9-13

--

--

Not Used

14

BU/WH

--

Output Shaft Speed Sensor Signal High

15

GN/WH

--

Vehicle Speed Signal

16

YE/BK

--

Input Shaft Speed Sensor Signal High

17-18

--

--

Not Used

19

PK

--

PA Signal

20

GN

--

C Signal

21

--

--

Not Used

22

L-BU

--

Stop Lamp Switch Signal

23

BU

--

Serial Data

24-26

--

--

Not Used

### Transmission Control Module (TCM) X2 (MFA)

#### Connector Part Information

OEM: KET MG 651803
Description: 16-Way F .060-II Connector (GN)

#### Transmission Control Module (TCM) X2 (MFA)

Pin

Wire

Circuit

Function

1

0.5 D-GN/WH

3009

Low Reference

2

0.5 YE/BK

3004

Automatic Transmission Input Shaft Speed (ISS) Sensor - High Signal

3

0.5 OG

440

Battery Positive Voltage

4

0.5 D-BU/WH

3005

Automatic Transmission Input Shaft Speed (ISS) Sensor - Low Signal

5

0.5 YE/BK

3007

Automatic Transmission Output Shaft Speed (OSS) Sensor - Low Signal

6

0.5 RD/D-BU

3012

Park/Neutral Position (PNP) Switch L3 Switch Signal

7

0.5 BN

3051

Shield Ground

0.5 BK (North America)

8

0.5 D-GN/WH

817

Vehicle Speed Signal

9

--

--

Not Used

10

0.5 D-BU/WH

3006

Automatic Transmission Output Shaft Speed (OSS) Sensor - High Signal

11

0.5 L-GN/BK

3013

Park/Neutral Position (PNP) Switch L4 Signal

12

1.25 BK/WH

251

Ground

13

1.25 BK/WH

251

Ground

14

--

--

Not Used

15

0.5 L-GN/RD

3011

Park/Neutral Position (PNP) Switch L2 Switch Signal

16

--

--

Not Used

### Transmission Control Module (TCM) X2 (MLQ)

#### Connector Part Information

OEM: AMP 1318757-1 B
Description: 26-Way F 025/090 SER 26POS Plug Assembly (WH)

#### Transmission Control Module (TCM) X2 (MLQ)

Pin

Wire

Circuit

Function

1

0.5 D-GN/WH

2383

Park Neutral Position (PNP) Switch Reverse Signal

0.5 D-GN/WH

24

Backup Lamp Supply Voltage

2

--

--

Not Used

3

0.5 YE

1481

Hold Mode Indicator Control

4

0.5 D-GN/WH

1135

Auto Shift Lock Solenoid Supply Voltage

5

--

--

Not Used

6

0.5 D-BU/WH

1296

Input Shaft Speed (ISS) Sensor High Signal

7

0.5 WH

2377

Park Neutral Position (PNP) Switch Drive Signal

8

0.5 YE

2381

Park Neutral Position (PNP) Switch Neutral Signal

9-15

--

--

Not Used

16

0.5 YE/BK

1297

Input Shaft Speed (ISS) Sensor Low Signal

17

--

--

Not Used

18

0.5 GY

2380

Park Neutral Position (PNP) Switch Low Gear Signal

19

0.5 PK

2384

Park Neutral Position (PNP) Switch 2nd Gear Signal

20

0.5 D-GN

2382

Park Neutral Position (PNP) Switch Park Signal

21

--

--

Not Used

22

0.5 L-BU

20

Stop Lamp Switch Signal

23

0.5 D-BU

2000

Serial Data

24

--

--

Not Used

25

0.5 D-GN/WH

817

Vehicle Speed Signal

26

--

--

Not Used

### Transmission Control Module (TCM) X3 (MFA)

#### Connector Part Information

OEM: KET MG 651802
Description: 16-Way F .060-II Connector (GY)

#### Transmission Control Module (TCM) X3 (MFA)

Pin

Wire

Circuit

Function

1

0.5 D-BU/RD

3010

Park/Neutral Position (PNP) Switch L1 Signal

2-3

--

--

Not Used

4

0.5 D-GN/WH

1135

Auto Shift Lock Solenoid Supply Voltage

5

--

--

Not Used

6

0.85 OG

2020

Voltage Reference

7

0.85 OG

2020

Voltage Reference

8

0.85 L-BU/BK

3688

Voltage Reference

9-14

--

--

Not Used

15

1.25 PK

439

Ignition 1 Voltage

16

1.25 PK

439

Ignition 1 Voltage

### Turn Signal Lamp - Left Front (Except North America)

#### Connector Part Information

OEM: KET MG 610320
Description: 2-Way F SWP Series (BK)

#### Turn Signal Lamp - Left Front (Except North America)

Pin

Wire

Circuit

Function

1

BK

50

Ground

2

L-BU

14

Left Turn Signal Lamps Supply Voltage

### Turn Signal Lamp - Left Rear

#### Connector Part Information

OEM: 15354859
Description: 2-Way F Lamp Socket BB W-3 (WH)

#### Turn Signal Lamp - Left Rear

Pin

Wire

Circuit

Function

A

YE

14

Left Turn Signal Lamps Supply Voltage

G

BK

50

Ground

### Turn Signal Lamp - Right Front (Except North America)

#### Connector Part Information

OEM: KET MG 610320
Description: 2-Way F SWP Series (BK)

#### Turn Signal Lamp - Right Front (Except North America)

Pin

Wire

Circuit

Function

1

BK

150

Ground

2

L-BU

15

Right Turn Signal Lamps Supply Voltage

### Turn Signal Lamp - Right Rear

#### Connector Part Information

OEM: 15354859
Description: 2-Way F Lamp Socket BB W-3 (WH)

#### Turn Signal Lamp - Right Rear

Pin

Wire

Circuit

Function

A

YE

14

Left Turn Signal Lamps Supply Voltage

G

BK

50

Ground

### Turn Signal Multifunction Switch

#### Connector Part Information

OEM: KET MG 610203
Description: 7-Way F 118 (PA) Series (BK)

#### Turn Signal Multifunction Switch

Pin

Wire

Circuit

Function

1

L-BU

14

Left Turn Signal Lamps Supply Voltage

2

PK

16

Turn Signal Flasher Signal

3

D-BU

15

Right Turn Signal Lamps Supply Voltage

4

L-GN

11

Headlamp High Beam Supply Voltage

5

PU

12

Headlamp Low Beam Supply Voltage

6

L-BU

1346

Headlamp Relay Supply Voltage

L-BU/BK

2346

Flash to Pass Signal (Except North America)

7

OG

140

Battery Positive Voltage

### Turn Signal Repeater Lamp - Left

#### Connector Part Information

OEM: KET MG 610320
Description: 2-Way F SWP Series (WH)

#### Turn Signal Repeater Lamp - Left

Pin

Wire

Circuit

Function

1

L-BU

14

Left Turn Signal Lamps Supply Voltage (North America)

BK

50

Ground

2

BK

1150

Ground (North America)

PU

709

Left Park Lamps Supply Voltage

### Turn Signal Repeater Lamp - Right

#### Connector Part Information

OEM: KET MG 610320
Description: 2-Way F SWP Series (WH)

#### Turn Signal Repeater Lamp - Right

Pin

Wire

Circuit

Function

1

L-BU

15

Right Turn Signal Lamps Supply Voltage (North America)

BK

150

Ground

2

BK

150

Ground (North America)

BN/WH

309

Right Park Lamps Supply Voltage

### Turn Signal/Hazard Flasher Module

#### Connector Part Information

OEM: AK 36906
Description: 9-Way Relay Connector (GN)

#### Turn Signal/Hazard Flasher Module

Pin

Wire

Circuit

Function

1

--

--

Not Used

2

L-BU

1508

Turn Signal Switch Signal

3-5

--

--

Not Used

6

PK

16

Turn Signal Flasher Signal

7

--

--

Not Used

8

BK

250

Ground

9

--

--

Not Used

### Variable Effort Steering Actuator

#### Connector Part Information

OEM: PED 12052643
Description: 2-Way F Metri-Pack 150 Series, Sealed (BN)

#### Variable Effort Steering Actuator

Pin

Wire

Circuit

Function

A

0.5 L-GN

1703

Variable Effort Steering Actuator Control

B

0.5 BN/BK

1738

Variable Effort Steering Actuator Supply Voltage

### Vehicle Speed Sensor (VSS) (MLQ)

#### Connector Part Information

OEM: YAZAKI 7283-1232-30
Description: 3-Way F Connector (BK)

#### Vehicle Speed Sensor (VSS) (MLQ)

Pin

Wire

Circuit

Function

1

0.5 PK

839

Ignition 1 Voltage

2

0.5 BK/WH

51

Ground

3

0.5 D-GN/WH

817

Vehicle Speed Signal

### Vehicle Speed Sensor (VSS) (Manual Transmission)

#### Connector Part Information

OEM: PED 12059595
Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Vehicle Speed Sensor (VSS) (Manual Transmission)

Pin

Wire

Circuit

Function

A

0.5 BK/WH

251

Ground

0.5 BK

251

Ground (Diesel)

B

0.5 D-GN/WH

817

Vehicle Speed Signal

C

0.5 PK/D-BU

539

Ignition 1 Voltage

0.5 PK/BK

539

Ignition 1 Voltage (Diesel)

### Wastegate Solenoid (LMN)

#### Connector Part Information

OEM: TYCO 827551-3
Description: 2-Way F Timmer Sealed

#### Wastegate Solenoid (LMN)

Pin

Wire

Circuit

Function

1

GN/BK

--

Wastegate Solenoid Control

2

PK/WH

--

Battery Positive Voltage

### Water In Fuel Sensor (LMN)

#### Connector Part Information

OEM: TYCO 85205-1
Description: 3-Way F JPT Sealed

#### Water In Fuel Sensor (LMN)

Pin

Wire

Circuit

Function

1

BN/WH

--

Signal

2

BK

--

Ground

3

PK

--

Battery Positive Voltage

### Wheel Speed Sensor (WSS) - Front

#### Connector Part Information

OEM: Bosch 2264-420424
Description: 2-Way F Metri-Pack 150 Series Sealed (GY)

#### Wheel Speed Sensor (WSS) - Front

Pin

Wire

Circuit

Function

A

0.5 BN

873

Left Front Wheel Speed Sensor Signal

0.5 WH

873

Left Front Wheel Speed Sensor Signal (Diesel)

0.5 PU

872

Right Front Wheel Speed Sensor Signal

B

0.5 L-BU

830

Left Front Wheel Speed Sensor Return

0.5 OG

830

Left Front Wheel Speed Sensor Return (Diesel)

0.5 YE

833

Right Front Wheel Speed Sensor Return

### Wheel Speed Sensor (WSS) - Rear

#### Connector Part Information

OEM: PED 12052644
Description: 2-Way F Metri-Pack 150 Series Sealed (GY)

#### Wheel Speed Sensor (WSS) - Rear

Pin

Wire

Circuit

Function

A

0.5 WH

885

Left Rear Wheel Speed Sensor Signal

0.5 WH

883

Right Rear Wheel Speed Sensor Signal

B

0.5 GY

884

Left Rear Wheel Speed Sensor Return

0.5 GY

882

Right Rear Wheel Speed Sensor Return

### Window Motor - Left Front

#### Connector Part Information

OEM: KET MG 610320
Description: 2-Way F SWP Series (BK)

#### Window Motor - Left Front

Pin

Wire

Circuit

Function

1

1.25 D-BU

164

Power Window Motor Driver Front Up Control

2

1.25 BN

165

Power Window Motor Driver Front Down Control

### Window Motor - Left Rear

#### Connector Part Information

OEM: AMP 174198-1
Description: 2-Way M Connector (WH)

#### Window Motor - Left Rear

Pin

Wire

Circuit

Function

1

2 D-BU

668

Power Window Motor Left Rear Up Control

2

2 BN

669

Power Window Motor Left Rear Down Control

### Window Motor - Right Front

#### Connector Part Information

OEM: KET MG 610320
Description: 2-Way F SWP Series (BK)

#### Window Motor - Right Front

Pin

Wire

Circuit

Function

1

2 D-BU

666

Power Window Motor Passenger Front Up Control

2

2 BN

667

Power Window Motor Passenger Front Down Control

### Window Motor - Right Rear

#### Connector Part Information

OEM: AMP 174198-1
Description: 2-Way M Connector

#### Window Motor - Right Rear

Pin

Wire

Circuit

Function

1

2 D-BU

668

Power Window Motor Right Rear Up Control

2

2 BN

669

Power Window Motor Right Rear Down Control

### Window Switch - Driver - Front Power Only

#### Connector Part Information

OEM: KET MG 651050
Description: 8-Way F 090-II Series (WH)

#### Window Switch - Driver - Front Power Only

Pin

Wire

Circuit

Function

1

1.25 BN

165

Power Window Motor Driver Front Down Control

2

D-BU

1307

Power Window Master Switch Lockout Control

3

L-BU

166

Power Window Master Switch Passenger Front Up Signal

4

1.25 RD

581

Power Window Master Switch Lockout Control

5

2 OG

580

Power Window Supply Voltage

6

1.25 D-BU

164

Power Window Motor Driver Front Up Control

7

2 BK

1150

Ground

8

PU

167

Power Window Master Switch Passenger Front Down Signal

### Window Switch - Left Front - Front/Rear Power

#### Connector Part Information

OEM: KET MG 651110
Description: 14-Way F 090-II Series (WH)

#### Window Switch - Left Front - Front/Rear Power

Pin

Wire

Circuit

Function

1

1.25 BN

165

Power Window Motor Driver Front Down Control

2

1.25 D-BU

164

Power Window Motor Driver Front Up Control

3

1.25 RD

581

Power Window Master Switch Lockout Control

4

2 PU

167

Power Window Master Switch Passenger Front Down Signal

5

OG/D-BU

64

Auto Up (A33)

6

2 L-BU

166

Power Window Master Switch Passenger Front Up Signal

7

7 D-BU

1307

Power Window Master Switch Lockout Control

8

2 PU/RD

169

Power Window Master Switch Lockout Control

9

OG/D-BU

64

Auto Up (A33)

10

2 OG

580

Power Window Supply Voltage

11

2 BK

1150

Ground

12

2 D-GN

168

Power Window Master Switch Left Rear Up Signal

13

2 PU/WH

171

Power Window Master Switch Right Rear Down Signal

14

2 L-GN

170

Power Window Master Switch Right Rear Up Signal

### Window Switch - Left Rear

#### Connector Part Information

OEM: KET MG 651050
Description: 8-Way F 090-II Series (WH)

#### Window Switch - Left Rear

Pin

Wire

Circuit

Function

1

2 BN

669

Power Window Motor Left Rear Down Control

2

--

--

Not Used

3

2 D-BU

668

Power Window Motor Left Rear Up Control

4

2 PU

169

Power Window Master Switch Left Rear Down Signal

5

--

--

Not Used

6

1.25 D-BU

1307

Power Window Master Switch Lockout Control

7

0.5 BK

1250

Ground

8

2 D-GN

168

Power Window Master Switch Left Rear Up Signal

### Window Switch - Right Front

#### Connector Part Information

OEM: KET MG 651050
Description: 8-Way F 090-II Series (WH)

#### Window Switch - Right Front

Pin

Wire

Circuit

Function

1

2 BN

667

Power Window Motor Right Rear Up Control

2

--

--

Not Used

3

2 D-BU

666

Power Window Motor Passenger Front Up Control

4

2 PU

167

Power Window Master Switch Passenger Front Down Signal

5

--

--

Not Used

6

2 D-BU

1307

Power Window Master Switch Lockout Control

7

0.5 BK

350

Ground

8

2 L-BU

166

Power Window Master Switch Passenger Front Up Signal

### Window Switch - Right Rear

#### Connector Part Information

OEM: KET MG 651050
Description: 8-Way F 090-II Series (WH)

#### Window Switch - Right Rear

Pin

Wire

Circuit

Function

1

2 BN

669

Power Window Motor Right Rear Down Control

2

--

--

Not Used

3

2 D-BU

668

Power Window Motor Right Rear Up Control

4

2 PU

169

Power Window Master Switch Right Rear Down Signal

5

--

--

Not Used

6

1.25 D-BU

1307

Power Window Master Switch Lockout Control

7

0.5 BK

1250

Ground

8

2 D-GN

168

Power Window Master Switch Right Rear Up Signal

### Windshield Washer Fluid Pump (Hatchback)

#### Connector Part Information

OEM: KET MG 641362
Description: 3-Way F Connector (GY)

#### Windshield Washer Fluid Pump (Hatchback)

Pin

Wire

Circuit

Function

1

1.25 RD

228

Windshield Washer Pump Control

2

2 BK

1150

Ground

3

1.25 D-GN

392

Rear Window Wiper Motor Control

### Windshield Washer Fluid Pump (Notchback)

#### Connector Part Information

OEM: KET MG 640605
Description: 2-Way F 090 WP Series (WH)

#### Windshield Washer Fluid Pump (Notchback)

Pin

Wire

Circuit

Function

1

1.25 BK

50

Ground

2

1.25 RD

228

Washer Switch Signal

### Windshield Wiper Motor (w/CE1)

#### Connector Part Information

OEM: KUM PB 625-08027
Description: 8-Way F NMWP 08F-B Assembly (BK)

#### Windshield Wiper Motor (w/CE1)

Pin

Wire

Circuit

Function

1

1.25 D-GN

95

Windshield Wiper Motor Low Speed

2

1.25 BN

96

Windshield Wiper Switch Off/Delay Signal

3

1.25 BK

1150

Ground

4

0.5 L-GN

227

Outside Moisture Sensor Signal

5

1.25 PU

92

Windshield Wiper Motor High Speed

6

0.85 D-BU

1112

Outside Moisture Sensor Signal 1

7

0.5 D-GN

2228

Outside Moisture Sensor Signal 2

D-GN/WH

8

1.25 RD/D-BU

441

Ignition 3 Voltage

### Windshield Wiper Motor (w/o CE1)

#### Connector Part Information

OEM: KUM PB 625-08027
Description: 8-Way F NMWP 08F-B Assembly (BK)

#### Windshield Wiper Motor (w/o CE1)

Pin

Wire

Circuit

Function

1

1.25 D-GN

95

Windshield Wiper Motor Low Speed

2

0.85 YE

112

Windshield Wiper Switch Signal

3

1.25 BK

1150

Ground

4

--

--

Not Used

5

1.25 PU

92

Windshield Wiper Motor High Speed

6

1.25 BN

96

Windshield Wiper Off/Delay Signal

7

1.25 RD

228

Windshield Washer Pump Control

8

1.25 RD/D-BU

441

Ignition 3 Voltage

### Windshield Wiper/Washer Switch A

#### Connector Part Information

OEM: KET MG 610154
Description: 9-Way F 118 (PA) Series (WH)

#### Windshield Wiper/Washer Switch A

Pin

Wire

Circuit

Function

1

0.5 WH

393

Rear Window Wiper Motor Control (w/Rear Wipers)

2

1.25 D-GN

392

Rear Window Washer Pump Control (w/Rear Wipers)

3

1.25 BN

441

Ignition 1 Voltage

4

1.25 RD

228

Windshield Washer Pump Control

5

1.25 D-GN

95

Windshield Wiper Motor Low Speed

6

1.25 L-BU

97

Windshield Wiper Switch Off/Delay Signal

7

1.25 GY

91

Windshield Wiper Switch Pulse Delay Signal

8

1.25 BN

441

Ignition 1 Voltage

9

1.25 PU

92

Windshield Wiper Motor High Speed

### Windshield Wiper/Washer Switch B (w/Rear Fog Lamps)

#### Connector Part Information

OEM: AMP 368501-1
Description: 4-Way F 070 Series MLC Plug Hsg 4P (WH)

#### Windshield Wiper/Washer Switch B (w/Rear Fog Lamps)

Pin

Wire

Circuit

Function

1

GY

91

Windshield Wiper Switch Pulse Delay Signal

2

YE

112

Windshield Wiper Switch Signal 1

3

PU

1977

Outside Moisture Sensor Signal 1

4

BK

250

Ground

### Windshield Wiper/Washer Switch B (w/o Rear Fog Lamps)

#### Connector Part Information

OEM: AMP 174463-1
Description: 2-Way M 070 Series Multilock 2P (WH)

#### Windshield Wiper/Washer Switch B (w/o Rear Fog Lamps)

Pin

Wire

Circuit

Function

1

YE

112

Windshield Wiper Switch Signal 1

2

GY

91

Windshield Wiper Switch Pulse Delay Signal

### Wiper Washer Rain Sensor (CE1)

#### Connector Part Information

OEM: MLX 43645-0800
Description: 8-Way F Micro-Fit (3.0) 8 Circuit Single Row Receptacle

#### Wiper Washer Rain Sensor (CE1)

Pin

Wire

Circuit

Function

1

0.85 D-BU

1112

Outside Moisture Sensor Signal 1

2

0.5 D-GN

2228

Outside Moisture Sensor Signal 2

3

0.5 BK

850

Ground

4

0.5 PK

639

Ignition 1 Voltage

5

0.85 YE

112

Windshield Wiper Switch Signal 1

6

1.25 RD

228

Windshield Wiper Pump Control

7

0.5 L-GN

227

Outside Moisture Sensor Signal 2

8

--

--

Not Used

### Wiper Motor Rear

#### Connector Part Information

OEM: KET MG 610394
Description: 3-Way F Series Sealed (WH)

#### Wiper Motor Rear

Pin

Wire

Circuit

Function

1

0.5 WH

393

Rear Window Wiper Motor Control

2

1.25 BK

750

Ground

3

1.25 PK

441

Ignition 3 Voltage