For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Dash Seal Retaining Ring Nuts | 7 N·m | 62 lb in
Key Interlock Solenoid Screws | 2 N·m | 18 lb in
Key Reminder Switch Screws | 2 N·m | 18 lb in
Steering Column Jacket Assembly Front Bracket Nuts and Bolts | 22 N·m | 16 lb ft
Steering Column Jacket Assembly Rear Bracket Nuts | 22 N·m | 16 lb ft
Steering Shaft Universal Joint Pinch Bolt | 25 N·m | 18 lb ft
Steering Wheel Horn Cap Screws | 4.5 N·m | 40 lb in
Steering Wheel Nut | 38 N·m | 28 lb ft
Steering Wheel Position Sensor Screw | 2 N·m | 18 lb in
Upper and Lower Intermediate Shaft Pinch Bolt | 25 N·m | 18 lb ft
Upper and Lower Steering Column Cover Panel Screws | 2.5 N·m | 22 lb in