For 1990-2009 cars

Table 1: | Park/Neutral Position (PNP) Switch
Table 2: | Shift Program Switch
Table 3: | Transmission Connector
Table 4: | Transmission Control Module (TCM) A
Table 5: | Transmission Control Module (TCM) B
Table 6: | Transmission Control Module (TCM) C

#### Park/Neutral Position (PNP) Switch

Connector Part Information |

• | KET MG 641299

• | 10-Way F SSD & 0509 Connector (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | 439 | Ignition 1 Voltage
2 | L-GN/RD | 3011 | Park/Neutral Position (PNP) L2 Signal
3 | D-BU/RD | 3010 | Park/Neutral Position (PNP) L1 Signal
4 | RD/D-BU | 3012 | Park/Neutral Position (PNP) L3 Signal
5 | L-GN/BK | 3013 | Park/Neutral Position (PNP) L4 Signal
6 | -- | -- | Not Used
7 | PK | 839 | Ignition 1 Voltage
8 | L-GN | 24 | Backup Lamp Supply Voltage
9 | OG/BK | 434 | Automatic Transmission Shift Lock Control
10 | BK/WH | 251 | Ground

#### Shift Program Switch

Connector Part Information |

• | KET MG 610366

• | 4-Way F PCB 040 Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN/WH | 1135 | Auto Shift Lock Solenoid Supply Voltage
2 | BN/WH | 309 | Right Park Lamp Supply Voltage
3 | D-GN | 44 | Instrument Panel Lamps Dimmer Switch Signal
4 | BK | 1050 | Ground

#### Transmission Connector

Connector Part Information |

• | KOSTAL 09430010

• | 16-Way F Connector (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-BU/WH | 3006 | Automatic Transmission Output Shaft Speed (OSS) Sensor - High Signal
2 | YE/BK | 3007 | Automatic Transmission Output Shaft Speed (OSS) Sensor - Low Signal
3 | L-BU/BK | 3688 | Voltage Reference
4 | D-GN/WH | 3009 | Low Reference
5 | OG | 2020 | Voltage Reference
6 | D-GN/BK | 3021 | Pressure Control Solenoid (PCS) 3 Control
7 | BN | 3022 | Pressure Control Solenoid (PCS) 4 Control
8 | -- | -- | Not Used
9 | GY | 3008 | Transmission Fluid Temperature Sensor Signal
10 | BN/WH | 3023 | Pressure Control Solenoid (PCS) 5 Control
11 | D-GN/WH | 3024 | Pressure Control Solenoid (PCS) 6 Control
12 | WH/BK | 3025 | Shift Solenoid (SS) 1 Control
13 | WH/BN | 3026 | Shift Solenoid (SS) 2 Control
14 | -- | -- | Not Used
15 | D-BU/WH | 3005 | Automatic Transmission Input Shaft Speed (ISS) Sensor - Low Signal
16 | YE/BK | 3004 | Automatic Transmission Input Shaft Speed (ISS) Sensor - High Signal

#### Transmission Control Module (TCM) A

Connector Part Information |

• | KET MG 651804

• | 16-Way F .060-II Connector (BU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | WH/BN | 3026 | Shift Solenoid (SS) 2 Control
A2 | D-GN | 3017 | Transmission Mode Signal Power
A3 | BN | 3022 | Pressure Control Solenoid (PCS) 4 Control
A4 | GY | 3008 | Transmission Fluid Temperature Sensor Signal
A5 | L-BU | 20 | Stop Lamp Supply Voltage
A6 | YE | 1481 | Hold Mode Indicator Control
A7 | BN | 2000 | Serial Data
A8 | PU | 1807 | CAN Serial Data - High
A9 | WH/BK | 3025 | Shift Solenoid (SS) 1 Control
A10 | BN/WH | 3023 | Pressure Control Solenoid (PCS) 5 Control
A11 | D-GN/BK | 3021 | Pressure Control Solenoid (PCS) 3 Control
A12 | D-GN/WH | 3024 | Pressure Control Solenoid (PCS) 6 Control
A13-A15 | -- | -- | Not Used
A16 | YE | 710 | CAN Serial Data - Low

#### Transmission Control Module (TCM) B

Connector Part Information |

• | KET MG 651803

• | 16-Way F .060-II Connector (GN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
B1 | D-GN/WH | 3009 | Low Reference
B2 | YE/BK | 3004 | Automatic Transmission Input Shaft Speed (ISS) Sensor - High Signal
B3 | OG | 440 | Battery Positive Voltage
B4 | D-BU/WH | 3005 | Automatic Transmission Input Shaft Speed (ISS) Sensor - Low Signal
B5 | YE/BK | 3007 | Automatic Transmission Output Shaft Speed (OSS) Sensor - Low Signal
B6 | RD/D-BU | 3012 | Park/Neutral Position (PNP) Switch L3 Switch Signal
B7 | BN | 3051 | Shield Ground
BK (North America)
B8 | D-GN/WH | 817 | Vehicle Speed Signal
B9 | -- | -- | Not Used
B10 | D-BU/WH | 3006 | Automatic Transmission Output Shaft Speed (OSS) Sensor - High Signal
B11 | L-GN/BK | 3013 | Park/Neutral Position (PNP) Switch L4 Signal
B12 | BK/WH | 251 | Ground
B13 | BK/WH | 251 | Ground
B14 | -- | -- | Not Used
B15 | L-GN/RD | 3011 | Park/Neutral Position (PNP) Switch L2 Switch Signal
B16 | -- | -- | Not Used

#### Transmission Control Module (TCM) C

Connector Part Information |

• | KET MG 651802

• | 16-Way F .060-II Connector (GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
C1 | D-BU/RD | 3010 | Park/Neutral Position (PNP) Switch L1 Signal
C2-C3 | -- | -- | Not Used
C4 | D-GN/WH | 1135 | Auto Shift Lock Solenoid Supply Voltage
C5 | -- | -- | Not Used
C6 | OG | 2020 | Voltage Reference
C7 | OG | 2020 | Voltage Reference
C8 | L-BU/BK | 3688 | Voltage Reference
C9-C14 | -- | -- | Not Used
C15 | PK | 439 | Ignition 1 Voltage
C16 | PK | 439 | Ignition 1 Voltage