For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Console Armrest Screws | 1.5 N·m | 15 lb in
Console Compartment Door Hinge Screws | 1.5 N·m | 15 lb in
Hood Release Lever Screws | 2.5 N·m | 22 lb in
HVAC Upper Duct Screws | 3 N·m | 27 lb in
I/P Assembly 10 mm Screws | 9 N·m | 80 lb in
I/P Assembly Upper Nuts | 9 N·m | 80 lb in
I/P Carrier Bolts | 20 N·m | 177 lb in
I/P Carrier Lower Center Bolts | 9 N·m | 80 lb in
I/P End Cap Screw | 2.5 N·m | 22 lb in
I/P Module Opening Screw | 3 N·m | 27 lb in
I/P Storage Compartment Opening Screw | 3 N·m | 27 lb in
Knee Bolster Fastener | 9 N·m | 80 lb in
Knee Bolster Trim Panel Screw | 2.5 N·m | 22 lb in
Storage Compartment Assembly Fastener | 3 N·m | 27 lb in
Storage Compartment Door Fastener | 3 N·m | 27 lb in
Storage Compartment Latch | 3 N·m | 27 lb in