For 1990-2009 cars

### XM Activation

Important: After replacement of an XM receiver, call XM radio to deactivate the receiver that has been removed from the vehicle.

1. Turn the radio ON, tune to the XM channel 0, and record the radio ID. The radio ID will be needed for activation of the receiver.
2. From the USA, Call XM radio at 1-800-556-3600 to activate the receiver. From Canada, call 1-877-438-9677.
3. Park the vehicle outside in an area with an unobstructed view of the southern sky.
4. Leave the vehicle outside with the ignition switch in the ACC position and the radio on for 30 minutes to activate XM service.
5. Once activated, the radio will receive the remaining XM channels.