For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Actuator, Electric | 22 N·m | 16 lb ft
Brake Hose Retaining Bolt | 25 N·m | 18 lb ft
Differential Carrier Assembly Bearing Cap Bolts | 63 N·m | 46 lb ft
Differential Carrier Assembly Mounting Bracket to Carrier Bolts | 152 N·m | 112 lb ft
Differential Carrier Assembly Mounting Bracket to Frame Bolts | 152 N·m | 112 lb ft
Differential Housing Cover Bolts | 30 N·m | 22 lb ft
Intermediate Shaft Housing Assembly to Axle Housing Bolts | 60 N·m | 44 lb ft
Intermediate Shaft Housing to Disconnect Housing Bolts | 48 N·m | 35 lb ft
Pinion Shaft Lock Screw/Bolt | 25 N·m | 18 lb ft
Plug, Drain and Fill | 32 N·m | 24 lb ft
Ring Gear Bolts | 120 N·m | 89 lb ft