For 1990-2009 cars

### Removal Procedure

1. Remove the front seats. Refer to Split Bench Seat Replacement or Front Seat Replacement - Bucket .
2. Remove the rear seats, if equipped. Refer to Rear Bench Seat Replacement .
3. Remove the storage bins, if equipped. Refer to Rear Storage Compartment Replacement .
4. Remove the jack and tool storage bracket. Refer to Jack and Tool Stowage Container Bracket Replacement .
5. For extended and crew cabs, remove the jack tools from the floor.
6. Remove the floor console, if equipped. Refer to Console Replacement .
7. Remove the lower center instrument panel (I/P) trim. Refer to Instrument Panel Lower Center Trim Replacement .
8. Remove the front door sill plates. Refer to Front Side Door Sill Plate Replacement .
9. Remove the left hinge pillar trim panel. Refer to Body Hinge Pillar Trim Panel Replacement - Left Side .
10. Remove the right hinge pillar trim panel. Refer to Body Hinge Pillar Trim Panel Replacement - Right Side .
11. Remove the rear door sill plates, if equipped. Refer to Rear Side Door Sill Plate Replacement .
12. Remove the lower center pillar trim panels, if equipped. Refer to Center Pillar Lower Trim Panel Replacement .
13. Remove the body rear trim panel. Refer to Body Rear Trim Panel Replacement .
14. Remove the lower body rear corner trim panels. Refer to Body Side Rear Lower Trim Panel Replacement .
15. Remove the carpet from the vehicle.

### Installation Procedure

1. Position the carpet in the vehicle.
2. Install the lower body rear corner trim panels. Refer to Body Side Rear Lower Trim Panel Replacement .
3. Install the body rear trim panel. Refer to Body Rear Trim Panel Replacement .
4. Install the lower center pillar trim panels, if equipped. Refer to Center Pillar Lower Trim Panel Replacement .
5. Install the rear door sill plates, if equipped. Refer to Rear Side Door Sill Plate Replacement .
6. Install the left hinge pillar trim panel. Refer to Body Hinge Pillar Trim Panel Replacement - Left Side .
7. Install the right hinge pillar trim panel. Refer to Body Hinge Pillar Trim Panel Replacement - Right Side .
8. Install the front door sill plates. Refer to Front Side Door Sill Plate Replacement .
9. Install the lower center I/P trim. Refer to Instrument Panel Lower Center Trim Replacement .
10. Install the floor console, if equipped. Refer to Console Replacement .
11. For extended and crew cabs, install the jack tools to the floor.
12. Install the jack and tool storage bracket. Refer to Jack and Tool Stowage Container Bracket Replacement .
13. Install the storage bins, if equipped. Refer to Rear Storage Compartment Replacement .
14. Install the rear seats, if equipped. Refer to Rear Bench Seat Replacement .
15. Install the front seats. Refer to Split Bench Seat Replacement or Front Seat Replacement - Bucket .