For 1990-2009 cars

Connector 1: | JX105
Connector 2: | JX106

### JX105

#### Connector Part Information

- OEM: 12191928
- Service: 88986418
- Description: 12-Way F Metri-Pack 280 Series (BK) Indexing May Vary

#### Terminal Part Information

- Pins: B, H, H
- Terminal/Tray: 12110842/4
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: E, E, J
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: D, F, L, B, C, M, M
- Terminal/Tray: 12110842/4
- Core/Insulation Crimp: Pins A, D, F, L - F/G
- Core/Insulation Crimp: Pins B, C, M, M - C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### JX105

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 BK | 850 | Ground
C | 1 BK | 850 | Ground
D | 3 BK | 850 | Ground
E | 0.35 BK | 850 | Ground
E | 0.35 BK | 850 | Ground
F | 3 BK | 850 | Ground
G | -- | -- | Not Used
H | 0.35 BK | 850 | Ground
H | 0.35 BK | 850 | Ground
J | 0.35 BK | 850 | Ground (UE1)
K | -- | -- | Not Used
L | 3 BK | 850 | Ground
M | 1 BK | 850 | Ground (Crew Cab with A31)
M | 1 BK | 850 | Ground (ZQ6)

### JX106

#### Connector Part Information

- OEM: 12191928
- Service: 88986418
- Description: 12-Way F Metri-Pack 280 Series (BK) Indexing May Vary

#### Terminal Part Information

- Pins: A
- Terminal/Tray: 15324340/19
- Core/Insulation Crimp: F/G
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: B, F, G
- Terminal/Tray: 12110842/4
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: D, E, L, M, K
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: Pins D, E, L, M - C/A
- Core/Insulation Crimp: Pins K, K - E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### JX106

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 2 BK | 2050 | Ground
C | 0.8 BK | 2050 | Ground (UY7)
D | 1 BK | 2050 | Ground (A31)
E | 2 BK | 2050 | Ground (Crew Cab with A31)
F | 2 BK | 2050 | Ground
G | 2 BK | 2050 | Ground
H-J | -- | -- | Not Used
K | 0.5 BK | 2050 | Ground (4WD)
0.5 BK | 2050 | Ground (4WD)
L | 1 BK | 2050 | Ground (AG2)
M | 1 BK | 2050 | Ground (AG1)