For 1990-2009 cars

### Removal Procedure

1. Remove the accessory trim panel. Refer to Instrument Panel Accessory Trim Plate Replacement .
2. Remove the radio. Refer to Radio Replacement .
3. Lower the instrument panel (I/P) compartment door to a full down position.
4. Disconnect the radio extension antenna cable (1).
5. Remove the clip retaining the extension cable.
6. Remove the cable from the vehicle.

### Installation Procedure

1. Install the cable to the vehicle.
2. Install the clip retaining the extension cable.
3. Connect the radio extension antenna cable (1).
4. Close the I/P compartment door.
5. Install the radio. Refer to Radio Replacement .
6. Install the accessory trim panel. Refer to Instrument Panel Accessory Trim Plate Replacement .