For 1990-2009 cars

### Removal Procedure

1. Remove the windshield wiper arms. Refer to Windshield Wiper Arm Replacement .
2. Remove the air inlet grill panel push-pin retainers.
3. Disconnect the washer hose.
4. Remove the air inlet grille panel from the vehicle.

### Installation Procedure

1. Position the air inlet grille panel to the vehicle.
2. Connect the washer hose.
3. Install the push-pin retainers.
4. Install the windshield wiper arms. Refer to Windshield Wiper Arm Replacement .