For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
1-2 Shift Solenoid (1-2SS) Valve (M30) | In the automatic transmission | Powertrain Component Views | Component Connector End Views
2-3 Shift Solenoid (2-3SS) Valve (M30) | In the automatic transmission | Powertrain Component Views | Component Connector End Views
3-2 Shift Solenoid (3-2SS) Valve (M30) | In the automatic transmission | Powertrain Component Views | Component Connector End Views
A/C Compressor Clutch (C60) | Behind the A/C compressor pulley, part of the A/C compressor left front lower engine | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
A/C Refrigerant Pressure Sensor | On the high pressure hose connection to the compressor right rear of engine compartment | Powertrain Component Views | Component Connector End Views
A/T Shift Lock Control Solenoid | On lower steering column behind left knee bolster | Instrument Panel/Center Console Component Views | Component Connector End Views
Accelerator Pedal Position (APP) Sensor | On the accelerator pedal bracket behind left I/P | Instrument Panel/Center Console Component Views | Component Connector End Views
Accessory Switch | In the center of the I/P | Instrument Panel/Center Console Component Views | Component Connector End Views
Ambient Air Temperature Sensor (DF8) | Attached to the front center of the radiator support behind grille | Powertrain Component Views | Component Connector End Views
Ambient Light Sensor | In the right side of the I/P upper trim panel | Instrument Panel/Center Console Component Views | Component Connector End Views
Automatic Transmission Fluid Pressure (TFP) Manual Valve position Switch (M30) | In the automatic transmission | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Auxiliary Power Outlet 1 | In the right center of the I/P | Instrument Panel/Center Console Component Views | Component Connector End Views
Auxiliary Power Outlet 2 | In the left center of the I/P | Instrument Panel/Center Console Component Views | Component Connector End Views
Backup Lamp - Left | Left rear of vehicle | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Backup Lamp - Right | Right rear of vehicle | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Backup Lamp Switch (MA5) | Left side of the engine compartment, on top of the transmission | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Battery | Left front of the underhood compartment | Powertrain Component Views | Component Connector End Views
Blower Motor | Below the right side of the I/P near the I/P compartment | Instrument Panel/Center Console Component Views | Component Connector End Views
Blower Motor Resistor Assembly | Attached to the bottom of the blower behind right side of I/P | Instrument Panel/Center Console Component Views | Component Connector End Views
Body Control Module (BCM) | Right lower A-pillar behind right front kick panel | Instrument Panel/Center Console Component Views | Component Connector End Views
Brake Fluid Level Switch | On the left side of the brake fluid reservoir in the left rear of the engine compartment | Powertrain Component Views | Component Connector End Views
Camshaft Position (CMP) Actuator Solenoid - Bank 1 Exhaust | On the top right front of the engine | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Camshaft Position (CMP) Sensor (2.9L) | At the top front right of the engine | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Camshaft Position (CMP) Sensor 1 (3.7L) | At the top front right of the engine | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Camshaft Position (CMP) Sensor 2 (3.7L) | At the top front left of the engine | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Cargo Lamp | Mounted near the roof line at the rear of the cab | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Center High Mounted Stop Lamp (CHMSL) | Mounted near the roof line at the rear of the cab | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Clutch Position Sensor (MA5) | Mounted to the clutch pedal assembly | -- | Component Connector End Views
Courtesy Lamp - Footwell Left | Located in the left front footwell | Instrument Panel/Center Console Component Views | Component Connector End Views
Courtesy Lamp - Footwell Right | Located in the right front footwell | Instrument Panel/Center Console Component Views | Component Connector End Views
Crankshaft Position (CKP) Sensor | At the left rear of the engine block below the starter | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Cruise Control On/Off Switch (K34) | Part of the turn signal/multifunction switch | -- | Component Connector End Views
Data Link Connector (DLC) | Below the I/P left side near brake pedal | Instrument Panel/Center Console Component Views | Component Connector End Views
Digital Radio Receiver (U2K) | Behind right side of I/P above I/P compartment below passenger inflator module | Instrument Panel/Center Console Component Views | Component Connector End Views
Dome Lamp | In the center of the headliner | Passenger Compartment/Roof Component Views | Component Connector End Views
Door Jamb Switch - Driver | Inside the left front door | Passenger Compartment/Roof Component Views | Component Connector End Views
Door Jamb Switch - Front Passenger | Inside the right front door | Passenger Compartment/Roof Component Views | Component Connector End Views
Door Jamb Switch - Left Rear (Crew Cab) | Inside the left rear door | Passenger Compartment/Roof Component Views | Component Connector End Views
Door Jamb Switch - Right Rear (Crew Cab) | Inside the right rear door | Passenger Compartment/Roof Component Views | Component Connector End Views
Door Lock Actuator - Driver (AU3) | In the center rear of the driver door, near door latch | Door Component Views | Component Connector End Views
Door Lock Actuator - Front Passenger (AU3) | In the center rear of the passenger door, near door latch | Door Component Views | Component Connector End Views
Door Lock Actuator - Left Rear (Crew Cab AU3) | In the center rear of the left rear door, near door latch | Door Component Views | Component Connector End Views
Door Lock Actuator - Right Rear (Crew Cab AU3) | In the center rear of the right rear door, near door latch | Door Component Views | Component Connector End Views
Door Lock and Window Switch - Driver (A31/AU3) | Attached to the left front door accessory mount plate | Door Component Views | Component Connector End Views
Door Lock and Window Switch - Front Passenger (A31/AU3) | Attached to the right front door accessory mount plate | Door Component Views | Component Connector End Views
Electronic Brake Control Module (EBCM) | In left rear of engine compartment to the left of master cylinder | Powertrain Component Views | Component Connector End Views
Engine Control Module (ECM) | Right rear corner of the engine compartment | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Engine Coolant Temperature (ECT) Sensor | Top rear center of engine | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Engine Oil Pressure (EOP) Sensor | On the right front lower area of engine above oil filter | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Evaporative Emission (EVAP) Canister Purge Solenoid | Left side of engine below intake in back of alternator | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Evaporative Emission (EVAP) Canister Vent Solenoid | Attached to the side of the EVAP canister above spare tire | Wheels/Vehicle Underbody Component Views | Component Connector End Views
Evaporator Temperature Sensor (C60) | Behind the right lower I/P towards the left I/P compartment | Instrument Panel/Center Console Component Views | Component Connector End Views
Fog Lamp - Left Front (T96) | In the left side of the front bumper | Powertrain Component Views | Component Connector End Views
Fog Lamp - Right Front (T96) | In the right side of the front bumper | Powertrain Component Views | Component Connector End Views
Front Axle Actuator (4WD) | On the right center of the front axle housing | Wheels/Vehicle Underbody Component Views | Component Connector End Views
Fuel Injector 1 | On the left side of the engine attached to the fuel rail at the number 1 cylinder | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Fuel Injector 2 | On the left side of the engine attached to the fuel rail at the number 2 cylinder | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Fuel Injector 3 | On the left side of the engine attached to the fuel rail at the number 3 cylinder | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Fuel Injector 4 | On the left side of the engine attached to the fuel rail at the number 4 cylinder | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Fuel Injector 5 (3.7L) | On the left side of the engine attached to the fuel rail at the number 5 cylinder | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Fuel Pump and Sender Assembly | Mounted on top of the fuel tank | Wheels/Vehicle Underbody Component Views | Component Connector End Views
Fuel Tank Pressure (FTP) Sensor | At the top left rear of the fuel tank | Wheels/Vehicle Underbody Component Views | Component Connector End Views
Fuse Block - AIR Solenoid (K18) | Lower right front of the engine compartment | -- | Component Connector End Views
Fuse Block - Underhood | In the underhood compartment, above the left front wheel well | Powertrain Component Views | Electrical Center Identification Views
Generator | At the left front of the engine | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Generator Battery Control Module | Left front of the engine compartment near the battery | -- | Component Connector End Views
Hazard Switch | Center of the I/P, above the HVAC control assembly | Instrument Panel/Center Console Component Views | Component Connector End Views
Headlamp Dimmer Switch | In the turn signal/multifunction switch | -- | Component Connector End Views
Headlamp - High Beam - Left (TT5) | On the left front of vehicle | Powertrain Component Views | Component Connector End Views
Headlamp - High Beam - Right (TT5) | On the right front of vehicle | Powertrain Component Views | Component Connector End Views
Headlamp - LH (TT5) | On the left front of vehicle | Powertrain Component Views | Component Connector End Views
Headlamp - Low Beam - Left (TT5) | On the left front of vehicle | Powertrain Component Views | Component Connector End Views
Headlamp - Low Beam - Right (TT5) | On the right front of vehicle | Powertrain Component Views | Component Connector End Views
Headlamp - RH (-TT5) | On the right front of vehicle | Powertrain Component Views | Component Connector End Views
Headlamp and Panel Dimmer Switch | On the left side of the I/P | Instrument Panel/Center Console Component Views | Component Connector End Views
Heated Oxygen Sensor (HO2S) 1 | On the exhaust manifold on the right side of the engine | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Heated Oxygen Sensor (HO2S) 2 | In the exhaust pipe, adjacent to the transmission | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Heated Seat Module - Driver (KA1) | In the driver seat bottom | Passenger Compartment/Roof Component Views | Component Connector End Views
Heated Seat Module - Passenger (KA1) | In the passenger seat bottom | Passenger Compartment/Roof Component Views | Component Connector End Views
Heater Element Seat Back - Driver (KA1) | In the driver seat back | Passenger Compartment/Roof Component Views | Component Connector End Views
Heater Element Seat Back - Passenger (KA1) | In the passenger seat back | Passenger Compartment/Roof Component Views | Component Connector End Views
Heater Element Seat Cushion - Driver (KA1) | In the driver seat cushion | -- | Component Connector End Views
Heater Element Seat Cushion - Passenger (KA1) | In the passenger seat cushion | Passenger Compartment/Roof Component Views | Component Connector End Views
Horn Assembly | At the left front side of the engine compartment behind grille | Powertrain Component Views | Component Connector End Views
Horn Switch | In the steering wheel | Instrument Panel/Center Console Component Views | Component Connector End Views
HVAC Control Module | In the I/P center trim panel, beneath the radio | Instrument Panel/Center Console Component Views | Component Connector End Views
Ignition Coil 1 | In the center front of cam cover at number 1 cylinder | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Ignition Coil 2 | In the center, center of cam cover at number 2 cylinder | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Ignition Coil 3 | In the center, center of cam cover at number 3 cylinder | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Ignition Coil 4 | In the center, center of cam cover at number 4 cylinder | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Ignition Coil 5 (3.7L) | In the center rear of cam cover at number 5 cylinder | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Ignition Switch | On the right side of the steering column | Instrument Panel/Center Console Component Views | Component Connector End Views
Inflatable Restraint Front End Sensor - Left | On left underside of front frame crossmember | Powertrain Component Views | Component Connector End Views
Inflatable Restraint Front End Sensor - Right | On right underside of front frame crossmember | Powertrain Component Views | Component Connector End Views
Inflatable Restraint I/P Module | In the I/P above the I/P compartment | -- | Component Connector End Views
Inflatable Restraint Passenger Presence System (PPS) Module | Under the passenger seat on the underside of the cushion | Passenger Compartment/Roof Component Views | Component Connector End Views
Inflatable Restraint Passenger Presence System (PPS) Sensor | In the front passenger seat cushion | -- | Component Connector End Views
Inflatable Restraint Passenger Seat Belt Tension Sensor | Part of the seat belt buckle - passenger | Passenger Compartment/Roof Component Views | Component Connector End Views
Inflatable Restraint Roof Rail Module - Left (ASF) | In roof above driver door | Passenger Compartment/Roof Component Views | Component Connector End Views
Inflatable Restraint Roof Rail Module - Right (ASF) | In roof above front passenger door | Passenger Compartment/Roof Component Views | Component Connector End Views
Inflatable Restraint Seat Position Sensor (SPS) - Left | On the driver seat track | Passenger Compartment/Roof Component Views | Component Connector End Views
Inflatable Restraint Seat Position Sensor (SPS) - Right | On the passenger seat track | Passenger Compartment/Roof Component Views | Component Connector End Views
Inflatable Restraint Sensing and Diagnostic Module (SDM) | Beneath the lower console | -- | Component Connector End Views
Inflatable Restraint Side Impact Sensor (SIS) - Left (ASF) | Inside driver door | Door Component Views | Component Connector End Views
Inflatable Restraint Side Impact Sensor (SIS) - Right (ASF) | Inside passenger door | Door Component Views | Component Connector End Views
Inflatable Restraint Steering Wheel Module | In the steering column | Instrument Panel/Center Console Component Views | Component Connector End Views
Inflatable Restraint Steering Wheel Module Coil | In the steering column | -- | Component Connector End Views
Inside Rearview Mirror | Attached to the upper center of the windshield | -- | Component Connector End Views
Instrument Panel Cluster (IPC) | On the left side of the I/P above the steering column | Instrument Panel/Center Console Component Views | Component Connector End Views
Intake Air Temperature (IAT)/Mass Air Flow (MAF) Sensor | Attached to the air intake duct, front of the engine compartment | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Knock Sensor (KS) (2.9L) | Attached to the top left rear of the engine | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Knock Sensor (KS) (3.7L) | Below the intake manifold, near the front of the engine | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
License Lamp - Left | At the center of the rear bumper | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
License Lamp - Right | At the center of the rear bumper | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Longitudinal Accelerometer Sensor (4WD) | Below driver seat under carpet | Passenger Compartment/Roof Component Views | Component Connector End Views
Lumbar Adjuster/Heater Switch - Driver (AG1) | In driver seat bottom side trim panel | Door Component Views | Component Connector End Views
Lumbar Adjuster/Heater Switch - Passenger (AG2) | In passenger seat bottom side trim panel | Door Component Views | Component Connector End Views
Lumbar Pump Motor - Driver (AG1) | In driver seat bottom | Passenger Compartment/Roof Component Views | Component Connector End Views
Lumbar Pump Motor - Passenger (AG2) | In passenger seat bottom | Passenger Compartment/Roof Component Views | Component Connector End Views
Manifold Absolute Pressure (MAP) Sensor | At the top right side rear of the engine, on the intake manifold | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Outside Rearview Mirror - Driver (DE6) | Mounted on the outside of the driver door | Door Component Views | Component Connector End Views
Outside Rearview Mirror - Front Passenger (DE6) | Mounted on the outside of the front passenger door | Door Component Views | Component Connector End Views
Outside Rearview Mirror Switch (DE6) | On the interior panel of the left front door | Door Component Views | Component Connector End Views
Park Brake Switch | Left lower side of the I/P | Instrument Panel/Center Console Component Views | Component Connector End Views
Park/Neutral Position (PNP) Switch (M30) | On the lower left side of the transmission | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Park Lamp - Left Front | Left front of vehicle | Powertrain Component Views | Component Connector End Views
Park Lamp - Right Front | Right front of vehicle | Powertrain Component Views | Component Connector End Views
Park/Turn Signal Lamp - Left Front | Left front of vehicle | Powertrain Component Views | Component Connector End Views
Park/Turn Signal Lamp - Right Front | Right front of vehicle | Powertrain Component Views | Component Connector End Views
Pressure Control (PC) Solenoid Valve (M30) | In the automatic transmission | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Radio | In the center of the I/P | Instrument Panel/Center Console Component Views | Component Connector End Views
Recirculation Actuator (C60) | Above the blower motor, on the right side of the I/P carrier | Instrument Panel/Center Console Component Views | Component Connector End Views
Recliner Motor | In driver seat bottom | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Adjuster Switch - Driver (AG1) | In driver seat bottom side trim panel | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Adjuster Switch - Passenger (AG2) | In passenger seat bottom side trim panel | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Belt Buckle - Driver | Mounted to the side of the driver seat | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Belt Buckle - Passenger | Mounted to the side of the passenger seat | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Belt Pretensioner - Left Front (Regular/Crew Cab) | At the left inner B-pillar | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Belt Pretensioner - Left Front (Extended Cab) | In left rear door | Door Component Views | Component Connector End Views
Seat Belt Pretensioner - Right Front (Extended Cab) | In right rear door | Door Component Views | Component Connector End Views
Seat Belt Pretensioner - Right Front (Regular/Crew Cab) | At the right inner B-pillar | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Belt Switch - Left | Part of the seat belt buckle - driver | -- | Component Connector End Views
Seat Belt Switch - Right | Part of the seat belt buckle - passenger | -- | Component Connector End Views
Seat Circuit Breaker | In the driver seat harness, under the driver seat near X307 | -- | Component Connector End Views
Seat Motors - Driver (AG1) | In driver seat bottom | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Motors - Passenger (AG2) | In driver seat bottom | Passenger Compartment/Roof Component Views | Component Connector End Views
Seat Position Switch - Left | In driver seat track | -- | Component Connector End Views
Seat Position Switch - Right | In passenger seat track | -- | Component Connector End Views
Secondary Air Injection (AIR) Pump (3.7L K18) | Lower right front of the engine compartment | -- | Component Connector End Views
Secondary Air Injection (AIR) Pump Relay (3.7L K18) | Lower right front of the engine compartment | -- | Component Connector End Views
Secondary Air Injection (AIR) Solenoid (3.7L K18) | Upper right side of the engine | -- | Component Connector End Views
Speaker - Left Front Door | Inside left front door | Door Component Views | Component Connector End Views
Speaker - Left Front Door Tweeter (UQ2) | On the top of the left front door | Door Component Views | Component Connector End Views
Speaker - Left Rear Door (Extended/Crew Cab) | Inside the left rear door | Door Component Views | Component Connector End Views
Speaker - Right Front Door | Inside right front door | Door Component Views | Component Connector End Views
Speaker - Right Front Door Tweeter (UQ2) | On the top of the right front door | Door Component Views | Component Connector End Views
Speaker - Right Rear Door (Extended/Crew Cab) | Inside the right rear door | Door Component Views | Component Connector End Views
Starter Solenoid | Attached to the lower right rear of the engine | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Stop Lamp Switch | Above the brake pedal assembly | Instrument Panel/Center Console Component Views | Component Connector End Views
Stop Lamp - Left Rear | Left rear of vehicle | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Stop Lamp - Right Rear | Right rear of vehicle | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
TCC Brake/Cruise Release Switch | Lower left of the I/P above brake pedal | Instrument Panel/Center Console Component Views | Component Connector End Views
Throttle Body | On the left side center top of the engine | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Torque Converter Clutch (TCC) Solenoid Valve (M30) | In the automatic transmission | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Torque Converter Clutch Pulse Width Modulation (TCC PWM) Solenoid Valve (M30) | In the automatic transmission | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Trailer Lighting Converter (Trailer Accessory) | Rear of the vehicle, part of the trailer accessory harness | -- | Component Connector End Views
Trailer Connector (Trailer Accessory) | Rear of the vehicle, part of the trailer accessory harness | -- | Component Connector End Views
Transfer Case Encoder Motor (4WD) | Part of the transfer case | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Transfer Case 2/4 Wheel Indicator Switch (4WD) | Lower right side of transfer case | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Transfer Case Neutral Switch (4WD) | Upper right side of transfer case | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Transfer Case Shift Control Module (4WD) | Under driver seat carpet | -- | Component Connector End Views
Turn Signal Lamp - Left Rear | Left rear of vehicle | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Turn Signal Lamp - Right Rear | Right rear of vehicle | Luggage Compartment/Rear of Vehicle Component Views | Component Connector End Views
Turn Switch | In the turn signal/multifunction switch | -- | Component Connector End Views
Turn Signal/Multifunction Switch | On the left side of steering column | Instrument Panel/Center Console Component Views | Component Connector End Views
Vehicle Communication Interface Module (VCIM) (UE1) | Right side of I/P | Instrument Panel/Center Console Component Views | Component Connector End Views
Vehicle Speed Sensor (VSS) | Attached to the output shaft at the left rear of the transfer case | Front of Vehicle/Engine Compartment Component Views | Component Connector End Views
Window Switch - Left Rear (Crew Cab A31) | Attached to the left rear door accessory mount plate | Door Component Views | Component Connector End Views
Window Switch - Right Rear (Crew Cab A31) | Attached to the right rear door accessory mount plate | Door Component Views | Component Connector End Views
Wheel Speed Sensor (WSS) - Left Front | Attached to the left front wheel hub | Wheels/Vehicle Underbody Component Views | Component Connector End Views
Wheel Speed Sensor (WSS) - Right Front | Attached to the right front wheel hub | Wheels/Vehicle Underbody Component Views | Component Connector End Views
Window Motor - Driver (A31) | Attached to the interior of the left front door | Door Component Views | Component Connector End Views
Window Motor - Front Passenger (A31) | Attached to the interior of the right front door | Door Component Views | Component Connector End Views
Window Motor - Left Rear (Crew Cab A31) | Attached to the interior of the left rear door | Door Component Views | Component Connector End Views
Window Motor - Right Rear (Crew Cab A31) | Attached to the interior of the right rear door | Door Component Views | Component Connector End Views
Windshield Washer Fluid Pump | Mounted on the fluid reservoir in the underhood compartment right rear | Powertrain Component Views | Component Connector End Views
Windshield Wiper Motor | Under the center of the front cowling | Powertrain Component Views | Component Connector End Views
Windshield Wiper/Washer Switch | In the turn signal/multifunction switch | -- | --
X100 (4 cavities - 4WD) | Engine harness to the front axle jumper harness, in the engine compartment on right center lower wheel well | Harness Routing Views | Inline Harness Connector End Views
X101 (5 cavities - 2.9L) | Engine harness to the fuel rail harness, in the engine compartment rear center of engine | Harness Routing Views | Inline Harness Connector End Views
X101 (6 cavities - 3.7L) | Engine harness to the fuel rail harness, in the engine compartment rear center of engine | Harness Routing Views | Inline Harness Connector End Views
X102 (16 cavities) | Body harness to the chassis harness, in the engine compartment left center wheel well behind battery next to EBCM | Harness Routing Views | Inline Harness Connector End Views
X103 (2 cavities) | Forward lamp harness to body harness, front of engine compartment right front inner fender below air cleaner next to X104 | Harness Routing Views | Inline Harness Connector End Views
X104 (8 cavities) | Forward lamp harness to body harness, front of engine compartment right front inner fender below air cleaner next to X103 | Harness Routing Views | Inline Harness Connector End Views
X105 (14 cavities - 4WD) | Engine harness to the body harness, in the engine compartment left side front near battery | Harness Routing Views | Inline Harness Connector End Views
X106 (3 cavities - 2WD) | Engine harness to the body harness, in the engine compartment left side front near battery | Harness Routing Views | Inline Harness Connector End Views
X107 (3 cavities) | Forward lamp harness to front turn signal harness, behind park/turn signal lamp - right front | Harness Routing Views | Inline Harness Connector End Views
X108 (3 cavities) | Forward lamp harness to front turn signal harness, behind park/turn signal lamp - left front | Harness Routing Views | Inline Harness Connector End Views
X109 (1 cavity) | Battery harness to engine harness | Harness Routing Views | Inline Harness Connector End Views
X125 (14 cavities) | Engine harness to body harness near the fuse block - underhood | -- | Inline Harness Connector End Views
X175 (20 cavities - M30) | Engine harness to the transmission harness, right side of the transmission | Harness Routing Views | Inline Harness Connector End Views
X200 (40 cavities) | I/P harness to the body harness, behind the I/P left side above brake pedal assembly on lower A-pillar | Harness Routing Views | Inline Harness Connector End Views
X201 (22 cavities) | I/P harness to the body harness, behind right kick panel lower A-pillar | Harness Routing Views | Inline Harness Connector End Views
X202 (9 cavities - AU3) | Driver door harness to the body harness, in center of drivers front door post between door hinges next to X209 | Harness Routing Views | Inline Harness Connector End Views
X203 (10 cavities) | I/P harness to the HVAC harness, behind the I/P compartment right side of I/P clipped on HVAC case | Harness Routing Views | Inline Harness Connector End Views
X204 (22 cavities) | Steering column harness to the I/P harness, at the base of the steering column | Harness Routing Views | Inline Harness Connector End Views
X208 (4 cavities) | I/P harness to the body harness, behind the I/P left side behind knee bolster above brake pedal | Harness Routing Views | Inline Harness Connector End Views
X209 (18 cavities) | Body harness to the driver door harness, in center of driver front door post between door hinges next to X202 | Harness Routing Views | Inline Harness Connector End Views
X210 (18 cavities) | Body harness to the passenger door harness, in center of passenger front door post between door hinges next to X211 | Harness Routing Views | Inline Harness Connector End Views
X211 (9 cavities - AU3) | Passenger door harness to the body harness, in center of passenger front door post between door hinges next to X210 | Harness Routing Views | Inline Harness Connector End Views
X275 (4 cavities) | Body harness to the steering wheel harness, behind left I/P knee bolster at base of steering column near X204 | Harness Routing Views | Inline Harness Connector End Views
X307 (7 cavities - AG1) | Body harness to the driver seat harness, below the driver seat | Harness Routing Views | Inline Harness Connector End Views
X310 ( cavities) | Dome lamp harness to the body harness, in left A-pillar | Harness Routing Views | Inline Harness Connector End Views
X311 (2 cavities - Extended Cab) | Body harness to the left rear passenger door harness, in left rear passenger door | Harness Routing Views | Inline Harness Connector End Views
X312 (2 cavities - Extended Cab) | Body harness to the right rear passenger door harness, in right rear passenger door | Harness Routing Views | Inline Harness Connector End Views
X313 (12 cavities) | Body harness to passenger seat harness, under passenger seat | Harness Routing Views | Inline Harness Connector End Views
X314 (4 cavities) | Body harness to driver seat harness, under driver seat | Harness Routing Views | Inline Harness Connector End Views
X315 (5 cavities - AG2) | Body harness to the passenger seat harness, below the passenger seat | Harness Routing Views | Inline Harness Connector End Views
X316 (2 cavities - Crew Cab − A31) | Body harness to the left rear passenger door harness, in left lower B-pillar between door hinges | Harness Routing Views | Inline Harness Connector End Views
X316 (10 cavities - Crew Cab A31) | Body harness to the left rear passenger door harness, in left lower B-pillar between door hinges | Harness Routing Views | Inline Harness Connector End Views
X316 (4 cavities - Extended Cab) | Body harness to left rear passenger door harness, in left rear passenger door | Harness Routing Views | Inline Harness Connector End Views
X317 (2 cavities - Crew Cab - A31) | Body harness to the right rear passenger door harness, in right lower B-pillar between door hinges | Harness Routing Views | Inline Harness Connector End Views
X317 (10 cavities - Crew Cab A31) | Body harness to the right rear passenger door harness, in right lower B-pillar between door hinges | Harness Routing Views | Inline Harness Connector End Views
X317 (4 cavities - Extended Cab) | Body harness to right rear passenger door harness, in right rear passenger door | Harness Routing Views | Inline Harness Connector End Views
X318 (4 cavities - KA1) | Passenger seat harness to heat element, in passenger seat bottom | Harness Routing Views | Inline Harness Connector End Views
X319 (4 cavities - KA1) | Driver seat harness to heat element, in driver seat bottom | Harness Routing Views | Inline Harness Connector End Views
X320 (3 cavities) | At rear of headliner at 3rd brake light | -- | --
X400 (2 cavities) | Chassis harness to the license lamp harness, behind left license plate lamp in left side of rear bumper | Harness Routing Views | Inline Harness Connector End Views
X401 (6 cavities) (- Trailer Accessory) | Chassis harness to the left rear lamp assembly, behind left rear lamp | Harness Routing Views | Inline Harness Connector End Views
X401 (6 cavities) (Trailer Accessory | Trailer accessory harness to the left rear lamp assembly, behind left rear lamp | -- | Inline Harness Connector End Views
X402 (5 cavities) | Chassis harness to the right rear lamp assembly, behind right rear lamp | Harness Routing Views | Inline Harness Connector End Views
X403 (6 cavities) (Trailer Accessory | Chassis harness to the trailer accessory harness, behind left rear tail lamp | -- | Inline Harness Connector End Views
G100 | In the engine compartment on lower left side of engine block | Harness Routing Views | --
G101 | In the engine compartment on lower left side of engine block | Harness Routing Views | --
G102 | In the engine compartment on lower left side of engine block | Harness Routing Views | --
G103 | In the engine compartment on lower left side of engine block | Harness Routing Views | --
G104 | In the engine compartment on left inner front wheel well behind battery | Harness Routing Views | --
G105 | Ground splice pack in the engine compartment - left side inner fender near EBCM | Harness Routing Views | --
G106 | Ground splice pack in the engine compartment - right side inner fender behind air cleaner | Harness Routing Views | --
G300 | In the driver compartment under driver seat carpet on floor board | Harness Routing Views | --
G301 | In the passenger compartment under passenger seat carpet on floor board | Harness Routing Views | --
G302 | In the passenger compartment under center console near SDM | Harness Routing Views | --
J100 | (CKT 20) Body harness, approximately 14.5 cm (5.8 in) from the breakout to the accelerator pedal position (APP) switch | Harness Routing Views | --
J101 | (CKT 1) Battery Harness | Harness Routing Views | --
J102 | (CKT 24) Body harness, approximately 8 cm (3.2 in) from the breakout to the accelerator pedal position (APP) switch | Harness Routing Views | --
J103 (3.7L) | (CKT 439) Fuel injector harness, approximately 5 cm (2 in) from the breakout to fuel injector - 4 | -- | --
J104 (2.9L) | (CKT 839) Fuel injector harness, approximately 4 cm (1.6 in) from the breakout to fuel injector - 4 | -- | --
J105 | (CKT 414) In the engine harness approximately 24 cm (9.4 in) before the generator battery control module breakout | -- | --
J133 (M30) | (CKT 839) In the automatic transmission harness | -- | --
J200 | (CKT 2050) I/P harness, approximately 6 cm (2.4 in) from the breakout to the instrument panel cluster (IPC) | -- | --
J201 | (CKT 1151) I/P harness, approximately 7 cm (2.8 in) from the breakout to X204 | -- | --
J202 | (CKT 52) HVAC harness, approximately 14 cm (5.6 in) from the breakout to the recirculation actuator towards the blower motor resistor assembly | Harness Routing Views | --
J300 (Crew Cab) | (CKT 141) Body harness, approximately 5 cm (2 in) from the breakout to G300 | Harness Routing Views | --
J301 (AG1/AG2) | (CKT 2240) Body harness, approximately 12 cm (4.8 in) from the breakout to X314 | Harness Routing Views | --
J302 (Crew Cab A31) | (CKT 443) Body harness, approximately 4 cm (1.6 in) from the breakout to the accelerator pedal position (APP) switch | Harness Routing Views | --
J303 | (CKT 1151) Body harness, approximately 6 cm (2.4 in) from the breakout to X202, X208, X209 | Harness Routing Views | --
J304 | (CKT 1151) Body harness, approximately 91 cm (36.4 in) from the breakout to the accelerator pedal position (APP) switch towards the main harness | Harness Routing Views | --
J306 (AG1) | (CKT 2050) Driver seat harness, approximately 5 cm (2 in) from the breakout to X319 | -- | --
J307 (Crew Cab) | (CKT 1307) Body harness, approximately 4 cm (1.6 in) from the breakout to the accelerator pedal position (APP) switch | Harness Routing Views | --
J308 (Crew Cab A31) | (CKT 294) Body harness, approximately 10.5 cm (4.2 in) from the breakout to the accelerator pedal position (APP) switch | Harness Routing Views | --
J309 (Crew Cab A31) | (CKT 295) Body harness, approximately 17 cm (6.8 in) from the breakout to the accelerator pedal position (APP) switch | Harness Routing Views | --
J310 | (CKT 2759) Chassis harness, approximately 39 cm (15.6 in) before the fuel pump and sender assembly | Harness Routing Views | --
J311 | (CKT 407) Body harness, approximately 24.5 cm (9.8 in) from the breakout to G302 away from X313 | Harness Routing Views | --
J312 (AG1/AG2) | (CKT 1040) Driver seat harness, approximately 12.5 cm (5 in) from the breakout to X319 | -- | --
J313 (AG2) | (CKT 2240) Passenger seat harness, approximately 12.5 cm (5 in) from the breakout to X318 | -- | --
J314 (AG2) | (CKT 2050) Passenger seat harness, approximately 5 cm (2 in) from the breakout to X319 | -- | --
J315 (AG1) | (CKT RD) Heater element harness - driver | -- | --
J316 (AG2) | (CKT WH) Heater element harness - passenger | -- | --
J317 (AG2) | (CKT BK) Heater element harness - passenger | -- | --
J318 (AG2) | (CKT BK, BK/RD) Heater element harness - passenger | -- | --
J319 (AG2) | (CKT RD) Heater element harness - passenger | -- | --
J320 (AG1) | (CKT WH) Heater element harness - driver | -- | --
J321 (AG1) | (CKT BK) Heater element harness - driver | -- | --
J322 (AG1) | (CKT BK, BK/RD) Heater element harness - driver | -- | --
J400 | (CKT 9) Chassis harness, approximately 40.5 cm (16.2 in) from the breakout to the fuel pump and sender assembly toward the evaporative emission (EVAP) canister purge solenoid | Harness Routing Views | --
J401 | (CKT 850) Chassis harness, approximately 21 cm (8.4 in) from the breakout to the fuel pump and sender assembly toward the evaporative emission (EVAP) canister purge solenoid | Harness Routing Views | --
J402 | (CKT 19) Chassis harness, approximately 13 cm (5.2 in) from the breakout to X401 and X402 | Harness Routing Views | --
J403 | (CKT 20) Chassis harness, approximately 14 cm (5.6 in) from the main harness on the breakout to X401 and X402 | Harness Routing Views | --
J404 | (CKT 24) Chassis harness, approximately 75.5 cm (30.2 in) before X402 | Harness Routing Views | --
J405 (Trailer Accessory) | Trailer accessory harness, between the left rear tail lamp connector and the trailer lighting converter | -- | --
J406 (Trailer Accessory) | Trailer accessory harness, between the left rear tail lamp connector and the trailer lighting converter | -- | --
J407 (Trailer Accessory) | Trailer accessory harness, between the left rear tail lamp connector and the trailer lighting converter | -- | --
J408 (Trailer Accessory) | Trailer accessory harness, between the left rear tail lamp connector and the trailer lighting converter | -- | --
J409 (Trailer Accessory) | Trailer accessory harness, between the left rear tail lamp connector and the trailer lighting converter | -- | --
J500 | (CKT 850) Driver door harness, approximately 5 cm (2 in) from the breakout to the speaker - left front door tweeter | Harness Routing Views | --
J900 | (CKT 9) License lamp harness, approximately 44.5 cm (17.8 in) before the license lamp - RH | Harness Routing Views | --
J901 | (CKT 850) License lamp harness, approximately 24 cm (9.6 in) from the breakout to X400 towards the license lamp - RH | Harness Routing Views | --
JX105 | In the engine compartment on left inner front fender near EBCM | Harness Routing Views | Splice Pack Connector End Views
JX106 | In the engine compartment on right inner front fender behind air cleaner | Harness Routing Views | Splice Pack Connector End Views