For 1990-2009 cars

Figure 1: |

#### Left Side of the Engine Components (2.9L)

(1) | Manifold Absolute Pressure (MAP) Sensor
(2) | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
(3) | Knock Sensor (KS)
(4) | Starter
(5) | Crankshaft Position (CKP) Sensor
(6) | G102
(7) | G103
(8) | G101
(9) | A/C Compressor Clutch (C60)
(10) | Engine Block Heater (K05)
(11) | Generator

Figure 2: |

#### Top of the Engine Components (2.9L)

(1) | Manifold Absolute Pressure (MAP) Sensor
(2) | Throttle Body
(3) | Camshaft Position (CMP) Sensor
(4) | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Exhaust
(5) | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor
(6) | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor Connector

Figure 3: |

#### Right Side of the Engine Components (2.9L)

(1) | Ignition Coil 4
(2) | Fuel Injector 4
(3) | Ignition Coil 3
(4) | Fuel Injector 3
(5) | Ignition Coil 2
(6) | Fuel Injector 2
(7) | Fuel Injector 1
(8) | Ignition Coil 1
(9) | Engine Oil Pressure (EOP) Switch
(10) | Heated Oxygen Sensor (HO2S) 1
(11) | Heated Oxygen Sensor (HO2S) 1 Connector
(12) | Engine Coolant Temperature (ECT) Sensor

Figure 4: |

#### Left Side of the Engine Components (3.7L)

(1) | Starter
(2) | Knock Sensor (KS)
(3) | Crankshaft Position (CKP) Sensor
(4) | G102
(5) | G103
(6) | G101
(7) | A/C Compressor Clutch (C60)
(8) | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
(9) | Generator

Figure 5: |

#### Top of the Engine Components (3.7L)

(1) | Manifold Absolute Pressure (MAP) Sensor
(2) | Throttle Body
(3) | Camshaft Position (CMP) Sensor 2
(4) | Camshaft Position (CMP) Sensor 1
(5) | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Exhaust
(6) | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor
(7) | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor Connector

Figure 6: |

#### Right Side of the Engine Components (3.7L)

(1) | Fuel Injector 5
(2) | Ignition Coil 5
(3) | Fuel Injector 4
(4) | Ignition Coil 4
(5) | Fuel Injector 3
(6) | Ignition Coil 3
(7) | Fuel Injector 2
(8) | Ignition Coil 2
(9) | Fuel Injector 1
(10) | Ignition Coil 1
(11) | Engine Oil Pressure (EOP) Switch
(12) | Heated Oxygen Sensor (HO2S) 1
(13) | Engine Coolant Temperature (ECT) Sensor Connector

Figure 7: |

#### Engine - Front (LH8)

(1) | Throttle Body
(2) | Camshaft Position (CMP) Sensor

Figure 8: |

#### Engine - Left (LH8)

(1) | Engine Coolant Temperature (ECT) Sensor
(2) | Generator
(3) | Ignition Coil 1
(4) | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
(5) | Ignition Coil 3
(6) | Ignition Coil 5
(7) | Ignition Coil 7
(8) | Engine Oil Pressure (EOP) Sensor
(9) | Park/Neutral Position (PNP) Switch (M30)
(10) | Knock Sensor (KS) 1
(11) | Engine Block Heater Connector (K05)

Figure 9: |

#### Engine - Right Side (LH8)

(1) | Crankshaft Position (CKP) Sensor
(2) | Ignition Coil 8
(3) | Ignition Coil 6
(4) | Ignition Coil 4
(5) | Manifold Absolute Pressure (MAP) Sensor
(6) | Ignition Coil 2
(7) | A/C Compressor Clutch
(8) | Knock Sensor (KS) 2
(9) | Starter Motor

Figure 10: |

#### Engine - Top View (LH8)

(1) | Fuel Injector 2
(2) | Fuel Injector 4
(3) | Fuel Injector 6
(4) | Fuel Injector 8
(5) | Fuel Injector 7
(6) | Fuel Injector 5
(7) | Fuel Injector 3
(8) | Fuel Injector 1

Figure 11: |

#### Left Side of the Transmission Components (M30)

(1) | Automatic Transmission
(2) | Park/Neutral Position (PNP) Switch

Figure 12: |

#### Left Side of the Transmission Components (MA5)

(1) | Vehicle Speed Sensor (VSS)

Figure 13: |

#### Right Side of the Transmission Components (MA5)

(1) | Backup Lamp Switch

Figure 14: |

#### Inside the Transmission Components (M30)

(36) | Vehicle Speed Sensor (VSS)
(66) | Torque Converter Clutch (TCC) Solenoid Valve
(69) | Automatic Transmission Fluid Pressure (TFP) Manual Valve Position Switch
(367a) | 1-2 Shift Solenoid (SS) Valve
(367b) | 2-3 Shift Solenoid (SS) Valve
(377) | Pressure Control (PC) Solenoid Valve
(394) | 3-2 Shift Solenoid (3-2 SS) Valve Assembly
(396) | Torque Converter Clutch (TCC) Pulse Width Modulation (PWM) Solenoid Valve

Figure 15: |

#### Rear of the Transmission Components

(1) | Park/Neutral Position (PNP) Switch (M30)
(2) | Heated Oxygen Sensor (HO2S) 2
(3) | Vehicle Speed Sensor (VSS)
(4) | Transfer Case Neutral Switch (4WD)
(5) | Transfer Case 2/4 Wheel Indicator Switch (4WD)
(6) | Transfer Case Encoder Motor (4WD)
(7) | Transfer Case