For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Conditioning (A/C) Condenser to Radiator Bolt | 28 N·m | 21 lb ft
Coolant Heater | 50 N·m | 37 lb ft
Coolant Recovery Reservoir Bolt (at Wheelhouse Panel) | 12 N·m | 106 lb in
Coolant Recovery Reservoir Bolt (to Bracket) | 10 N·m | 89 lb in
Fan Blade Bolt | 27 N·m | 20 lb ft
Fan Clutch Nut | 56 N·m | 41 lb ft
Radiator Mounting Bracket Bolt | 28 N·m | 21 lb ft
Thermostat Housing Bolt | 10 N·m | 89 lb in
Water Outlet Housing Bolt | 10 N·m | 89 lb in
Water Pump Bolt | 10 N·m | 89 lb in
Water Pump Pulley Bolt | 25 N·m | 18 lb ft