For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Differential Drive Pinion and Ring Gear Backlash | 0.08-0.25 mm | 0.003-0.010 in
Differential Drive Pinion and Ring Gear Backlash - Preferred | 0.13-0.18 mm | 0.005-0.007 in
Pinion Bearing Preload - New Bearings | 1.7-3.4 N·m | 15-30 lb in
Pinion Bearing Preload - Used Bearings | 1.1-2.3 N·m | 10-20 lb in
Pinion and Differential Case Bearing Preload - New Bearings | 3.4-6.2 N·m | 30-55 lb in
Pinion and Differential Case Bearing Preload - Used Bearings | 2.8-5.1 N·m | 25-45 lb in