For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Door Lock Switch Plate Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Door Lock Switch Plate Retainer
3 | Door Lock Switch Plate Assembly Tip Disconnect the electrical connector.
4 | Front Door Window Switch Screw (Qty: 2) Tighten 2 N·m (18 lb in)
5 | Front Door Window Switch Assembly