For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor Mounting Bolt | 50 N·m | 37 lb ft
A/C Evaporator and Blower Module Shield Screws | 2.2 N·m | 19 lb in
A/C Refrigerant Pressure Sensor | 4.8 N·m | 42 lb in
Air Distributor Duct Mounting Screw | 1.9 N·m | 17 lb in
Air Inlet Assembly Mounting Stud | 4.5 N·m | 40 lb in
Air Outlet Assembly Retaining Screw | 2.5 N·m | 22 lb in
Blower Motor and Fan Assembly Mounting Screw | 1.9 N·m | 17 lb in
Blower Motor Relay Bracket Mounting Screw | 1.9 N·m | 17 lb in
Blower Motor Resistor Mounting Screw | 1.9 N·m | 17 lb in
Compressor Discharge Hose to Condenser Fitting | 28 N·m | 21 lb ft
Compressor Pressure Relief Valve | 9 N·m | 80 lb in
Compressor Suction and Discharge Hose to Compressor | 33 N·m | 24 lb ft
Compressor Suction Hose to TXV | 48 N·m | 35 lb ft
Condenser Insulator Retaining Screw | 1.9 N·m | 17 lb in
Evaporator Case Section to Blower Case Section Retaining Screw | 1.9 N·m | 17 lb in
Evaporator Tube to Condenser Fitting | 10 N·m | 2.25 lb ft
Floor Air Outlet Mounting Screw | 1.9 N·m | 17 lb in
Heater Core Access Cover Screw | 1.9 N·m | 17 lb in
Heater Inlet and Outlet Hoses Bracket Bolt | 25 N·m | 18 lb ft
Heater Inlet Hose Fitting at Intake Manifold | 23.5 N·m | 17 lb ft
Heater Outlet Hose Bracket Bolt | 25 N·m | 18 lb ft
Heater/Vent Module Mounting Nut | 4.5 N·m | 40 lb in
Heater/Vent Module Mounting Screw | 4.5 N·m | 40 lb in
Heater/Vent Module Mounting Stud | 4.5 N·m | 40 lb in
Intermediate Bracket Bolts | 10 N·m | 88 lb in
Knee Bolster Bracket Nuts | 5.5 N·m | 49 lb in
Receiver Drier Clamp Screw | 10 N·m | 88 lb in