For 1990-2009 cars

#### Range Reference Table

Range | Park | Reverse | Neutral | OD | D | 2 | 1
--- | --- | --- | --- | --- | --- | --- | ---
Gear |  |  |  | 1st | 2nd | 3rd | 4th | 1st | 2nd | 3rd | 1st** | 2nd | 1st | 2nd***
1-2 Shift Solenoid | ON* | ON* | ON* | ON | OFF | OFF | ON | ON | OFF | OFF | ON | OFF | ON | OFF
2-3 Shift Solenoid | ON* | ON* | ON* | ON | ON | OFF | OFF | ON | ON | OFF | ON | ON | ON | ON
2-4 Band | -- | -- | -- | -- | A | -- | A | -- | A | -- | -- | A | -- | A
Reverse Input Clutch | -- | A | -- | -- | -- | -- | -- | -- | -- | -- | -- | -- | -- | --
Overrun Clutch | -- | -- | -- | -- | -- | -- | -- | -- | -- | A | A | A | A | A
Forward Clutch | -- | -- | -- | A | A | A | A | A | A | A | A | A | A | A
Forward Sprag Clutch Assembly | -- | -- | -- | H | H | H | -- | H | H | H | H | H | H | H
3-4 Clutch | -- | -- | -- | -- | -- | A | A | -- | -- | A | -- | -- | -- | --
Lo/Roller Clutch | -- | -- | -- | H | -- | -- | -- | H | -- | -- | H | -- | H | --
Lo/Rev Clutch | A | A | -- | -- | -- | -- | -- | -- | -- | -- | -- | -- | A | --

- A = Applied
- H = Holding
- ON = The solenoid is energized.
- OFF = The solenoid is de-energized.
- *Shift Solenoid state is a function of vehicle speed and may change if the vehicle speed increases sufficiently in Park, Reverse or Neutral. However, this does not affect the operation of the transmission.
- **Manual Second-First gear is electronically prevented under normal operating conditions.
- ***Manual First-Second gear is only available above approximately 48-56 km/h (30-35 mph).