For 1990-2009 cars

### Removal Procedure

1. Remove the bolt securing the child seat restraint bracket to the vehicle.
2. Remove the child seat restraint bracket from the vehicle.

### Installation Procedure

1. Position the child seat restraint bracket by hooking the 2 tabs on the rear of the bracket into the slots in the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolt which retains the child seat restraint bracket to the vehicle.

Tighten
Tighten the child seat restraint bracket bolt to 52.5 N·m (39 lb ft).