For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Backing Plate Bolt | 135 N·m | 100 lb ft
Bearing Cap Bolts | 75 N·m | 55 lb ft
Brake Junction Block Retaining Bolt | 20 N·m | 15 lb ft
Brake Line Retaining Bolts | 20 N·m | 15 lb ft
Differential Housing Cover Bolts | 30 N·m | 20 lb ft
Fill Plug | 33 N·m | 24 lb ft
Pinion Shaft Lock Bolt | 25 N·m | 18 lb ft
Propeller Shaft U-Bolts | 76 N·m | 56 lb ft
Ring Gear Bolts | 120 N·m | 89 lb ft
Shock Absorber Bolts | 95 N·m | 70 lb ft