For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Linear Shift Assembly Bolt | 10 N·m | 89 lb in
Lower Intermediate Steering Shaft Bolt | 45 N·m | 33 lb ft
Lower Steering Column Trim Cover Bolt | 3 N·m | 27 lb in
Multifunction Turn Signal Switch Housing Bolt | 2.5 N·m | 22 lb in
Shift Lever Bolt | 20 N·m | 15 lb ft
Steering Column Bolt | 27 N·m | 20 lb ft
Steering Column Jacket Bolt | 17 N·m | 13 lb ft
Steering Column Nut | 30 N·m | 22 lb ft
Steering Wheel Nut | 35 N·m | 26 lb ft
Tilt Lever Bolt | 1 N·m | 9 lb in
Turn Signal Multifunction Switch Bolt | 7 N·m | 62 lb in
Upper Intermediate Steering Shaft Bolt (at the lower intermediate steering shaft) | 23 N·m | 17 lb ft
Upper Intermediate Steering Shaft Bolt (at the steering column) | 47 N·m | 35 lb ft