For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Endgate Handle Bolts | 9 N·m | 80 lb in
Endgate Latch Bolts | 25 N·m | 18 lb ft
Endgate Striker Bolts | 25 N·m | 18 lb ft
Endgate Handle Lock Cylinder Bolts | 9 N·m | 80 lb in
Front Door Latch Bolts | 9 N·m | 80 lb in
Front Door Latch Screws | 7 N·m | 62 lb in
Front Door Switch Plate Screws | 2 N·m | 18 lb in
Front Door Outside Handle Bolts | 9 N·m | 80 lb in
Front Door Outside Handle Cylinder Bolt | 9 N·m | 80 lb in
Front Door Striker Screws | 25 N·m | 18 lb ft
Rear Door Latch Bolts | 9 N·m | 80 lb in
Rear Door Latch Screws | 7 N·m | 62 lb in
Rear Outside Access Door Latch | 9 N·m | 80 lb in
Rear Outside Door Handle Bolts | 9 N·m | 80 lb in
Rear Side Access Door Lower Latch Nuts | 9 N·m | 80 lb in
Rear Side Access Door Lower Latch Bolts | 9 N·m | 80 lb in
Rear Side Access Door Lower Latch Bolts | 9 N·m | 80 lb in
Rear Side Access Door Lower Striker Bolts | 25 N·m | 18 lb ft
Rear Side Access Door Upper Striker Bolts | 25 N·m | 18 lb ft