For 1990-2009 cars

Connector 1: | Door Lock Actuator - Driver w/AU3
Connector 2: | Door Lock Actuator - Front Passenger w/AU3
Connector 3: | Door Lock Actuator - Left Rear (Crew Cab) w/AU3
Connector 4: | Door Lock Actuator - RIght Rear (Crew Cab) w/AU3
Connector 5: | Door Lock and Window Switch - Driver C1 w/A31 or AU3
Connector 6: | Door Lock and Window Switch - Driver C2 w/A31 or AU3
Connector 7: | Door Lock and Window Switch - Front Passenger w/A31 or AU3

### Door Lock Actuator - Driver w/AU3

#### Connector Part Information

- OEM: 15383439
- Service: 89046646
- Description: 2-Way F 090 II Sealed (WH)

#### Terminal Part Information

- Terminal/Tray: 8100-0461/6
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Door Lock Actuator - Driver w/AU3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | TN | 694 | Door Lock Actuator Unlock Control
2 | GY | 295 | Door Lock Actuator Lock Control

### Door Lock Actuator - Front Passenger w/AU3

#### Connector Part Information

- OEM: 15383439
- Service: 89046646
- Description: 2-Way F 090 II Sealed (WH)

#### Terminal Part Information

- Terminal/Tray: 8100-0461/6
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Door Lock Actuator - Front Passenger w/AU3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | TN | 294 | Door Lock Actuator Unlock Control
2 | GY | 295 | Door Lock Actuator Lock Control

### Door Lock Actuator - Left Rear (Crew Cab) w/AU3

#### Connector Part Information

- OEM: 15383439
- Service: 89046646
- Description: 2-Way F 090 II Sealed (WH)

#### Terminal Part Information

- Terminal/Tray: 8100-0461/6
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Door Lock Actuator - Left Rear (Crew Cab) w/AU3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | TN | 294 | Door Lock Actuator Unlock Control
2 | GY | 295 | Door Lock Actuator Lock Control

### Door Lock Actuator - RIght Rear (Crew Cab) w/AU3

#### Connector Part Information

- OEM: 15383439
- Service: 89046646
- Description: 2-Way F 090 II Sealed (WH)

#### Terminal Part Information

- Terminal/Tray: 8100-0461/6
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Door Lock Actuator - Right Rear (Crew Cab) w/AU3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | TN | 294 | Door Lock Actuator Unlock Control
2 | GY | 295 | Door Lock Actuator Lock Control

### Door Lock and Window Switch - Driver C1 w/A31 or AU3

#### Connector Part Information

- OEM: 12105465
- Service: 88987940
- Description: 8-Way F 090 II (WH

#### Terminal Part Information

- Pins: 1, 2, 3, 4, 5, 6, 7, 8
- Terminal/Tray: 12129960/19
- Core/Insulation Crimp: Pins 1, 2, 3, 4, 5 - C/A
- Core/Insulation Crimp: Pins 6, 7, 8 - See Terminal Repair Kit
- Release Tool/Test Probe: 12094429/J-35616-18 (BK)

#### Door Lock and Window Switch - Driver C1 w/A31 or AU3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 1240 | Battery Positive Voltage
2 | TN | 694 | Driver Door Lock Actuator Unlock Control
3 | BK | 850 | Ground
4 | GY | 295 | Door Lock Actuator Lock Control
5 | TN | 294 | Door Lock Actuator Unlock Control
6 | YE | 443 | Accessory Voltage
7 | D-BU | 164 | Power Window Motor Left Front Up Control
8 | BN | 165 | Power Window Motor Left Front Down Control

### Door Lock and Window Switch - Driver C2 w/A31 or AU3

#### Connector Part Information

- OEM: 15380363
- Service: 15380363
- Description: 14-Way F 040 III (WH)

#### Terminal Part Information

- Pins: 1, 2, 4, 5, 6, 7, 8, 9, 11, 12, 13
- Terminal/Tray: 15355438/20
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-12 (BU)

#### Door Lock and Window Switch - Driver C2 w/A31 or AU3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-BU | 1307 | Power Window Master Switch Lockout Signal
2 | BN | 9 | Park Lamp Supply Voltage
3 | -- | -- | Not Used
4 | PU | 171 | Power Window Master Switch Right Rear Down Signal
5 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal
6 | D-BU | 245 | Passenger Door Lock Switch Unlock Control
7 | L-BU | 244 | Passenger Door Lock Switch Lock Control
8 | L-BU | 166 | Power Window Master Switch Right Front Up Signal
9 | TN | 167 | Power Window Master Switch Right Front Down Signal
10 | -- | -- | Not Used
11 | YE | 1187 | Power Window Master Switch Left Rear Down Signal
12 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal
13 | WH | 194 | Door Unlock Control
14 | -- | -- | Not Used

### Door Lock and Window Switch - Front Passenger w/A31 or AU3

#### Connector Part Information

- OEM: 15383359
- Service: 15383359
- Description: 12-Way F 090 II (WH)

#### Terminal Part Information

- Pins: 3, 4, 6, 7, 8, 9, 10, 11, 12, 5
- Terminal/Tray: 12129960/19
- Core/Insulation Crimp: Pins 3, 4, 6, 7, 8, 9, 10, 11, 12 - See Terminal Repair Kit
- Core/Insulation Crimp: Pins 5 - C/A
- Release Tool/Test Probe: 12094429/J-35616-18 (BK)

#### Door Lock and Window Switch - Front Passenger w/A31 or AU3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | D-BU | 245 | Passenger Door Lock Switch Unlock Control
4 | L-BU | 244 | Passenger Door Lock Switch Lock Control
5 | BK | 2050 | Ground
6 | BN | 9 | Park Lamp Supply Voltage
7 | D-BU | 1307 | Power Window Master Switch Lockout Signal
8 | TN | 167 | Power Window Master Switch Right Front Down Signal
9 | L-BU | 166 | Power Window Master Switch Right Front Up Signal
10 | BN | 667 | Power Window Motor Right Front Down Control
11 | YE | 443 | Accessory Voltage
12 | D-BU | 666 | Power Window Motor Right Front Up Control