For 1990-2009 cars

Figure 1: |

#### LR of the Engine Compartment

(1) | G104
(2) | Starter
(3) | Generator Positive Voltage Connector
(4) | Battery
(5) | G100
(6) | Fuse Block-Underhood
(7) | Ring Terminal Battery
(8) | Ring Terminal Generator
(9) | Battery Positive Terminal
(10) | Generator

Figure 2: |

#### Engine Compartment (2.8L)

(1) | Powertrain Control Module (PCM) C2
(2) | Powertrain Control Module (PCM) C3
(3) | Throttle Body
(4) | Manifold Absolute Pressure (MAP) Sensor
(5) | Evaporative Emission (EVAP) Canister Purge Solenoid
(6) | Knock Sensor (KS)
(7) | Generator
(8) | Crankshaft Position (CKP) Sensor
(9) | C105 (4WD) or C106 (2WD) (Engine Harness to Body Harness)
(10) | Fuse Block - Underhood C2
(11) | A/C Compressor Clutch (C60)
(12) | G101
(13) | G103
(14) | G102
(15) | Engine Oil Pressure (EOP) Sensor
(16) | Camshaft Position (CMP) Sensor
(17) | C100 (4WD) (Engine Harness to Front Axle Jumper Harness)
(18) | Camshaft Position (CMP) Actuator Solenoid - Bank 1 Exhaust
(19) | Intake Air Temperature (IAT)/Mass Air Flow (MAF) Sensor

Figure 3: |

#### Engine Compartment (3.5L)

(1) | Powertrain Control Module (PCM) C2
(2) | Powertrain Control Module (PCM) C3
(3) | Throttle Body
(4) | Manifold Absolute Pressure (MAP) Sensor
(5) | Evaporative Emission (EVAP) Canister Purge Solenoid
(6) | Knock Sensor (KS) 2
(7) | Generator
(8) | C105 (4WD) or C106 (2WD) (Engine Harness to Body Harness)
(9) | Fuse Block - Underhood C2
(10) | Camshaft Position (CMP) Sensor 2
(11) | Crankshaft Position (CKP) Sensor
(12) | A/C Compressor Clutch
(13) | Knock Sensor (KS) 1
(14) | G101
(15) | G103
(16) | G102
(17) | Engine Oil Pressure (EOP) Sensor
(18) | Camshaft Position Sensor 1
(19) | C100 (4WD) (Engine Harness to Front Axle Jumper Harness)
(20) | Camshaft Position (CMP) Actuator Solenoid - Bank 1 Exhaust
(21) | Intake Air Temperature (IAT)/Mass Air Flow (MAF) Sensor

Figure 4: |

#### Left and Right Sides of Engine Compartment

(1) | Wheel Speed Sensor (WSS) - LF
(2) | Brake Fluid Level Switch
(3) | Windshield Wiper Motor
(4) | Pass-through Grommet
(5) | Electronic Brake Control Module (EBCM)
(6) | Splice Pack SP105/G105
(7) | C102 (Body Harness to Chassis Harness)
(8) | C105 (4WD) or C106 (2WD) (Engine Harness to Body Harness)
(9) | Fuse Block - Underhood C4
(10) | Fuse Block - Underhood C5
(11) | Fuse Block - Underhood C7
(12) | Fuse Block - Underhood C6
(13) | C104 (Forward Lamp Harness to Body Harness) and C103 (Forward Lamp Harness to Body Harness)
(14) | Splice Pack SP106/G106
(15) | Wheel Speed Sensor (WSS) - RF
(16) | Powertrain Control Module (PCM) C1
(17) | Windshield Washer Fluid Pump
(18) | Pass-through Grommet
(19) | A/C Refrigerant Pressure Sensor

Figure 5: |

#### Passenger Compartment (Regular Cab)

(1) | Body Control Module (BCM) C1
(2) | C201 (I/P Harness to Body Harness)
(3) | G301
(4) | G302
(5) | Cargo Lamp/Center High Mounted Stop Lamp (CHMSL)
(6) | Door Jamb Switch - Front Passenger
(7) | C313 (Body Harness to Passenger Seat Harness)
(8) | Seat Belt Pretensioner - RF
(9) | Inflatable Restraint Sensing and Diagnostic Module (SDM)
(10) | Transfer Case Shift Control Module
(11) | C314 (Body Harness to Driver Seat Harness)
(12) | G Sensor
(13) | Seat Belt Pretensioner - LF
(14) | Door Jamb Switch - Driver
(15) | G300
(16) | Stop Lamp Switch
(17) | TCC Brake/Cruise Release Switch
(18) | Park Brake Switch
(19) | S303
(20) | Clutch Switch
(21) | Clutch Start Switch
(22) | C208 (I/P Harness to Body Harness)
(23) | C202 (Driver Door Harness to Body Harness)
(24) | C209 (Body Harness to Driver Door Harness)
(25) | C200 (I/P Harness to Body Harness)
(26) | C275 (Body Harness to Steering Wheel Harness)
(27) | Inflatable Restraint Roof Rail Module - Left
(28) | Accelerator Pedal Position (APP) Sensor
(29) | C310 (Dome Lamp Harness to Body Harness)
(30) | C210 and C211 (A31) (Body Harness to Passenger Door Harness)
(31) | Inflatable Restraint Roof Rail Module - Right
(32) | Inside Rearview Mirror

Figure 6: |

#### Passenger Compartment (Extended Cab)

(1) | C310 (Dome Lamp Harness to Body Harness)
(2) | C201 (I/P Harness to Body Harness)
(3) | G301
(4) | G302
(5) | Inflatable Restraint Sensing and Diagnostic Module (SDM)
(6) | C313 (Body Harness to Passenger Seat Harness)
(7) | C317 (Body Harness to RR Passenger Door Harness)
(8) | C312 (Body Harness to RR Passenger Door Harness)
(9) | Cargo Lamp/Center High Mounted Stop Lamp (CHMSL)
(10) | C316 (Body Harness to LR Passenger Door Harness)
(11) | C311 (Body Harness to LR Passenger Door Harness)
(12) | C314 (Body Harness to Driver Seat Harness)
(13) | Transfer Case Shift Control Module C1
(14) | Transfer Case Shift Control Module C2
(15) | G Sensor
(16) | G300
(17) | Accelerator Pedal Position (APP) Sensor
(18) | S102
(19) | S100
(20) | Stop Lamp Switch
(21) | TCC Brake/Cruise Release Switch
(22) | Park Brake Switch
(23) | Clutch Switch
(24) | Inflatable Restraint Roof Rail Module - Right
(25) | C211 (A31) (Body Harness to Passenger Door Harness)
(26) | C210 (A31) (Body Harness to Passenger Door Harness)
(27) | C200 (I/P Harness to Body Harness)
(28) | C275 (Body Harness to Steering Wheel Harness)
(29) | Clutch Start Switch
(30) | Body Control Module (BCM) C1
(31) | C209 (Body Harness to Driver Door Harness)
(32) | C202 (Driver Door Harness to Body Harness)
(33) | Inside Rearview Mirror

Figure 7: |

#### Passenger Compartment (Crew Cab)

(1) | Body Control Module (BCM) C1
(2) | C201 (I/P Harness to Body Harness)
(3) | G301
(4) | G302
(5) | Inflatable Restraint Sensing and Diagnostic Module (SDM)
(6) | C317 (A31) or C317 (w/oA31) (Body Harness to RR Passenger Door Harness)
(7) | Cargo Lamp/Center High Mounted Stop Lamp (CHMSL)
(8) | Door Jamb Switch - Front Passenger
(9) | Seat Belt Pretensioner - RF
(10) | Door Jamb Switch - RR
(11) | C313 (Body Harness to Passenger Seat Harness)
(12) | C316 (A31) or C316 (w/oA31) (Body Harness to LR Passenger Door Harness)
(13) | C314 (Body Harness to Driver Seat Harness)
(14) | Seat Belt Pretensioner - LF
(15) | Door Jamb Switch - LR
(16) | Door Jamb Switch - Driver
(17) | Transfer Case Shift Control Module C1, C2
(18) | G Sensor
(19) | G300
(20) | Stop Lamp Switch
(21) | TCC Brake/Cruise Release Switch
(22) | Park Brake Switch
(23) | S303
(24) | Clutch Switch
(25) | Clutch Start Switch
(26) | C208 (I/P Harness to Body Harness)
(27) | C202 (Driver Door Harness to Body Harness)
(28) | C209 (Body Harness to Driver Door Harness)
(29) | C200 (I/P Harness to Body Harness)
(30) | C275 (Body Harness to Steering Wheel Harness)
(31) | Inflatable Restraint Roof Rail Module - Left
(32) | Accelerator Pedal Position (APP) Sensor
(33) | C310 (Dome Lamp Harness to Body Harness)
(34) | C210 and C211 (A31) (Body Harness to Passenger Door Harness)
(35) | Inflatable Restraint Roof Rail Module - Right
(36) | Inside Rearview Mirror

Figure 8: |

#### Left Side of I/P

(1) | C275 (Body Harness to Steering Wheel Harness)
(2) | A/T Shift Lock Control Solenoid Connector
(3) | Body Harness
(4) | Accelerator Pedal Position (APP) Sensor Connector
(5) | Accelerator Pedal
(6) | Accelerator Pedal Position (APP) Sensor
(7) | A/T Shift Lock Control Solenoid
(8) | Ignition Lock Cylinder Case (Ignition Switch Location)