For 1990-2009 cars

Table 1: | Body Control Module (BCM)
Table 2: | Powertrain Control Module (PCM)

#### Body Control Module (BCM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF
Auto Learn Timer | Security Data | Seconds | 0-600
Content Theft State | Security Data | Off/Pre-arm/Armed/Pre-alarm/Alarm/Tamper | Off
Driver Door Ajar Switch | Inputs | Door Closed/Door Ajar | Door Closed
Passnager Door Ajar Switch | Inputs | Door Closed/Door Ajar | Door Closed
Passlock State | Security Data | Ignition Off/Normal Decision/Learn Passlock/Tamper/Monitor Passlock/Fail Enable/ Fail Enable Dec/Seedkey Lrn Pend/Seedkey Learn/Auto Learn Pend/Auto Learn | Normal Decision
Seed and Key Timer | Security Data | Seconds | 0-600
Tamper Timer | Security Data | Seconds | 0-600
VTD Fuel Diasble | Security Data | Active/Inactive | Inactive

#### Powertrain Control Module (PCM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF
PCM/VCM in VTD Fail Enable | Engine Data 3 | Yes/No | No
VTD Auto. Learn Timer | Engine Data 3 | Active/Inactive | Inactive
VTD Fuel Disable | Engine Data 3 | Acitve/Inactive | Inactive
VTD Fuel Disable Until Ign. Off | Engine Data 3 | Yes/No | No
VTD Password | Engine Data 3 | OK/Incorrect | OK