For 1990-2009 cars

### Engine Compartment Point to Point Measurements

Location | Length
--- | ---
a | 1372 mm
b | 1536 mm
c | 729 mm
d | 1536 mm
e | 860 mm
f | 850 mm
g | 729 mm
All dimensions are measured from a zero line, a center line, and a common datum. All dimensions are symmetrical unless otherwise specified.

### Radiator Support Point to Point Measurements

Location | Length
--- | ---
a | 787 mm
b | 403 mm
c | 403 mm
d | 787 mm