For 1990-2009 cars

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine OFF/Vehicle Stationary for at Least 60 Minutes/Tire Pressures Adjusted to Recommended kPa/psi.
Battery Voltage | Data Display | Volts | 12.5
LF Pressure Sensor ID | Data Display | Numeric/******** | Numeric
LF Pressure Sensor Mode | Data Display | Stationary/Wake/Drive/Learn/Re-measure/Low Bat/ N/A | Stationary
LF Tire Pressure | Data Display | kPa/psi | 35 psi
LR Pressure Sensor ID | Data Display | Numeric/******** | Numeric
LR Pressure Sensor Mode | Data Display | Stationary/Wake/Drive/Re-measure/Learn/Low Bat/ N/A | Stationary
LR Tire Pressure | Data Display | kPa/psi | 35 psi
RF Pressure Sensor ID | Data Display | Numeric/******** | Numeric
RF Pressure Sensor Mode | Data Display | Stationary/Wake/Drive/Re-measure/Learn/Low Bat/ N/A | Stationary
RF Tire Pressure | Data Display | kPa/psi | 35 psi
RR Pressure Sensor ID | Data Display | Numeric/******** | Numeric
RR Pressure Sensor Mode | Data Display | Stationary/Wake/Drive/Re-measure/Learn/Low Bat/ N/A | Stationary
RR Tire Pressure | Data Display | kPa/psi | 35 psi
Sensor Learn Mode | Data Display | Active/Inactive | Inactive
Selected Front Tire Pressure | Data Display | kPa/psi | 35 psi
Selected Rear Tire Pressure | Data Display | kPa/psi | 35 psi
Selected Tire Type | Data Display | P-Metric Standard/P-Metric Extended/Load Range C/Load Range D/Load Range E | P-Metric Standard
TPM System Enabled | Data Display | Yes/No | Yes
Vehicle Speed | Data Display | km/h/mph | 0