For 1990-2009 cars

### Driver Information Center (DIC)

The driver information center (DIC) consists of a double line 14 character display placed in the lower center area of the instrument panel cluster (IPC). The DIC will display vehicle information, configuration, and warning parameters to the driver.

The display parameters are cycled, changed, and acknowledged using a control stem. Pressing the stem for 1 second will display the DIC options. Pressing the stem for more than 2 seconds will select an option.

### DIC Displays

The driver information center (DIC) parameters are displayed by order of priority as follows (from highest to lowest) :

• | Service Diagnostics

• | Feature Programming

• | Driver Warnings

• | Vehicle Information

#### Vehicle Information

Vehicle information provides feedback to the driver on vehicle performance, mileage, maintenance or related information. When the English/Metric status changes, any applicable vehicle information data values will also change.

#### Odometer

The odometer is capable of displaying values from 0-999,999 KM or MI. If the ignition is in the OFF or UNLOCK/ACC position, the odometer can be displayed by pressing the trip/reset switch. The odometer will remain displayed for 5 seconds.

#### Trip Odometers

The trip odometer is capable of displaying values from 0-9999.9 KM or MI. When the maximum value is reached, the trip odometer will roll over to 0.0. Holding the control stem for greater than 4 seconds while the trip odometer is displayed will reset the displayed trip odometer to 0.0 upon release of the stem. The trip odometer will remain displayed after being reset.

#### Engine Oil Life

Engine Oil Life percentage values are based on serial data messages to the instrument panel cluster (IPC). The IPC requests this value when Engine Oil Life is selected on the DIC. Engine Oil Life is capable of displaying values from 0 to 100%. Pressing the control stem for longer than 2 seconds while Engine Oil Life is displayed on the DIC will reset the value to 100%. An audible warning will sound confirming that the system has been reset. Display appears as OIL LIFE: XXX%.

### Display Language

The driver information center (DIC) is capable of displaying messages in more than one language. The DIC language selection procedure is as follows:

1. With the engine OFF, turn the key to ON, but do not start the engine.
2. Close all doors so the DOORS message does not display in the DIC.
3. Momentarily press and release the trip reset stem until the current language is displayed: English, French or Spanish.
4. To select a different language, press and hold the trip reset stem until the next language appears.
5. Repeat Step 4 until the desired language is displayed. Once the desired language is shown on the DIC display, the language is set.
6. To exit language selection, momentarily press and release the trip stem. All DIC messages will now display in the language selected.

### Feature Programming

Refer to Personalization Description and Operation.

#### Driver Warnings

For the list of Driver Warnings, refer to Indicator/Warning Message Description and Operation.