For 1990-2009 cars

Connector 1: | Digital Radio Receiver (U2K)
Connector 2: | Radio C1
Connector 3: | Radio C2
Connector 4: | Speaker - Left Front Door
Connector 5: | Speaker - Left Front Door Tweeter (UQ3)
Connector 6: | Speaker - Left Rear Door (Extended/Crew Cab)
Connector 7: | Speaker - Right Front Door
Connector 8: | Speaker - Right Front Door Tweeter (UQ3)
Connector 9: | Speaker - Right Rear Door (Extended/Crew Cab)
Connector 10: | Vehicle Communications Interface Module (VCIM) C1
Connector 11: | Vehicle Communications Interface Module (VCIM) C2

### Digital Radio Receiver (U2K)

#### Connector Part Information

- OEM: 15394150
- Service: 15394150
- Description: 16-Way F ASM (WH)

#### Terminal Part Information

- Pins: 2, 3, 7, 9, 10, 16
- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Digital Radio Receiver (U2K)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BN/WH | 367 | Remote Playback Device Left Audio Signal
3 | D-GN/WH | 368 | Remote Playback Device Right Audio Signal
4-6 | -- | -- | Not Used
7 | PU | 1807 | Class 2 Serial Data
8 | -- | -- | Not Used
9 | BK/WH | 1151 | Ground
10 | BK/WH | 372 | Remote Playback Device Audio Common Signal
11-15 | -- | -- | Not Used
16 | OG | 1140 | Battery Positive Voltage

### Radio C1

#### Connector Part Information

- OEM: 12110088
- Service: 15306210
- Description: 24-Way F Micro-Pack 100 Series (GY)

#### Terminal Part Information

- Pins: A1, A2, A8, A9, A10, A11, B8, B9, B10, B11
- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

- Pins: A12, B1
- Terminal/Tray: 12146448/19
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Radio C1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | PU | 1807 | Class 2 Serial Data
A2 | PU | 1807 | Class 2 Serial Data
A3-A7 | -- | -- | Not Used
A8 | GY | 118 | Left Front Speaker Output (-)
A9 | TN | 201 | Left Front Speaker Output (+)
A10 | D-BU | 46 | Right Rear Speaker Output (+)
A11 | L-BU | 115 | Right Rear Speaker Output (-)
A12 | BK/WH | 1151 | Ground
B1 | OG | 1140 | Battery Positive Voltage
B2-B7 | -- | -- | Not Used
B8 | YE | 116 | Left Rear Speaker Output (-)
B9 | BN | 199 | Left Rear Speaker Output (+)
B10 | L-GN | 200 | Right Front Speaker Output (+)
B11 | D-GN | 117 | Right Front Speaker Output (-)
B12 | -- | -- | Not Used

### Radio C2

#### Connector Part Information

- OEM: 12064799
- Service: 15305996
- Description: 12-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Pins: C, G, H, J, K, L, M
- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Radio C2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | BARE | 1573 | Drain Wire (U2K)
D-F | -- | -- | Not Used
G | PU | 1807 | Class 2 Serial Data
H | D-GN/WH | 368 | Remote Playback Device Right Audio Signal (U2K)
J | BN/WH | 367 | Remote Playback Device Left Audio Signal (U2K)
K | BK/WH | 372 | Remote Playback Device Audio Common Signal (U2K)
L | OG/BK | 1406 | Remote Playback Device Left Audio Signal (UE1)
M | L-BU | 1405 | Remote Playback Device Audio Common Signal (UE1)

### Speaker - Left Front Door

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Left Front Door

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GY | 118 | Left Front Speaker Output (-)
B | TN | 201 | Left Front Speaker Output (+)

### Speaker - Left Front Door Tweeter (UQ3)

#### Connector Part Information

- OEM: 15427362
- Service: 88987841
- Description: 2-Way M 090 II (WH)

#### Terminal Part Information

- Terminal/Tray: 15305100/19
- Core/Insulation Crimp: A/E/A
- Release Tool/Test Probe: 12094429/J-35616-19 (BK)

#### Speaker - Left Front Door Tweeter (UQ3)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | 118 | Left Front Speaker Output (-)
2 | TN | 201 | Left Front Speaker Output (+)

### Speaker - Left Rear Door (Extended/Crew Cab)

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Left Rear Door (Extended/Crew Cab)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YE | 116 | Left Rear Speaker Output (-)
B | BN | 199 | Left Rear Speaker Output (+)

### Speaker - Right Front Door

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Right Front Door

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | D-GN | 117 | Right Front Speaker Output (-)
B | L-GN | 200 | Right Front Speaker Output (+)

### Speaker - Right Front Door Tweeter (UQ3)

#### Connector Part Information

- OEM: 15427362
- Service: 88987841
- Description: 2-Way M 090 II (WH)

#### Terminal Part Information

- Terminal/Tray: 15305100/19
- Core/Insulation Crimp: A/E/A
- Release Tool/Test Probe: 12094429/J-35616-19 (BK)

#### Speaker - Right Front Door Tweeter (UQ3)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN | 117 | Right Front Speaker Output (-)
2 | L-GN | 200 | Right Front Speaker Output (+)

### Speaker - Right Rear Door (Extended/Crew Cab)

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - Right Rear Door (Extended/Crew Cab)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YE | 115 | Right Rear Speaker Output (-)
B | BN | 46 | Right Rear Speaker Output (+)

### Vehicle Communications Interface Module (VCIM) C1

#### Connector Part Information

- OEM: 15383038
- Service: 15306351
- Description: 16-Way F 040II (WH)

#### Terminal Part Information

- Pins: 2, 3, 6, 11
- Terminal/Tray: 15355438/20
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-12 (BU)

- Pins: 7, 16
- Terminal/Tray: 175266-5/15
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: 15315247/J-35616-16 (L-GN)

#### Vehicle Communications Interface Module (VCIM) C1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BN/WH | 2517 | Keypad Red LED Signal
3 | YE/BK | 2516 | Keypad Green LED Signal
4-5 | -- | -- | Not Used
6 | L-GN/BK | 2515 | Keypad Supply Voltage
7 | BK/WH | 1151 | Ground
8-10 | -- | -- | Not Used
11 | D-GN/WH | 2514 | Keypad Signal
12-15 | -- | -- | Not Used
16 | OG | 340 | Battery Positive Voltage

### Vehicle Communications Interface Module (VCIM) C2

#### Connector Part Information

- OEM: 15383039
- Service: 88952886
- Description: 12-Way F 040II (WH)

#### Terminal Part Information

- Pins: 1, 2, 5, 8, 9, 10
- Terminal/Tray: 15355438/20
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-12 (BU)

#### Vehicle Communications Interface Module (VCIM) C2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 1405 | Remote Playback Device Audio Common Signal
2 | OG/BK | 1406 | Remote Playback Device Left Audio Signal
3-4 | -- | -- | Not Used
5 | PU | 1807 | Class 2 Serial Data
6-7 | -- | -- | Not Used
8 | BARE | 2012 | Drain Wire
9 | GY | 655 | Cellular Microphone Signal
10 | BARE | 1705 | Drain Wire
11-12 | -- | -- | Not Used