For 1990-2009 cars

#### C1 Remote Control Door Lock Receiver

Connector Part Information |

• | 12129431

• | 16-Way F Metri-Pack Series 280 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 694 | Power Door Lock Motor Feed-Driver Door Unlock
B | WHT | 194 | Power Door Lock Relay Feed-Unlock Coil
C | -- | -- | Not Used
D | -- | -- | Not Used
E | ORN | 40 | Fuse Output-Battery-Type III Fuse
F | -- | -- | Not Used
G | BLK/WHT | 56 | Trunk Release Motor Feed
H | -- | -- | Not Used
J | PNK | 39 | Fuse Output-Ignition 1-Type III Fuse
K | WHT/BLK | 572 | Keyless Entry Enable Signal
L | BLK/WHT | 1455 | Keyless Entry Program Enable Signal
M | -- | -- | Not Used
N | BLK | 150 | Ground
P | -- | -- | Not Used
R | LT BLU | 195 | Power Door Lock Relay Feed-Lock Coil
S | WHT | 156 | Courtesy Light Output