For 1990-2009 cars

#### Fastener Tightening Specifications

Application | Specification
--- | ---
Metric | English
Crossover Pipe | 22 N·m | 16 lb ft
Exhaust Manifold Pipe Assembly to Manifold Nut | 35 N·m | 26 lb ft
Muffler Hanger to Frame | 27 N·m | 20 lb ft
Muffler Hanger to Muffler Bolt | 15 N·m | 11 lb ft
Muffler Strap | 16 N·m | 12 lb ft
Three Way Catalytic Converter to Intermediate Pipe Bolts | 29 N·m | 21 lb ft