For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: Noise occurs in 5th speed gear only
1 |

1. Disassemble the transaxle case. Refer to Transmission Case Disassemble

Check the following components for wear or damage.

• | The 5th speed constant-mesh gears

• | The 5th synchronizer

• | The output gear

Are any of the components worn or damaged?

Go to Step 2

Refer to Isolating Noise

2 | Service, repair, or replace the components as necessary. Refer to Transmission Case Assemble Did the noise disappear? |  | System OK | Refer to Isolating Noise