For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Booster to Pedal Bracket | 27 N·m | 20 lb ft
Brake Hose to Caliper | 44 N·m | 32 lb ft
Brake Pedal to Bracket | 27 N·m | 20 lb ft
Brake Pipe Tube Nuts | 23 N·m | 17 lb ft
Brake Pipes at Master Cylinder | 23 N·m | 17 lb ft
Caliper Bleeder Screw | 13 N·m | 115 lb in
Caliper Mounting Bolts | 51 N·m | 38 lb ft
Master Cylinder Assembly to Power Booster Nuts | 27 N·m | 20 lb ft
Master Cylinder to Booster | 27 N·m | 20 lb ft
Proportioner Valve Caps | 27 N·m | 20 lb ft
Wheel Cylinder Bleeder Screw | 7 N·m | 62 lb in
Wheel Cylinder to Backing Plate | 20 N·m | 15 lb ft