For 1990-2009 cars

Application | N·m | Lbs Ft | Lbs In
--- | --- | --- | ---
Backup Light Switch | 33 | 24 | --
Clutch Housing Cover Bolt | 10 | -- | 89
Shift Cable Cover Bolt | 1.4 | -- | 12
Shift Control Box Bolt | 17 | 13 | --
Shift Control Box Nut | 24 | 18 | --
Shift Linkage Retainer Nut | 23 | 17 | --
Shift Retainer Nut | 10 | -- | 89
Speedometer/Vehicle Speed Sensor Housing Bolt | 9 | -- | 80
Transaxle-to-Engine Mounting Bolts and Stud | 75 | 55 | --
Transaxle Mount Bolt | 75 | 55 | --
Transaxle Mount Through Bolt | 60 | 44 | --
Transaxle Shift Cable Bracket Nut | 10 | -- | 89
Transaxle Shift Lever Nut | 10 | -- | 89