For 1990-2009 cars

# SMU-SECTION 5E -REV WHEEL SPEED SENSOR RESISTANCE

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 5E - REVISED WHEEL SPEED SENSOR RESISTANCE SPECIFICATIONS

#### MODELS: 1997 CHEVROLET MALIBU 1997 OLDSMOBILE CUTLASS

THIS BULLETIN IS BEING ISSUED TO REVISE THE WHEEL SPEED SENSOR RESISTANCE SPECIFICATIONS (DTC'S C1221 - C1235) ON PAGES 5E1-54 THROUGH 5E1-101 OF THE SERVICE MANUAL.

FRONT AND REAR WHEEL SPEED SENSOR RESISTANCE RANGE HAS BEEN CHANGED TO 950 - 1250 OHMS.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.