For 1990-2009 cars

# INFO ON NEW SPEC TOOL J28467- 330 ENG SUPPORT FIXTURE ADAPT

#### SUBJECT: NEW SPECIAL TOOL - J28467-330 ENGINE SUPPORT FIXTURE ADAPTER

#### MODELS/YEARS: 1992-93 ACHIEVA W/3.3L (VIN N)

#### SERVICE INFORMATION:

Use J 28467-330 Engine Support Fixture Adapter for supporting the engine when servicing engine/transmission components. - To use J 28467-330 adapter:

1 . Loosen pilot bolts on both ends of adapter.

2. Place pilot bolts in holes in tie bar, refer to the illustration below - View B.

3. Tighten pilot bolts.

4. Attach J 28467-A to strut towers and place the leg of J 28467-A on adapter as shown in the illustration.

5. Attach engine support hooks to engine support fixture and engine lift hooks.

#### Note: Failure to use J 28467-330 in conjunction with J 28467-A to support engine may cause damage to body or engine components.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.