For 1990-2009 cars

# STALL ON COLD START DIAG./INSTALL NEW PROM

#### SUBJECT: ENGINE DOES NOT STAY RUNNING ON COLD START - DIAGNOSE/INSTALL NEW PROM

#### MODEL/YEARS: 1991 CUTLASS CALAIS AND 1992-93 ACHIEVA WITH 3300 (VIN N) ENGINE

This bulletin cancels and supersedes bulletin 92-T-39 which should be discarded.

Some 1991 Cutlass Calais and 1992-93 Achieva models equipped with the 3300 (VIN N) engine, may experience a condition described as engine does not stay running on initial cold start.

If this condition is experienced and cannot be repaired by using currently published service diagnostic procedures, it may be necessary to install a new service PROM after basic engine controls and systems performance have been verified.

PARTS INFORMATION: Parts are currently available from GMSPO.

PROM PROM PROM SERVICE SCANNER BROADCAST YEAR(S) EMISSIONS AXLE PART NUMBER I.D. NO. CODE ------- --------- ---- ------------ -------- --------- 1992-93 Federal 2.39 16188352 6204 BDHN

1992-93 California 2.39 16188355 6214 BDHP

1991 Federal 2.39 16184606 4024 BCUR

1991 California 2.39 16184611 4034 BCUS

WARRANTY INFORMATION: Use applicable Labor Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.