For 1990-2009 cars

#### Range Reference Chart

Range | Park | Reverse | Neutral | OD | D | 2 | 1
--- | --- | --- | --- | --- | --- | --- | ---
Gear |  |  |  | 1st | 2nd | 3rd | 4th | 1st | 2nd | 3rd | 1st | 2nd | 1st
1-2 Shift Solenoid | ON | ON | ON | ON | OFF | OFF | ON | @ ON | @ OFF | @ OFF | @ ON | @ OFF | @ON
2-3 Shift Solenoid | ON | ON | ON | ON | ON | OFF | OFF | @ ON | @ ON | @ OFF | @ ON | @ ON | @ON
4th Clutch | -- | -- | -- | -- | -- | -- | A | -- | -- | -- | -- | --
Reverse Band | -- | A | -- | -- | -- | -- | -- | -- | -- | -- | -- | --
2nd Clutch | -- | -- | -- | -- | A | A | A | -- | A | A | -- | A | --
3rd Clutch | -- | -- | -- | -- | -- | A | * | -- | -- | A | -- | -- | A
3rd Sprag Clutch | -- | -- | -- | -- | -- | H | O | -- | -- | H | -- | -- | H
Input Clutch | * | A | * | A | * | -- | -- | A | * | A | A | * | A
Input Sprag Clutch | * | H | * | H | O | -- | -- | H | O | H | H | O | H
2/1 Band | -- | -- | -- | -- | -- | -- | -- | -- | -- | -- | A | A | A
1/2 Support Roller Clutch | -- | -- | -- | H | H | O | O | H | H | O | H | H | H
Forward Band | -- | -- | -- | A | A | A | A | A | A | A | A | A | A

- A = Applied
- H = Holding
- O = Overrun
- * Applied but not effective
- @ The solenoid's state follows a shift pattern which depends upon vehicle speed, throttle position, and selected gear range.
- ON = The solenoid is energized.
- OFF = The solenoid is de-energized