For 1990-2009 cars

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
Battery | Left side of engine compartment | 8A-201-4 Fig. 8 | -- | --
Clutch Pedal Position Switch | LH lower I/P near steering column | 8A-201-26 Fig. 52 | -- | --
Engine Compartment Fuse Center | Left side of engine compartment | 8A-201-4 Fig. 8 | -- | --
Fusible Link G | Lower front of engine | 8A-201-1 Fig. 1 | -- | --
Generator | Rear of engine | 8A-201-4 Fig. 7 | 202-53 | --
Ignition Switch | Steering column | 8A-201-33 Fig. 65 | 202-23 | --
Instrument Panel Cluster | Left side of I/P | 8A-201-27 Fig. 54 | 202-24 | --
Transaxle Range Switch | Left side of engine compartment | 8A-201-2 Fig. 4 | 202-28 | --
Powertrain Control Module (PCM) | RH front of I/P | 8A-201-23 Fig. 45 | 202-29 | --
Starter Motor | Front of engine | 8A-201-1 Fig. 1 | -- | --
Starter Solenoid | Front of engine | 8A-201-1 Fig. 1 | -- | --
CONNECTORS:
C100 | LH upper front of dash | 8A-201-30 Fig. 60 | 202-0 | --
C207 | RH lower I/P | 8A-201-30 Fig. 59 | 202-8 | --
GROUNDS:
G101 | Left inner fender | 8A-201-38 Fig. 75 | -- | --
G110 | Front of engine compartment | 8A-201-3 Fig. 6 | -- | --
SPLICES:
S202 | Lower LH of steering column | 8A-201-33 Fig. 65 | -- | --
S277 | Center I/P near tie bar | 8A-201-34 Fig. 67 | -- | --
S278 | RH rear of engine compartment | 8A-201-1 Fig. 2 | -- | --
S414 | Engine compartment front of dash | 8A-201-2 Fig. 3 | -- | --
GROMMETS:
P201 | RH upper I/P | 8A-201-1 Fig. 2 | -- | --