For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Check for proper tightness of the stabilizer shaft. Is the stabilizer shaft loose? | -- | Go to Stabilizer Shaft Replacement | Go to Step 2
2 | Check the condition of the strut dampeners, shock absorbers or mounting. Are the strut dampeners, shock absorbers or mounting worn? | -- | Go to Strut Assembly Replacement | Go to Step 3
3 | Check the condition of the springs. Are the springs broken or worn? | -- | Go to Strut, Strut Component and/or Spring Replacement in Front Suspension | Go to Step 4
4 | Check for vehicle overloading. Is the vehicle overloaded? | -- | Remove excess weight. | System OK