For 1990-2009 cars

Table 1: | C1
Table 2: | Left Door Lock Switch
Table 3: | Right Door Lock Switch
Table 4: | Outside Left Front Rear View Mirror Motor
Table 5: | Outside Right Front Rear View Mirror Motor
Table 6: | Outside Left Front Rear View Mirror Switch
Table 7: | Right Front Side Window Switch
Table 8: | Master Window Switch C1
Table 9: | Master Window Switch C2 (4 Door Only)

#### C1

Connector Part Information |

• | 12160707

• | 22-Way (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PNK | 539 | Fuse Output - Ignition 1 - Type III Fuse
2 | ORN | 140 | Fuse Output - Battery - Type III Fuse
3 | BRN | 27 | Hazard Flasher Output
4 | PPL | 16 | Turn Signal Flasher Output
5 | BLK | 150 | Ground
A | DK GRN/WHT | 817 | Vehicle Speed Signal - 4000 Pulses/Mile
B | -- | -- | Not Used
C | PPL | 16 | Turn Signal Flasher Output
D | BRN | 9 | Park Lamp Feed
E | LT GRN | 80 | Key Reminder Switch Signal
F | LT BLU | 292 | Rear Defogger Switch Signal - Primary
G | LT BLU | 395 | Door Handle Switch Signal - Right Front
H | LT GRN/BLK | 394 | Door Handle Switch Signal - Left Front
J | ORN/BLK | 17866 | Transaxle Park/Neutral Signal
K | BLK/WHT | 238 | Seat Belt Switch Signal
L | PPL | 681 | Rear Defogger Switch Signal - Secondary
M | PNK | 39 | Fuse Output - Ignition 1 - Type III Fuse
N | BRN | 994 | Automatic Door Lock/Unlock Power Feed
P | LT BLU | 195 | Power Door Lock Relay Feed - Lock Coil
R | ORN | 1640 | Fuse Output - Battery - Type III Fuse
S | BLK | 28 | Horn Relay Output - Coil
T | DK GRN | 29 | Horn Feed

#### Left Door Lock Switch

Connector Part Information |

• | 12160882

• | 8-Way F Metri-Pack Series 280 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | ORN | 40 | Power Door Lock Switch Feed
C | BLK | 150 | Ground
D | WHT | 194 | Power Door Unlock Output
E-F | -- | -- | Not Used
G | GRY | 8 | Switch Illumination Feed
H | LT BLU | 195 | Power Door Lock Output

#### Right Door Lock Switch

Connector Part Information |

• | 12160882

• | 8-Way F Metri-Pack Series 280 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | ORN | 40 | Power Door Lock Switch Feed
C | BLK | 250 | Ground
D | WHT | 194 | Power Door Unlock Output
E-F | -- | -- | Not Used
G | GRY | 8 | Switch Illumination Feed
H | BLU | 195 | Power Door Lock Output

#### Outside Left Front Rear View Mirror Motor

Connector Part Information |

• | 12047786

• | 4-Way M Metri-Pack Series 150 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 1499 | Power Mirror Select Signal-Left Mirror
B | WHT | 81 | Power Mirror Motor Feed-Left Horizontal Motor-Right Direction
C | YEL | 88 | Power Mirror Feed-Left Vertical Motor-Up Direction
D | -- | -- | Not Used

#### Outside Right Front Rear View Mirror Motor

Connector Part Information |

• | 12047786

• | 4-Way M Metri-Pack Series 150 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU/ WHT | 1497 | Power Mirror Select Switch Signal-Right Mirror
B | RED/WHT | 881 | Power Mirror Motor Feed-Right Horizontal Motor-Right Direction
C | BRN/WHT | 1498 | Power Mirror Motor Feed-Right Vertical Motor-Up Direction
D | -- | -- | Not Used

#### Outside Left Front Rear View Mirror Switch

Connector Part Information |

• | 12047886

• | 8-Way F Metri-Pack Series 150 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 1498 | Power Mirror Motor Feed-Right Vertical Motor-Up Direction
B | RED/WHT | 881 | Power Mirror Motor Feed-Right Horizontal Motor-Right Direction
C | LT BLU/ WHT | 1497 | Power Mirror Select Switch Signal-Right Mirror
D | BLK | 150 | Ground
E | ORN | 1732 | Electronic Control Unit Output-12 Volt-Inadvertent Lead Control
F | WHT | 81 | Power Mirror Motor Feed-Left Horizontal Motor-Right Direction
G | YEL | 88 | Power Mirror Motor Feed-Left Vertical Motor-Up Direction
H | LT GRN | 1499 | Power Mirror Select Switch Signal-Left Mirror

#### Right Front Side Window Switch

Connector Part Information |

• | 12064998

• | 8-Way F Metri-Pack Series 280 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 166 | Power Window Master Switch Output-Right Front Window-Up
B | BRN | 141 | Fuse Output-Ignition
C | BLK | 250 | Ground
D | DK BLU | 666 | Power Window Motor Feed-Right Front Window-Up
E | TAN | 167 | Power Window Master Switch Output-Right Front Window-Down
F | -- | -- | Not Used
G | GRY | 8 | Instrument Panel Lamp Feed
H | BRN | 667 | Power Window Motor Feed-Right Front Window-Down

#### Master Window Switch C1

Connector Part Information |

• | 12052854

• | 7-Way F Metri-Pack Series 280 (BLK) Left Front Side Window Switch (2-Door and 4-Door)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Instrument Panel Lamp Feed
B | BLK | 150 | Ground
C | TAN | 167 | Power Window Master Switch Output - Right Front Window - Down
D | BRN | 165 | Power Window Motor Feed - Left Front Window - Down (4-Door Only)
D | DK BLU | 164 | Power Window Motor Feed - Left Front Window - Up (2-Door Only)
E | DK BLU | 164 | Power Window Motor Feed - Left Front Window - Up (4-Door Only)
E | BRN | 165 | Power Window Motor Feed - Left Front Window - Down (2-Door Only)
F | LT BLU | 166 | Power Window Master Switch Output - Right Front Window - Up
G | BRN | 141 | Fuse Output - Ignition 3 - Type III Fuse

#### Master Window Switch C2 (4 Door Only)

Connector Part Information |

• | 12041429

• | 5-Way F Metri-Pack Series 280 (BLK) Left Front Side Window Lockout Switch (4-Door Only)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 1307 | Power Window Master Switch Output - Lockout
B | PPL | 171 | Power Window Master Switch Output - Right Rear Window - Down
C | PPL | 169 | Power Window Master Switch Output - Left Rear Window - Down
D | DK GRN | 168 | Power Window Master Switch Output - Left Rear Window - Up
E | LT GRN | 170 | Power Window Master Switch Output - Right Rear Window - Up