For 1990-2009 cars

Figure 1: |

#### Belt Drive

(1) | Reservoir Assembly Hydraulic Pump (Typical)
(2) | Capstick Assembly, Reservoir
(3) | Actuator, Variable Assist Steering
(4) | Clip, Retaining
(5) | Clip, Reservoir Retaining (LH)
(6) | Clip, Reservoir Retaining (RH)
(7) | Pin, Pump Ring Dowel
(7) | Pin, Pump Ring Dowel
(8) | Shaft, Drive
(9) | Seal, O-ring
(10) | Housing Assembly, Hydraulic Pump
(11) | Seal, Drive Shaft
(12) | Spring, Flow Control
(13) | Valve Assembly, Control
(14) | Seal, O-ring
(15) | Fitting, O-ring Union
(16) | Plate, Thrust
(17) | Ring, Pump
(18) | Vane
(19) | Rotor, Pump
(20) | Ring, Shaft Retaining
(21) | Plate, Pressure
(22) | Seal, O-ring
(23) | Spring, Pressure Plate
(24) | Seal, O-ring
(25) | Cover, End
(26) | Ring, Retaining

Figure 2: |

#### Direct Drive

(1) | Clip, Retaining
(2) | Actuator, Variable Assist Steering
(3) | Fitting, O-ring Union
(4) | Seal, O-ring
(5) | Reservoir Assembly, Hydraulic Pump (Typical)
(6) | Capstick Assembly, Reservoir
(7) | Clip, Reservoir Retaining (LH)
(8) | Clip, Reservoir Retaining (RH)
(9) | Seal, O-ring
(10) | Pin, Pump Drive Dowel
(10) | Pin, Pump Drive Dowel
(11) | Shaft, Drive
(12) | Housing Assembly, Hydraulic Pump
(13) | Seal, Face
(14) | Valve Assembly, Control
(15) | Spring, Flow Control
(16) | Seal, O-ring
(17) | Plug, Housing
(18) | Plate, Thrust
(19) | Ring, Pump
(20) | Vane
(21) | Rotor, Pump
(22) | Ring, Shaft Retaining
(23) | Plate, Pressure
(24) | Seal, O-ring
(25) | Spring, Pressure Plate
(26) | Seal, O-ring
(27) | Cover, End
(28) | Ring, Retaining