For 1990-2009 cars

Name | Location | Locator View (8A Cell 201 Page #) | Figure | Connector Eng View
--- | --- | --- | --- | ---
24X Crankshaft Position (CKP) Sensor | Front of engine | 8 | 15 | --
7X Crankshaft Position (CKP) Sensor | Front right side of engine | 7 | 13 | --
A/C Compressor Relay | Right Rear Engine Compartment | 37 | 71 | 11-4
A/C Refrigerant Pressure Sensor | Right hand side of engine compartment | 31 | 61 | --
Camshaft Position (CMP) Sensor | Rear of engine | 4 | 7 | --
Data Link Connector (DLC) | On bottom of Instrument Panel, right of steering column | 25 | 50 | 202-20
Engine Coolant Temperature (ECT) Sensor | Top left rear of engine | 4 | 7 | --
Engine Oil level Lamp | Upper left hand side of Instrument Cluster | -- | Refer to I/P for diagnosis | --
Engine Oil Level Sensor | Right rear bottom of engine | 8 | 16 | --
Evaporative Emission Canister Purge Solenoid | Rear of Engine Compartment | 4 | 7 | --
Evaporative Emission Canister Vent Valve Solenoid | Rh front of engine Compartment | -- | -- | --
Exhaust Gas Recirculation (EGR) Valve | Upper left hand side of engine | 4 | 7 | 202-51
Fuel Injectors | Top of engine, mounted to fuel rail, at each cylinder intake port | 4 | 7 | --
Fuel Pressure Regulator | Mounted on the Fuel Injector Rail, top | -- | -- | --
Fuel Pump/Fuel Level Sender | Mounted inside fuel tank | -- | -- | --
Fuel Pump Relay | Right rear engine compartment | 2 | 3 | 202-53
Fuse Block | LH side of Instrument Panel | 25 | 42 | 11-0
Generator | Rear of engine | 4 | 7 | 202-53
Heated Oxygen Sensor 1 (HO2S1) | Rear of engine, in exhaust manifold | 4 | 7 | 202-54
Heated Oxygen Sensor 2 (HO2S2) | In exhaust system, behind Catalytic Converter | 5 | 10 | 202-29
Idle Air Control Valve (IAC) | Top of engine, front of Throttle Body Assembly | 6 | 12 | 202-54
Ignition Control Module (ICM) | Top right hand front of engine | -- | -- | --
Intake Air Temperature (IAT) Sensor | Left hand front of engine compartment, on air intake duct | 6 | 12 | --
Knock Sensor (KS) | Front of engine, above starter | 7 | 13 | --
Malfunction Indicator Lamp (MIL) | Upper right hand side of Instrument Panel | -- | Refer to I/P Cluster for Repairs | --
Manifold Absolute Pressure (MAP) Sensor | Top rear of engine, on intake manifold | 4 | 7 | --
Mass Air Flow (MAF) Sensor | Left hand front of engine compartment, in air cleaner duct before throttle body | 6 | 12 | --
Powertrain Control Module (PCM) | Right hand side of lower I/P | 23 | 45 | 202-29
Powertrain Control Module Ground | Right hand side of engine, behind Ignition Control Module Bracket | 12 | 22 | --
Positive Crankcase Ventilation Valve | Top, right hand, center of engine, below Manifold Absolute Pressure (MAP) Sensor | -- | -- | --
Cooling Fan | Left hand side behind radiator | 3 | 5 | --
Cooling Fan Relay | Right Rear of engine compartment | 2 | 3 | 202-50
SMCC II Cruise Control Module | Left hand rear of engine compartment,center front of dash | 17 | 33 | 202-19
Throttle Body | Mounted to the Upper Intake Manifold, top, left hand side of engine | -- | -- | --
Throttle Position (TP) Sensor | Top of engine, on Throttle Body Assembly | 16 | 12 | --
TCC Brake Switch | Lower left hand side of I/P | 26 | 52 | 202-49
Transaxle Range Switch / Park Neutral Position (PNP) Switch | Rear left hand side of engine compartment, mounted to top of transaxle | 2 | 4 | 202-28
Vehicle Speed Sensor (VSS) | Lower right hand of engine on Transaxle | 8 | 16 | --