For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: Noise occurs in REVERSE gear only
1 |

1. Disassemble the transaxle case. Refer to Transmission Case Disassemble

Check the following components for wear or damage.

• | The idler gear

• | The idler gear bushing

• | The input gear

• | The output gear

Are any of the components worn or damaged?

Go to Step 2.

Refer to Transmission Replacement

2 | Service, repair, or replace the components as necessary. Refer to Transmission Case Assemble Did the noise disappear? |  | System OK. | Refer to Transmission Replacement