For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 9886-01 Door Handle Clip Remover

1. Remove the spring clip (1) by inserting toolJ 9886-01 (2) between the handle (3) and the trim panel.
2. Remove the window regulator handle (1).

### Installation Procedure

1. Raise the window to the up position.
2. Install the clip (1) to the window regulator handle (3).
3. Position the window regulator handle (1) at an angle shown in the figure.
4. Push the window handle in order to secure.